<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="55.931" y2="0" width="0" layer="20"/>
<wire x1="55.931" y1="0" x2="55.931" y2="17.77" width="0" layer="20"/>
<wire x1="55.931" y1="17.77" x2="0" y2="17.77" width="0" layer="20"/>
<text>Probe adapter for the
Tektronics 1230 Logic Analyser</text>
</plain>
<libraries>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA13-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA05-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="physnoct">
<packages>
<package name="PHYSNOCT">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV1" library="con-lstb" package="MA13-2" value="">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="con-lstb" package="MA05-2" value="">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV3" library="con-lstb" package="MA05-2" value="">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV4" library="con-lstb" package="MA05-2" value="">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="physnoct" package="PHYSNOCT" value="PHYSNOCT"/>
<element name="U$2" library="SparkFun" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="SV2" pad="10"/>
<contactref element="SV3" pad="10"/>
<contactref element="SV4" pad="10"/>
<contactref element="SV4" pad="2"/>
<contactref element="SV4" pad="4"/>
<contactref element="SV4" pad="6"/>
<contactref element="SV4" pad="8"/>
<contactref element="SV1" pad="18"/>
<contactref element="SV1" pad="26"/>
<contactref element="SV1" pad="20"/>
<contactref element="SV1" pad="22"/>
<contactref element="SV1" pad="24"/>
</signal>
<signal name="A0">
<contactref element="SV2" pad="1"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="A1">
<contactref element="SV2" pad="2"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="A2">
<contactref element="SV2" pad="3"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="A4">
<contactref element="SV2" pad="5"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="A5">
<contactref element="SV2" pad="6"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="A6">
<contactref element="SV2" pad="7"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="A7">
<contactref element="SV2" pad="8"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="A8">
<contactref element="SV3" pad="1"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="A9">
<contactref element="SV3" pad="2"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="A10">
<contactref element="SV3" pad="3"/>
<contactref element="SV1" pad="11"/>
</signal>
<signal name="A11">
<contactref element="SV3" pad="4"/>
<contactref element="SV1" pad="12"/>
</signal>
<signal name="A12">
<contactref element="SV3" pad="5"/>
<contactref element="SV1" pad="13"/>
</signal>
<signal name="A13">
<contactref element="SV3" pad="6"/>
<contactref element="SV1" pad="14"/>
</signal>
<signal name="A14">
<contactref element="SV3" pad="7"/>
<contactref element="SV1" pad="15"/>
</signal>
<signal name="A15">
<contactref element="SV3" pad="8"/>
<contactref element="SV1" pad="16"/>
</signal>
<signal name="A3">
<contactref element="SV2" pad="4"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="CLK1">
<contactref element="SV4" pad="1"/>
<contactref element="SV1" pad="17"/>
</signal>
<signal name="QUAL">
<contactref element="SV4" pad="3"/>
<contactref element="SV1" pad="19"/>
</signal>
<signal name="CLK2">
<contactref element="SV4" pad="5"/>
<contactref element="SV1" pad="21"/>
</signal>
<signal name="EXT">
<contactref element="SV4" pad="7"/>
<contactref element="SV1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
