<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="130.79" y2="0" width="0" layer="20"/>
<wire x1="130.79" y1="0" x2="130.79" y2="25.3875" width="0" layer="20"/>
<wire x1="130.79" y1="25.3875" x2="0" y2="25.3875" width="0" layer="20"/>
<wire x1="0" y1="25.3875" x2="0" y2="0" width="0" layer="20"/>
<text>Illusion
Display</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="OPL Eagle Library">
<packages>
<package name="2P-SMD-5.0X3.2">
<description>3.2mm*5mm dimension &lt;br&gt;
8MHz available</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-CMT1102">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED10" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED11" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED12" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED13" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED14" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED15" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED16" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED17" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED18" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED19" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED20" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED21" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED22" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED23" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED24" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED25" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED26" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED27" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED28" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED29" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED3" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED30" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED31" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED32" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED33" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED34" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED35" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED36" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED37" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED38" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED39" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED4" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED40" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED41" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED42" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED43" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED44" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED45" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED46" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED47" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED48" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED49" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED5" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED50" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED51" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED52" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED53" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED54" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED55" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED56" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED57" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED58" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED59" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED6" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED60" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED61" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED62" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED63" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED64" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED65" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED66" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED67" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED68" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED69" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED7" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED70" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED71" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED72" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED8" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="LED9" library="adafruit" package="CHIPLED_0805" value=""/>
<element name="R1" library="adafruit" package="R0805" value="220Ω"/>
<element name="R2" library="adafruit" package="R0805" value="220Ω"/>
<element name="R3" library="adafruit" package="R0805" value="220Ω"/>
<element name="R4" library="adafruit" package="R0805" value="220Ω"/>
<element name="R5" library="adafruit" package="R0805" value="220Ω"/>
<element name="R6" library="adafruit" package="R0805" value="220Ω"/>
<element name="R7" library="adafruit" package="R0805" value="220Ω"/>
<element name="R8" library="adafruit" package="R0805" value="220Ω"/>
<element name="R9" library="adafruit" package="R0805" value="220Ω"/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP6" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="C12" library="SparkFun-Capacitors" package="0603-CAP" value="18pF"/>
<element name="C13" library="SparkFun-Capacitors" package="0603-CAP" value="18pF"/>
<element name="X1" library="OPL Eagle Library" package="2P-SMD-5.0X3.2" value="CRYSTAL-0500290P1"/>
<element name="SG2" library="SparkFun-Electromechanical" package="BUZZER-CMT1102" value="BUZZERSMD3"/>
<element name="JP1" library="adafruit" package="2X04" value=""/>
</elements>
<signals>
<signal name="PD0">
<contactref element="LED8" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="PD1">
<contactref element="LED16" pad="C"/>
<contactref element="LED15" pad="C"/>
<contactref element="LED14" pad="C"/>
<contactref element="LED13" pad="C"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED11" pad="C"/>
<contactref element="LED10" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="PD2">
<contactref element="R3" pad="1"/>
<contactref element="LED24" pad="C"/>
<contactref element="LED23" pad="C"/>
<contactref element="LED22" pad="C"/>
<contactref element="LED21" pad="C"/>
<contactref element="LED20" pad="C"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED18" pad="C"/>
<contactref element="LED17" pad="C"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="PD3">
<contactref element="R4" pad="1"/>
<contactref element="LED32" pad="C"/>
<contactref element="LED31" pad="C"/>
<contactref element="LED30" pad="C"/>
<contactref element="LED29" pad="C"/>
<contactref element="LED28" pad="C"/>
<contactref element="LED27" pad="C"/>
<contactref element="LED26" pad="C"/>
<contactref element="LED25" pad="C"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED17" pad="A"/>
<contactref element="LED25" pad="A"/>
<contactref element="LED33" pad="A"/>
<contactref element="LED41" pad="A"/>
<contactref element="LED49" pad="A"/>
<contactref element="LED57" pad="A"/>
<contactref element="LED65" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="LED66" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED26" pad="A"/>
<contactref element="LED34" pad="A"/>
<contactref element="LED42" pad="A"/>
<contactref element="LED50" pad="A"/>
<contactref element="LED58" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED67" pad="A"/>
<contactref element="LED59" pad="A"/>
<contactref element="LED51" pad="A"/>
<contactref element="LED43" pad="A"/>
<contactref element="LED35" pad="A"/>
<contactref element="LED27" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="LED68" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED19" pad="A"/>
<contactref element="LED36" pad="A"/>
<contactref element="LED44" pad="A"/>
<contactref element="LED52" pad="A"/>
<contactref element="LED60" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="2"/>
<contactref element="LED69" pad="A"/>
<contactref element="LED61" pad="A"/>
<contactref element="LED53" pad="A"/>
<contactref element="LED45" pad="A"/>
<contactref element="LED28" pad="A"/>
<contactref element="LED20" pad="A"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="LED70" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED21" pad="A"/>
<contactref element="LED29" pad="A"/>
<contactref element="LED37" pad="A"/>
<contactref element="LED54" pad="A"/>
<contactref element="LED62" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="2"/>
<contactref element="LED71" pad="A"/>
<contactref element="LED63" pad="A"/>
<contactref element="LED46" pad="A"/>
<contactref element="LED38" pad="A"/>
<contactref element="LED30" pad="A"/>
<contactref element="LED22" pad="A"/>
<contactref element="LED14" pad="A"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="2"/>
<contactref element="LED72" pad="A"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED23" pad="A"/>
<contactref element="LED31" pad="A"/>
<contactref element="LED39" pad="A"/>
<contactref element="LED47" pad="A"/>
<contactref element="LED55" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="2"/>
<contactref element="LED64" pad="A"/>
<contactref element="LED56" pad="A"/>
<contactref element="LED48" pad="A"/>
<contactref element="LED40" pad="A"/>
<contactref element="LED32" pad="A"/>
<contactref element="LED24" pad="A"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="AVCC">
<contactref element="U1" pad="18"/>
</signal>
<signal name="PD4">
<contactref element="LED40" pad="C"/>
<contactref element="LED39" pad="C"/>
<contactref element="LED38" pad="C"/>
<contactref element="LED37" pad="C"/>
<contactref element="LED36" pad="C"/>
<contactref element="LED35" pad="C"/>
<contactref element="LED34" pad="C"/>
<contactref element="LED33" pad="C"/>
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="PD5">
<contactref element="LED48" pad="C"/>
<contactref element="LED47" pad="C"/>
<contactref element="LED46" pad="C"/>
<contactref element="LED45" pad="C"/>
<contactref element="LED44" pad="C"/>
<contactref element="LED43" pad="C"/>
<contactref element="LED42" pad="C"/>
<contactref element="LED41" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="PD6">
<contactref element="LED56" pad="C"/>
<contactref element="LED55" pad="C"/>
<contactref element="LED54" pad="C"/>
<contactref element="LED53" pad="C"/>
<contactref element="LED52" pad="C"/>
<contactref element="LED51" pad="C"/>
<contactref element="LED50" pad="C"/>
<contactref element="LED49" pad="C"/>
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="PD7">
<contactref element="LED64" pad="C"/>
<contactref element="LED63" pad="C"/>
<contactref element="LED62" pad="C"/>
<contactref element="LED61" pad="C"/>
<contactref element="LED60" pad="C"/>
<contactref element="LED59" pad="C"/>
<contactref element="LED58" pad="C"/>
<contactref element="LED57" pad="C"/>
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="PB0">
<contactref element="LED72" pad="C"/>
<contactref element="LED71" pad="C"/>
<contactref element="LED70" pad="C"/>
<contactref element="LED69" pad="C"/>
<contactref element="LED68" pad="C"/>
<contactref element="LED67" pad="C"/>
<contactref element="LED66" pad="C"/>
<contactref element="LED65" pad="C"/>
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="SG2" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="C13" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="C12" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="28"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="13"/>
<contactref element="SG2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
