<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>5V</text>
<text>G</text>
<text>G</text>
<text>5</text>
<wire x1="9.271" y1="0" x2="0.889" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0.889" x2="0" y2="8.001" width="0" layer="20"/>
<wire x1="0.889" y1="8.89" x2="9.271" y2="8.89" width="0" layer="20"/>
<wire x1="10.16" y1="8.001" x2="10.16" y2="0.889" width="0" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>6-20V</text>
<text>+5V</text>
<text>+5V</text>
<text>5V 1A REG</text>
<text>T.KOSTKA</text>
<text>NOV-2016</text>
<wire x1="0.889" y1="8.89" x2="0" y2="8.001" width="0" layer="20"/>
<wire x1="0" y1="0.889" x2="0.889" y2="0" width="0" layer="20"/>
<wire x1="10.16" y1="0.889" x2="9.271" y2="0" width="0" layer="20"/>
<wire x1="10.16" y1="8.001" x2="9.271" y2="8.89" width="0" layer="20"/>
<text>6-20V</text>
</plain>
<libraries>
<library name="kcl_passives">
<packages>
<package name="IND1008">
<description>From Murata - TOKO DFE252012F-4R7M=P2</description>
</package>
<package name="C1206R">
<description>Chip capacitor land pattern, reflow soldering, size 1206.</description>
</package>
<package name="C0805R">
<description>Chip capacitor land pattern, reflow soldering, size 0805.</description>
</package>
<package name="C0402R">
<description>Chip capacitor land pattern, reflow soldering, size 0402.</description>
</package>
</packages>
</library>
<library name="kcl_ics">
<packages>
<package name="WSON10EP-3X3MM-TI">
</package>
</packages>
</library>
<library name="kcl_pdb360">
<packages>
<package name="OSHPARK-CASTELLATION">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L1" library="kcl_passives" package="IND1008" value="4.7uH">
<attribute name="PN" value="DFE252012F-4R7M=P2"/>
</element>
<element name="C1" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="VALUE"/>
<attribute name="PN" value="GRM155R71H104KE14D"/>
</element>
<element name="U1" library="kcl_ics" package="WSON10EP-3X3MM-TI" value="LM5360X">
<attribute name="PN" value="LM53601LQDSXTQ1"/>
</element>
<element name="J1" library="kcl_pdb360" package="OSHPARK-CASTELLATION" value="TPOSHPARK-CASTELLATION"/>
<element name="J2" library="kcl_pdb360" package="OSHPARK-CASTELLATION" value="TPOSHPARK-CASTELLATION"/>
<element name="J3" library="kcl_pdb360" package="OSHPARK-CASTELLATION" value="TPOSHPARK-CASTELLATION"/>
<element name="J4" library="kcl_pdb360" package="OSHPARK-CASTELLATION" value="TPOSHPARK-CASTELLATION"/>
<element name="C2" library="kcl_passives" package="C0402R" value="1uF">
<attribute name="PN" value="GRM155R70J105KA12J"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="kcl_passives" package="C0402R" value="0.01uF">
<attribute name="VALUE"/>
<attribute name="PN" value="885012205067"/>
</element>
<element name="C4" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="VALUE"/>
<attribute name="PN" value="GRM155R71H104KE14D"/>
</element>
<element name="C6" library="kcl_passives" package="C0805R" value="10uF">
<attribute name="PN" value="GRM21BR71A106KA73L"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="kcl_passives" package="C0805R" value="10uF">
<attribute name="PN" value="GRM21BR71A106KA73L"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="kcl_passives" package="C1206R" value="10uF">
<attribute name="PN" value="GRM31CR71E106KA12L"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="kcl_pdb360" package="OSHPARK-CASTELLATION" value="TPOSHPARK-CASTELLATION"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="PAD1"/>
<contactref element="U1" pad="PAD3"/>
<contactref element="U1" pad="PAD2"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="9"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="7"/>
<contactref element="J4" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="4"/>
<contactref element="L1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
