(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 61)
    (no_connects 0)
    (area 88.824999 45.644999 155.015001 111.835001)
    (thickness 1.6)
    (drawings 6)
    (tracks 105)
    (zones 0)
    (modules 26)
    (nets 23)
  )
  (page A)
  (title_block
    (title "Shutter Driver")
    (date 2017-02-20)
    (rev 1.1)
    (company "Rice University")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.50012 3.50012)
    (pad_drill 2.19964)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 88.9 45.72)
    (grid_origin 88.9 45.72)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 LOGIC)
  (net 5 "Net-(J1-Pad2)")
  (net 6 +5V)
  (net 7 OUT_1B)
  (net 8 OUT_2B)
  (net 9 "Net-(D1-Pad1)")
  (net 10 OUT_1A)
  (net 11 OUT_2A)
  (net 12 "Net-(R5-Pad1)")
  (net 13 "Net-(C4-Pad2)")
  (net 14 "Net-(C5-Pad2)")
  (net 15 "Net-(C1-Pad2)")
  (net 16 "Net-(C3-Pad2)")
  (net 17 "Net-(C5-Pad1)")
  (net 18 "Net-(H1-Pad2)")
  (net 19 "Net-(U2-Pad1)")
  (net 20 "Net-(U2-Pad8)")
  (net 21 "Net-(U3-Pad9)")
  (net 22 "Net-(R6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net LOGIC)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad9)")
  )
  (net_class IC_Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Shutter_Drive ""
    (clearance 0.2)
    (trace_width 1.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(H1-Pad2)")
    (add_net OUT_1A)
    (add_net OUT_1B)
    (add_net OUT_2A)
    (add_net OUT_2B)
    (add_net VCC)
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AB63EB)
    (at 93.98 107.95)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P1 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value IC_PWR (at -3.556 0 90) (layer F.SilkS))
    (fp_text user G (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AB63DD)
    (at 138.43 107.95)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P2 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value SHUTTER_PWR (at -3.556 -2.032 90) (layer F.SilkS))
    (fp_text user G (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 58953329)
    (at 144.78 67.31 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference H1 (at 1.27 -2.39 90) (layer F.SilkS))
    (fp_text value SEL_1 (at 4.445 4.445 180) (layer F.SilkS))
    (fp_text user OUT_2B (at -5.08 7.62 90) (layer F.SilkS))
    (fp_text user OUT_2A (at -5.08 5.08 90) (layer F.SilkS))
    (fp_text user OUT_1B (at -5.08 2.54 90) (layer F.SilkS))
    (fp_text user OUT_1A (at -5.08 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 OUT_1A))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(H1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 OUT_1B))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(H1-Pad2)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 OUT_2A))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(H1-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 OUT_2B))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(H1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 58953326)
    (at 129.54 67.31 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference H2 (at 1.27 -2.39 90) (layer F.SilkS))
    (fp_text value SEL_2 (at 4.445 3.81 180) (layer F.SilkS))
    (fp_text user OUT_2B (at -5.08 0 90) (layer F.SilkS))
    (fp_text user OUT_2A (at -5.08 2.54 90) (layer F.SilkS))
    (fp_text user OUT_1B (at -5.08 5.08 90) (layer F.SilkS))
    (fp_text user OUT_1A (at -5.08 7.62 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 OUT_2B))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 OUT_2A))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 OUT_1B))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 OUT_1A))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:Multiwatt_15_Vertical (layer F.Cu) (tedit 58953289)
    (at 139.7 92.71)
    (descr http://www.icbuy.com/education/package/mode_name/upload/education/package/061106/1737460368586001162805866.pdf)
    (fp_text reference U3 (at -11.43 -8.89) (layer F.SilkS))
    (fp_text value LMD18200 (at 0 -10.16) (layer F.SilkS))
    (pad 1 thru_hole oval (at -8.509 0) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at -6.8072 -5.08) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 OUT_2A))
    (pad 3 thru_hole oval (at -5.1054 0) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 LOGIC))
    (pad 4 thru_hole oval (at -3.4036 -5.08) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at -1.7018 0) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 6 thru_hole oval (at 0 -5.08) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 7 thru_hole oval (at 1.7018 0) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 3.4036 -5.08) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(R5-Pad1)"))
    (pad 9 thru_hole oval (at 5.1054 0) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(U3-Pad9)"))
    (pad 10 thru_hole oval (at 6.8072 -5.08) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 OUT_2B))
    (pad 11 thru_hole oval (at 8.509 0) (size 1.778 3.048) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/Multiwatt_15_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_BNC:BNC_Socket_TYCO-AMP_LargePads (layer F.Cu) (tedit 58953265)
    (at 96.52 53.34)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference J1 (at 8.255 -5.715 90) (layer F.SilkS))
    (fp_text value TTL (at 8.255 6.35 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at -5.08 0) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 0 5.08) (size 1.6002 2.49936) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at -2.54 5.08) (size 1.6002 2.49936) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_BNC:BNC_Socket_TYCO-AMP_LargePads (layer F.Cu) (tedit 5895325F)
    (at 147.32 53.34)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference J2 (at -8.255 -5.715 90) (layer F.SilkS))
    (fp_text value SHUTTER (at -8.255 4.445 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at -5.08 0) (size 3.50012 3.50012) (drill 2.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 0) (size 3.50012 3.50012) (drill 2.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 0 5.08) (size 1.6002 2.49936) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(H1-Pad2)"))
    (pad 2 thru_hole oval (at -2.54 5.08) (size 1.6002 2.49936) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C5-Pad1)"))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58953210)
    (at 100.33 71.12 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value CP (at 2.54 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 589531E6)
    (at 104.14 85.09 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 6.985 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.54 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 589531A5)
    (at 127 87.63 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 10nF (at 2.54 0 360) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 OUT_2A))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5895319A)
    (at 152.4 87.63 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 6.985 0 360) (layer F.SilkS))
    (fp_text value 10nF (at 2.54 0 360) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 OUT_2B))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 58953240)
    (at 114.3 62.23 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C5 (at 3.75 -10.06 270) (layer F.SilkS))
    (fp_text value C (at 3.81 0 360) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 589531CC)
    (at 95.25 99.06 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C6 (at 1 -3.56 180) (layer F.SilkS))
    (fp_text value 10uF (at 1 3.56 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5895327E)
    (at 114.3 97.79 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C7 (at 3.75 -10.06 270) (layer F.SilkS))
    (fp_text value 2500uF (at 3.81 0 360) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 58953163)
    (at 149.86 97.79 270)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 12.7 0 360) (layer F.SilkS))
    (fp_text value 5.6V (at 5.08 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Diodes_ThroughHole.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5895311E)
    (at 100.33 97.79 270)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 12.7 0 360) (layer F.SilkS))
    (fp_text value D (at 5.08 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Diodes_ThroughHole.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 58953140)
    (at 132.08 97.79 270)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 12.7 0 360) (layer F.SilkS))
    (fp_text value D (at 5.08 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Diodes_ThroughHole.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58953137)
    (at 127 105.41)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference H3 (at 0 5.08) (layer F.SilkS))
    (fp_text value PWR_SEL (at -2.54 1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 58953217)
    (at 96.52 73.66 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value RI (at 5.08 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 589531DC)
    (at 93.98 90.17)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -2.54 0) (layer F.SilkS))
    (fp_text value RL (at 5.08 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 LOGIC))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_Power_L25.0mm_W9.0mm_P30.48mm (layer F.Cu) (tedit 58953234)
    (at 106.68 50.8)
    (descr "Resistor, Axial_Power series, Axial, Horizontal, pin pitch=30.48mm, 7W, length*diameter=25*9mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
    (tags "Resistor Axial_Power series Axial Horizontal pin pitch 30.48mm 7W length 25mm diameter 9mm")
    (fp_text reference R3 (at 26.67 5.715) (layer F.SilkS))
    (fp_text value R (at 15.24 0.635) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (pad 2 thru_hole oval (at 30.48 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(C5-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_Power_L25.0mm_W9.0mm_P30.48mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5895315A)
    (at 144.78 97.79 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 12.065 0 360) (layer F.SilkS))
    (fp_text value 10k (at 5.08 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5895326F)
    (at 143.51 80.01 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 1.905 180) (layer F.SilkS))
    (fp_text value 2.7k (at 5.08 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 589531FB)
    (at 99.06 77.47 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at -0.635 -2.54 270) (layer F.SilkS))
    (fp_text value 6N139 (at 6.985 -2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 LOGIC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R6-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 589531AA)
    (at 110.49 80.01)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U2 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value IXDF604PI (at 3.81 10.01) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 OUT_1A))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 LOGIC))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 OUT_1B))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 LOGIC))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad8)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 58B6FA89)
    (at 104.14 93.98 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 12.7 0 180) (layer F.SilkS))
    (fp_text value R (at 5.08 0 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 LOGIC))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "1 = IXDF604PI\n2 = LMD18200" (at 123.825 78.74 90) (layer F.SilkS))
  (gr_text "Shutter Driver Rev. 1.1\n2017/02/20" (at 121.92 55.88) (layer B.SilkS))
  (gr_line (start 88.9 111.76) (end 154.94 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 45.72) (end 88.9 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 45.72) (end 154.94 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 45.72) (end 154.94 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 154.305 111.125) (xy 89.535 111.125) (xy 89.535 46.355) (xy 154.305 46.355)
      )
    )
  )
)
