<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="44.684" y2="0" width="0" layer="20"/>
<wire x1="44.684" y1="0" x2="44.684" y2="18.212" width="0" layer="20"/>
<wire x1="44.684" y1="18.212" x2="0" y2="18.212" width="0" layer="20"/>
<wire x1="0" y1="18.212" x2="0" y2="0" width="0" layer="20"/>
<text>AtomSoftTech</text>
<text>FT800 4.3 (PSP)</text>
<text>AtomSoft.wordpress.com</text>
<text>R2-R3</text>
<text>R4-R5</text>
<text>R6-R7</text>
<text>G2-G3</text>
<text>G4-G5</text>
<text>G6-G7</text>
<text>B2-B3</text>
<text>B4-B5</text>
<text>B6-B7</text>
<text>PCLK-DISP</text>
<text>HSYNC-VSYNC</text>
<text>DEN-X+</text>
<text>Y+-X-</text>
<text>Y--PWM</text>
<text>VCC-BLK</text>
<text>GND-BLA</text>
</plain>
<libraries>
<library name="AtomTech">
<description>PSP Joystick</description>
<packages>
<package name="2X16">
</package>
<package name="4_PIN_PSP_LCD_BL">
</package>
<package name="SOT23-T5">
</package>
<package name="INDUCTOR_1206">
</package>
<package name="3216-18">
</package>
<package name="CMHSH5-2L">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PSP_CONNECTOR">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="AtomTech" package="2X16" value="2X16"/>
<element name="U$3" library="AtomTech" package="4_PIN_PSP_LCD_BL" value="PSP_BACKLIGHT"/>
<element name="U$4" library="SparkFun" package="PSP_CONNECTOR" value="PSP_CONNECTOR"/>
<element name="U$1" library="AtomTech" package="SOT23-T5" value="LD6806TD/25H">
<attribute name="NAME"/>
</element>
<element name="IC1" library="AtomTech" package="SOT23-T5" value="NCP1402"/>
<element name="L1" library="AtomTech" package="INDUCTOR_1206" value="INDUCTOR_LQH32C"/>
<element name="C1" library="AtomTech" package="3216-18" value="68uf"/>
<element name="C2" library="rcl" package="C0805" value="10uf"/>
<element name="D1" library="AtomTech" package="CMHSH5-2L" value="CMHSH5-2L"/>
</elements>
<signals>
<signal name="R2">
<contactref element="U$2" pad="1"/>
<contactref element="U$4" pad="R2"/>
</signal>
<signal name="R3">
<contactref element="U$2" pad="2"/>
<contactref element="U$4" pad="R3"/>
</signal>
<signal name="R4">
<contactref element="U$2" pad="3"/>
<contactref element="U$4" pad="R4"/>
</signal>
<signal name="R5">
<contactref element="U$2" pad="4"/>
<contactref element="U$4" pad="R5"/>
</signal>
<signal name="R6">
<contactref element="U$2" pad="5"/>
<contactref element="U$4" pad="R6"/>
</signal>
<signal name="R7">
<contactref element="U$2" pad="6"/>
<contactref element="U$4" pad="R7"/>
</signal>
<signal name="G2">
<contactref element="U$2" pad="7"/>
<contactref element="U$4" pad="G2"/>
</signal>
<signal name="G4">
<contactref element="U$2" pad="9"/>
<contactref element="U$4" pad="G4"/>
</signal>
<signal name="G3">
<contactref element="U$2" pad="8"/>
<contactref element="U$4" pad="G3"/>
</signal>
<signal name="G5">
<contactref element="U$2" pad="10"/>
<contactref element="U$4" pad="G5"/>
</signal>
<signal name="G6">
<contactref element="U$2" pad="11"/>
<contactref element="U$4" pad="G6"/>
</signal>
<signal name="G7">
<contactref element="U$2" pad="12"/>
<contactref element="U$4" pad="G7"/>
</signal>
<signal name="B2">
<contactref element="U$2" pad="13"/>
<contactref element="U$4" pad="B2"/>
</signal>
<signal name="B3">
<contactref element="U$2" pad="14"/>
<contactref element="U$4" pad="B3"/>
</signal>
<signal name="B4">
<contactref element="U$2" pad="15"/>
<contactref element="U$4" pad="B4"/>
</signal>
<signal name="B5">
<contactref element="U$2" pad="16"/>
<contactref element="U$4" pad="B5"/>
</signal>
<signal name="B6">
<contactref element="U$2" pad="17"/>
<contactref element="U$4" pad="B6"/>
</signal>
<signal name="B7">
<contactref element="U$2" pad="18"/>
<contactref element="U$4" pad="B7"/>
</signal>
<signal name="PCLK">
<contactref element="U$2" pad="19"/>
<contactref element="U$4" pad="CK"/>
</signal>
<signal name="DISP">
<contactref element="U$2" pad="20"/>
<contactref element="U$4" pad="DISP"/>
</signal>
<signal name="HSYNC">
<contactref element="U$2" pad="21"/>
<contactref element="U$4" pad="HSYNC"/>
</signal>
<signal name="VSYNC">
<contactref element="U$2" pad="22"/>
<contactref element="U$4" pad="VSYNC"/>
</signal>
<signal name="DEN">
<contactref element="U$2" pad="23"/>
</signal>
<signal name="X+">
<contactref element="U$2" pad="24"/>
</signal>
<signal name="Y+">
<contactref element="U$2" pad="25"/>
</signal>
<signal name="X-">
<contactref element="U$2" pad="26"/>
</signal>
<signal name="Y-">
<contactref element="U$2" pad="27"/>
</signal>
<signal name="BLPWM">
<contactref element="U$2" pad="28"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="29"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="L1" pad="P$1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="31"/>
<contactref element="U$4" pad="R0"/>
<contactref element="U$4" pad="NC2"/>
<contactref element="U$4" pad="NC"/>
<contactref element="U$4" pad="GND3"/>
<contactref element="U$4" pad="B1"/>
<contactref element="U$4" pad="B0"/>
<contactref element="U$4" pad="G1"/>
<contactref element="U$4" pad="G0"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$4" pad="GND2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$4" pad="TEST2"/>
<contactref element="U$4" pad="TEST3"/>
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="C"/>
<contactref element="C2" pad="2"/>
<contactref element="U$4" pad="R1"/>
</signal>
<signal name="BLA">
<contactref element="U$2" pad="32"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="BLK">
<contactref element="U$2" pad="30"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="U$1" pad="5"/>
<contactref element="U$4" pad="VCC"/>
<contactref element="U$4" pad="VCC2"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="AVDD"/>
<contactref element="U$4" pad="AVDD2"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="A"/>
<contactref element="D1" pad="N"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="5"/>
<contactref element="L1" pad="P$2"/>
<contactref element="D1" pad="P"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
