<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="49.53" y1="17.57" x2="49.53" y2="2.75" width="0.1524" layer="20"/>
<wire x1="49.53" y1="2.75" x2="46.78" y2="0" width="0.1524" layer="20" curve="-90"/>
<wire x1="46.78" y1="0" x2="2.75" y2="0" width="0.1524" layer="20"/>
<wire x1="2.75" y1="0" x2="0" y2="2.75" width="0.1524" layer="20" curve="-90"/>
<wire x1="0" y1="2.75" x2="0" y2="17.57" width="0.1524" layer="20"/>
<wire x1="0" y1="17.57" x2="2.75" y2="20.32" width="0.1524" layer="20" curve="-90"/>
<wire x1="2.75" y1="20.32" x2="46.78" y2="20.32" width="0.1524" layer="20"/>
<wire x1="46.78" y1="20.32" x2="49.53" y2="17.57" width="0.1524" layer="20" curve="-90"/>
<text>S +5 G</text>
<text>GND NC NC TX RX +5</text>
<text>Mav2Duplex 
Arduino Pro Mini Carrier
www.flynoevil.com</text>
</plain>
<libraries>
<library name="arduino">
<description>Arduino devices&lt;br&gt;
&lt;br&gt;
Based on the following sources:&lt;br&gt;
https://www.arduino.cc/en/Main/Products&lt;br&gt;
&lt;br&gt;
Author: Eugen Mihailescu&lt;br&gt;
Source code: https://github.com/../&lt;br&gt;</description>
<packages>
<package name="PROMINI">
<description>Arduino Pro Mini footprint</description>
</package>
</packages>
</library>
<library name="SM06B-GHS-TB(LF)(SN)">
<description>&lt;GH 1.25mm header side entry 6 way JST GH Series, 1.25mm Pitch 6 Way Right Angle PCB Header, Solder Termination, 1A&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SM06B-GHS-TB">
<description>&lt;b&gt;SM06B-GHS-TB&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSW-103-08-G-S-RA">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AR1" library="arduino" package="PROMINI" value="">
<attribute name="MF" value="ARDUINO"/>
<attribute name="MPN" value="MINI"/>
</element>
<element name="J1" library="SM06B-GHS-TB(LF)(SN)" package="SM06B-GHS-TB" value="SM06B-GHS-TB(LF)(SN)">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="GH 1.25mm header side entry 6 way JST GH Series, 1.25mm Pitch 6 Way Right Angle PCB Header, Solder Termination, 1A"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="JST (JAPAN SOLDERLESS TERMINALS)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SM06B-GHS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7521800"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="J2" library="con-samtec" package="TSW-103-08-G-S-RA" value="TSW-103-08-G-S-S-RA">
<attribute name="MF" value="Samtec Inc."/>
<attribute name="MPN" value="TSW-103-08-G-S-RA"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="6"/>
<contactref element="AR1" pad="GND@1"/>
<contactref element="AR1" pad="GND@0"/>
<contactref element="AR1" pad="GND@2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="1"/>
<contactref element="AR1" pad="RAW"/>
<contactref element="AR1" pad="VCC@1"/>
<contactref element="AR1" pad="VCC@0"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="AR1" pad="TXO@1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="RXI">
<contactref element="J1" pad="2"/>
<contactref element="AR1" pad="RXI@1"/>
</signal>
<signal name="SIG">
<contactref element="AR1" pad="D10"/>
<contactref element="J2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
