(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 8)
    (no_connects 0)
    (area 148.23 107.879999 178.24 122.503001)
    (thickness 1.6)
    (drawings 21)
    (tracks 10)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P2-Pad4)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x09 locked (layer F.Cu) (tedit 58A78AD5)
    (at 154.305 109.855 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Blinkt (at -2.54 10.16 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad4)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x09.wrl
      (at (xyz 0 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58A78B1B)
    (at 154.305 120.015 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Out (at 2.159 1.651 180) (layer B.SilkS))
    (fp_text value Out (at 2.54 0.635 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58A78C31)
    (at 167.005 120.015 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference In (at 2.159 7.747 180) (layer B.SilkS))
    (fp_text value In (at 2.54 0 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 58A78DD6)
    (at 162.052 116.84)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "Blinkt - this side" (at 2.032 -2.794) (layer F.SilkS))
    (fp_text value D.Out (at 4.064 -0.508) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text Ck (at 174.752 111.76) (layer F.SilkS))
  (gr_text Da (at 171.958 111.76) (layer F.SilkS))
  (gr_text Gnd (at 159.512 112.014) (layer F.SilkS))
  (gr_text 5v (at 154.178 112.014) (layer F.SilkS))
  (gr_text Da (at 174.752 121.666) (layer B.SilkS))
  (gr_text Da (at 162.052 121.666) (layer B.SilkS))
  (gr_text Ck (at 172.212 121.666) (layer B.SilkS))
  (gr_text Ck (at 159.258 121.666) (layer B.SilkS))
  (gr_text "Gnd\n" (at 169.672 121.666) (layer B.SilkS))
  (gr_text "Gnd\n" (at 156.718 121.666) (layer B.SilkS))
  (gr_text 5v (at 166.878 121.666) (layer B.SilkS))
  (gr_text 5v (at 154.432 121.666) (layer B.SilkS))
  (gr_text "Ipswich Makerspace\nipswichmakerspace.com" (at 175.768 112.268) (layer B.SilkS))
  (gr_line (start 153.416 108.204) (end 175.26 108.204) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 121.412) (end 152.4 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 122.428) (end 153.416 122.428) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.276 109.22) (end 176.276 121.412) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.26 121.412) (end 176.276 121.412) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.416 121.412) (end 153.416 122.428) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.416 109.22) (end 152.4 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.26 109.22) (end 175.26 108.204) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name "Net-(P1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 152.4 108.204) (xy 176.276 108.204) (xy 176.276 122.428) (xy 152.4 122.428)
      )
    )
  )
  (zone (net 2) (net_name "Net-(P1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 176.276 122.428) (xy 152.4 122.428) (xy 152.4 108.204) (xy 176.276 108.204)
      )
    )
  )
)
