(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 25)
    (zones 0)
    (modules 2)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
  )
  (module gwb-t400-breakout:PinHeader_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 615E39AD)
    (at 140.97 134.366 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at 3.048 -1.143 180) (layer F.Fab))
    (fp_text value Conn_01x07_Male (at 3.048 7.493 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gwb-t400-breakout:gwb_module (layer F.Cu) (tedit 615A6ACC)
    (at 127 127)
    (fp_text reference U1 (at -1 -3.81) (layer F.Fab))
    (fp_text value gwb-module (at -1 -6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 2 smd rect (at 2 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 3 smd rect (at 4 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at 6 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 8 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 6 smd rect (at 10 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 7 smd rect (at 12 0) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (gr_text v1.0 (at 133.35 127) (layer B.SilkS))
  (gr_text GND (at 140.97 132.842 90) (layer B.SilkS))
  (gr_text CS (at 138.43 132.842 90) (layer B.SilkS))
  (gr_text SCK (at 135.89 132.842 90) (layer B.SilkS))
  (gr_text MOSI (at 133.35 132.842 90) (layer B.SilkS))
  (gr_text MISO (at 130.81 132.842 90) (layer B.SilkS))
  (gr_text RST (at 128.27 132.842 90) (layer B.SilkS))
  (gr_text VCC (at 125.73 132.842 90) (layer B.SilkS))
  (gr_text "GWB T400\nBreakout" (at 133.35 123.444) (layer B.SilkS))
  (gr_line (start 124.46 135.636) (end 142.24 135.636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.46 124.46) (end 124.46 135.636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.46 124.46) (end 125.60046 123.31954) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.60046 123.31954) (end 125.60046 119.49938) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.09954 119.49938) (end 125.60046 119.49938) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.09954 123.31954) (end 141.09954 119.49938) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 124.46) (end 141.09954 123.31954) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 124.46) (end 142.24 135.636) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 140.97 132.842 90) (layer F.SilkS))
  (gr_text CS (at 138.43 132.842 90) (layer F.SilkS))
  (gr_text SCK (at 135.89 132.842 90) (layer F.SilkS))
  (gr_text MOSI (at 133.35 132.842 90) (layer F.SilkS))
  (gr_text MISO (at 130.81 132.842 90) (layer F.SilkS))
  (gr_text RST (at 128.27 132.842 90) (layer F.SilkS))
  (gr_text VCC (at 125.73 132.842 90) (layer F.SilkS))
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.494 135.89) (xy 124.206 135.89) (xy 124.206 119.126) (xy 142.621 119.126)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.621 136.017) (xy 124.079 136.017) (xy 124.079 118.999) (xy 142.748 118.999)
      )
    )
  )
)
