<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="0" x2="34.29" y2="0" width="0" layer="20"/>
<wire x1="38.1" y1="3.81" x2="38.1" y2="34.29" width="0" layer="20"/>
<wire x1="34.29" y1="38.1" x2="3.81" y2="38.1" width="0" layer="20"/>
<wire x1="0" y1="34.29" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="38.1" x2="0" y2="34.29" width="0" layer="20" curve="90"/>
<wire x1="38.1" y1="34.29" x2="34.29" y2="38.1" width="0" layer="20" curve="90"/>
<wire x1="34.29" y1="0" x2="38.1" y2="3.81" width="0" layer="20" curve="90"/>
<text>CC6-0503SR-E</text>
<text>3.3V</text>
<text>Ground</text>
<text>CC6-0503SR-E
5V in
3.3V at 1.8A out
6 Watt

1/2019
for DryDrop
Tino, J.R.</text>
</plain>
<libraries>
<library name="Tino_EAGLE_Library">
<packages>
<package name="CC61205SRE">
<description>&lt;b&gt;CC6-1205SR-E-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="ESQ-104-XX-X-S">
</package>
<package name="MT_2.75_6">
</package>
<package name="FRAMATOME_10118194-0001LF">
<description>changed P$12 and P$13 from SMT Pads to polygons on tMask and Top to avoid DRC error with TH pad overlaping SMT pad.</description>
</package>
<package name="LEDM1608X55">
<description>From SnapEDA.  Added 57 tCAD 3D line.  Changed outline to 3mm x 1.5 mm.  Enlarged and centered Cathode mark dot.</description>
</package>
<package name="RESC1608X55L25N">
<description>Resistor, Chip; 1.60 mm L X 0.80 mm W X 0.55 mm H body&lt;p&gt;&lt;i&gt;PCB Libraries Packages&lt;/i&gt;

edited to line up to 0.05mm grid per http://www.innofour.com/4003/news/literature/pcb-design-perfection-starts-in-the-cad-library/pcb-design-perfection-starts-in-the-cad-library-part-2</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Tino_EAGLE_Library" package="CC61205SRE" value="CC6-0503SR-E">
<attribute name="DESCRIPTION" value="Isolated DC/DC Converters 3W 3.3V 0.8A"/>
<attribute name="HEIGHT" value="8.8mm"/>
<attribute name="MANUFACTURER_NAME" value="TDK LAMBDA"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CC6-0503SR-E"/>
<attribute name="MOUSER_PART_NUMBER" value="967-CC6-0503SR-E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Tino_EAGLE_Library" package="ESQ-104-XX-X-S" value="3.3V">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MT1" library="Tino_EAGLE_Library" package="MT_2.75_6" value="MOUNTING_HOLE_RB_PI"/>
<element name="MT2" library="Tino_EAGLE_Library" package="MT_2.75_6" value="MOUNTING_HOLE_RB_PI"/>
<element name="MT3" library="Tino_EAGLE_Library" package="MT_2.75_6" value="MOUNTING_HOLE_RB_PI"/>
<element name="MT4" library="Tino_EAGLE_Library" package="MT_2.75_6" value="MOUNTING_HOLE_RB_PI"/>
<element name="J3" library="Tino_EAGLE_Library" package="ESQ-104-XX-X-S" value="GND">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Tino_EAGLE_Library" package="FRAMATOME_10118194-0001LF" value="10118194-0001LF">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value="Conn Micro USB Type B RCP 5 POS 0.65mm Solder RA SMD 5 Terminal 1 Port T/R"/>
<attribute name="MF" value="FCI"/>
<attribute name="MP" value="10118194-0001LF"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DIP-4 FCI"/>
<attribute name="PRICE" value="0.24 USD"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Tino_EAGLE_Library" package="LEDM1608X55" value="LED-LEDM1608X55">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="Tino_EAGLE_Library" package="RESC1608X55L25N" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="5V_IN">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="3.3V_OUT">
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
