(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 469)
    (zones 0)
    (modules 36)
    (nets 156)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 33.02 173.736)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00020_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U1-Pad10)")
  (net 3 "Net-(U1-Pad11)")
  (net 4 "Net-(U1-Pad7)")
  (net 5 "Net-(U1-Pad9)")
  (net 6 "Net-(U1-Pad43)")
  (net 7 "Net-(U1-Pad41)")
  (net 8 "Net-(U1-Pad30)")
  (net 9 "Net-(U1-Pad35)")
  (net 10 "Net-(U1-Pad37)")
  (net 11 "Net-(U1-Pad39)")
  (net 12 V3_3)
  (net 13 "Net-(U3-Pad10)")
  (net 14 "Net-(U3-Pad9)")
  (net 15 "Net-(C2-Pad1)")
  (net 16 "Net-(C5-Pad1)")
  (net 17 "Net-(C2-Pad2)")
  (net 18 "Net-(C3-Pad1)")
  (net 19 "Net-(C3-Pad2)")
  (net 20 "Net-(C4-Pad1)")
  (net 21 "Net-(C7-Pad1)")
  (net 22 "Net-(C10-Pad1)")
  (net 23 "Net-(C7-Pad2)")
  (net 24 "Net-(C8-Pad1)")
  (net 25 "Net-(C8-Pad2)")
  (net 26 "Net-(C9-Pad1)")
  (net 27 "Net-(J1-Pad2)")
  (net 28 "Net-(J1-Pad3)")
  (net 29 "Net-(J1-Pad4)")
  (net 30 "Net-(J1-Pad5)")
  (net 31 "Net-(J1-Pad6)")
  (net 32 /CPU/IM_RXDATA)
  (net 33 /CPU/IM_TXDATA)
  (net 34 /CPU/IM_ENABLE)
  (net 35 /CPU/RS232_TXDATA)
  (net 36 /CPU/RS232_RXCLK)
  (net 37 /CPU/RS232_RXDATA)
  (net 38 /CPU/RS232_TXCLK)
  (net 39 /CPU/RS232_CLKOUT)
  (net 40 /CPU/RS232_ENABLE)
  (net 41 "Net-(D3-Pad2)")
  (net 42 "Net-(D2-Pad2)")
  (net 43 "Net-(D1-Pad2)")
  (net 44 "Net-(D1-Pad1)")
  (net 45 "Net-(D2-Pad1)")
  (net 46 "Net-(D3-Pad1)")
  (net 47 "Net-(J4-Pad2)")
  (net 48 "Net-(J5-Pad25)")
  (net 49 "Net-(J5-Pad24)")
  (net 50 "Net-(J5-Pad23)")
  (net 51 "Net-(J5-Pad22)")
  (net 52 "Net-(J5-Pad21)")
  (net 53 "Net-(J5-Pad19)")
  (net 54 "Net-(J5-Pad18)")
  (net 55 "Net-(J5-Pad16)")
  (net 56 "Net-(J5-Pad14)")
  (net 57 "Net-(J5-Pad13)")
  (net 58 "Net-(J5-Pad12)")
  (net 59 "Net-(J5-Pad11)")
  (net 60 "Net-(J5-Pad10)")
  (net 61 "Net-(J5-Pad9)")
  (net 62 "Net-(J5-Pad8)")
  (net 63 "Net-(J5-Pad6)")
  (net 64 "Net-(J5-Pad5)")
  (net 65 "Net-(J6-Pad25)")
  (net 66 "Net-(J6-Pad24)")
  (net 67 "Net-(J6-Pad23)")
  (net 68 "Net-(J6-Pad21)")
  (net 69 "Net-(J6-Pad20)")
  (net 70 "Net-(J6-Pad19)")
  (net 71 "Net-(J6-Pad18)")
  (net 72 "Net-(J6-Pad16)")
  (net 73 "Net-(J6-Pad14)")
  (net 74 "Net-(J6-Pad13)")
  (net 75 "Net-(J6-Pad12)")
  (net 76 "Net-(J6-Pad11)")
  (net 77 "Net-(J6-Pad10)")
  (net 78 "Net-(J6-Pad9)")
  (net 79 "Net-(J6-Pad4)")
  (net 80 "Net-(TR2-Pad5)")
  (net 81 "/RS-232 I/O/RXD")
  (net 82 "/RS-232 I/O/TXD")
  (net 83 "/RS-232 I/O/RXCLK")
  (net 84 "/RS-232 I/O/CLKOUT")
  (net 85 "/RS-232 I/O/TXCLK")
  (net 86 "Net-(U1-Pad6)")
  (net 87 "Net-(U1-Pad5)")
  (net 88 "Net-(U1-Pad12)")
  (net 89 "/RS-232 I/O/RS232_1")
  (net 90 "/RS-232 I/O/RS232_0")
  (net 91 "Net-(J7-PadTT)")
  (net 92 "Net-(J7-PadSS)")
  (net 93 "Net-(J7-PadRR)")
  (net 94 "Net-(J7-PadPP)")
  (net 95 "Net-(J7-PadLL)")
  (net 96 "Net-(J7-PadKK)")
  (net 97 "Net-(J7-PadHH)")
  (net 98 "Net-(J7-PadEE)")
  (net 99 "Net-(J7-PadCC)")
  (net 100 "Net-(J7-PadBB)")
  (net 101 "Net-(J7-PadAA)")
  (net 102 "Net-(J7-PadZ)")
  (net 103 "Net-(J7-PadY)")
  (net 104 "Net-(J7-PadX)")
  (net 105 "Net-(J7-PadW)")
  (net 106 "Net-(J7-PadU)")
  (net 107 "Net-(J7-PadT)")
  (net 108 "Net-(J7-PadS)")
  (net 109 "Net-(J7-PadP)")
  (net 110 "Net-(J7-PadM)")
  (net 111 "Net-(J7-PadL)")
  (net 112 "Net-(J7-PadK)")
  (net 113 "Net-(J7-PadH)")
  (net 114 "Net-(J7-PadE)")
  (net 115 "Net-(J7-PadD)")
  (net 116 "Net-(J7-PadC)")
  (net 117 "/Integral modem/IM_RXD_N")
  (net 118 "/Integral modem/IM_TXD_N")
  (net 119 "Net-(U1-Pad26)")
  (net 120 "Net-(U1-Pad27)")
  (net 121 "Net-(U1-Pad29)")
  (net 122 "Net-(R6-Pad2)")
  (net 123 "Net-(U1-Pad21)")
  (net 124 "Net-(R6-Pad1)")
  (net 125 "Net-(TR1-Pad5)")
  (net 126 "Net-(TR1-Pad2)")
  (net 127 "Net-(TR2-Pad2)")
  (net 128 "Net-(J8-PadTT)")
  (net 129 "Net-(J8-PadSS)")
  (net 130 "Net-(J8-PadRR)")
  (net 131 "Net-(J8-PadPP)")
  (net 132 "Net-(J8-PadLL)")
  (net 133 "Net-(J8-PadKK)")
  (net 134 "Net-(J8-PadHH)")
  (net 135 "Net-(J8-PadEE)")
  (net 136 "Net-(J8-PadDD)")
  (net 137 "Net-(J8-PadCC)")
  (net 138 "Net-(J8-PadAA)")
  (net 139 "Net-(J8-PadY)")
  (net 140 "Net-(J8-PadW)")
  (net 141 "Net-(J8-PadV)")
  (net 142 "Net-(J8-PadU)")
  (net 143 "Net-(J8-PadS)")
  (net 144 "Net-(J8-PadP)")
  (net 145 "Net-(J8-PadM)")
  (net 146 "Net-(J8-PadL)")
  (net 147 "Net-(J8-PadK)")
  (net 148 "Net-(J8-PadH)")
  (net 149 "Net-(J8-PadE)")
  (net 150 "Net-(J8-PadD)")
  (net 151 "Net-(J8-PadC)")
  (net 152 "/Integral modem/IM_RXD")
  (net 153 "/Integral modem/IM_TXD")
  (net 154 "Net-(R7-Pad1)")
  (net 155 "Net-(R7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net /CPU/IM_ENABLE)
    (add_net /CPU/IM_RXDATA)
    (add_net /CPU/IM_TXDATA)
    (add_net /CPU/RS232_CLKOUT)
    (add_net /CPU/RS232_ENABLE)
    (add_net /CPU/RS232_RXCLK)
    (add_net /CPU/RS232_RXDATA)
    (add_net /CPU/RS232_TXCLK)
    (add_net /CPU/RS232_TXDATA)
    (add_net "/Integral modem/IM_RXD")
    (add_net "/Integral modem/IM_RXD_N")
    (add_net "/Integral modem/IM_TXD")
    (add_net "/Integral modem/IM_TXD_N")
    (add_net "/RS-232 I/O/CLKOUT")
    (add_net "/RS-232 I/O/RS232_0")
    (add_net "/RS-232 I/O/RS232_1")
    (add_net "/RS-232 I/O/RXCLK")
    (add_net "/RS-232 I/O/RXD")
    (add_net "/RS-232 I/O/TXCLK")
    (add_net "/RS-232 I/O/TXD")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad14)")
    (add_net "Net-(J5-Pad16)")
    (add_net "Net-(J5-Pad18)")
    (add_net "Net-(J5-Pad19)")
    (add_net "Net-(J5-Pad21)")
    (add_net "Net-(J5-Pad22)")
    (add_net "Net-(J5-Pad23)")
    (add_net "Net-(J5-Pad24)")
    (add_net "Net-(J5-Pad25)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net "Net-(J6-Pad10)")
    (add_net "Net-(J6-Pad11)")
    (add_net "Net-(J6-Pad12)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(J6-Pad16)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(J6-Pad19)")
    (add_net "Net-(J6-Pad20)")
    (add_net "Net-(J6-Pad21)")
    (add_net "Net-(J6-Pad23)")
    (add_net "Net-(J6-Pad24)")
    (add_net "Net-(J6-Pad25)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad9)")
    (add_net "Net-(J7-PadAA)")
    (add_net "Net-(J7-PadBB)")
    (add_net "Net-(J7-PadC)")
    (add_net "Net-(J7-PadCC)")
    (add_net "Net-(J7-PadD)")
    (add_net "Net-(J7-PadE)")
    (add_net "Net-(J7-PadEE)")
    (add_net "Net-(J7-PadH)")
    (add_net "Net-(J7-PadHH)")
    (add_net "Net-(J7-PadK)")
    (add_net "Net-(J7-PadKK)")
    (add_net "Net-(J7-PadL)")
    (add_net "Net-(J7-PadLL)")
    (add_net "Net-(J7-PadM)")
    (add_net "Net-(J7-PadP)")
    (add_net "Net-(J7-PadPP)")
    (add_net "Net-(J7-PadRR)")
    (add_net "Net-(J7-PadS)")
    (add_net "Net-(J7-PadSS)")
    (add_net "Net-(J7-PadT)")
    (add_net "Net-(J7-PadTT)")
    (add_net "Net-(J7-PadU)")
    (add_net "Net-(J7-PadW)")
    (add_net "Net-(J7-PadX)")
    (add_net "Net-(J7-PadY)")
    (add_net "Net-(J7-PadZ)")
    (add_net "Net-(J8-PadAA)")
    (add_net "Net-(J8-PadC)")
    (add_net "Net-(J8-PadCC)")
    (add_net "Net-(J8-PadD)")
    (add_net "Net-(J8-PadDD)")
    (add_net "Net-(J8-PadE)")
    (add_net "Net-(J8-PadEE)")
    (add_net "Net-(J8-PadH)")
    (add_net "Net-(J8-PadHH)")
    (add_net "Net-(J8-PadK)")
    (add_net "Net-(J8-PadKK)")
    (add_net "Net-(J8-PadL)")
    (add_net "Net-(J8-PadLL)")
    (add_net "Net-(J8-PadM)")
    (add_net "Net-(J8-PadP)")
    (add_net "Net-(J8-PadPP)")
    (add_net "Net-(J8-PadRR)")
    (add_net "Net-(J8-PadS)")
    (add_net "Net-(J8-PadSS)")
    (add_net "Net-(J8-PadTT)")
    (add_net "Net-(J8-PadU)")
    (add_net "Net-(J8-PadV)")
    (add_net "Net-(J8-PadW)")
    (add_net "Net-(J8-PadY)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(TR1-Pad2)")
    (add_net "Net-(TR1-Pad5)")
    (add_net "Net-(TR2-Pad2)")
    (add_net "Net-(TR2-Pad5)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad9)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net GND)
    (add_net V3_3)
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 121.2215 148.3487)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 2.4892 2.2479) (layer F.SilkS))
    (fp_text value 51 (at 7.62 2.4003) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(R7-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 120.4214 120.904)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -2.2098 0) (layer F.SilkS))
    (fp_text value 51 (at 12.5857 -0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 118.618 112.776 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 7.366 -2.413 90) (layer F.SilkS))
    (fp_text value 150 (at 0.3683 -2.4892 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 123.571 112.776 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 7.366 -2.286 90) (layer F.SilkS))
    (fp_text value 150 (at 0.3683 -2.1971 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 128.651 112.776 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 7.366 -2.286 90) (layer F.SilkS))
    (fp_text value 150 (at 0.5461 -2.3876 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 145.034 132.9944 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.0678 2.5654) (layer F.SilkS))
    (fp_text value 1M (at 2.8829 2.3749) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 60E9E7EC)
    (at 130.683 116.586 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 12.446 0) (layer F.SilkS))
    (fp_text value 1M (at -1.2573 1.9558) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:RPi_Pico_SMD_TH (layer F.Cu) (tedit 60DA360D)
    (at 93.218 126.492)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value Pico (at 0 2.159) (layer F.Fab))
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2) (layer Cmts.User))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at -5.7 23.5) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.7 23.5) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.7 -23.5) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.7 -23.5) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad 43 thru_hole oval (at 2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad43)"))
    (pad 43 smd rect (at 2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad43)"))
    (pad 42 thru_hole rect (at 0 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 42 smd rect (at 0 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 41 thru_hole oval (at -2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad41)"))
    (pad 41 smd rect (at -2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad41)"))
    (pad "" np_thru_hole oval (at 2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad 21 smd rect (at 8.89 24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 8.89 21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 33 /CPU/IM_TXDATA))
    (pad 23 smd rect (at 8.89 19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 8.89 16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 34 /CPU/IM_ENABLE))
    (pad 25 smd rect (at 8.89 13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 32 /CPU/IM_RXDATA))
    (pad 26 smd rect (at 8.89 11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 8.89 8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 8.89 6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 8.89 3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 8.89 1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 8.89 -1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D1-Pad2)"))
    (pad 32 smd rect (at 8.89 -3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (pad 33 smd rect (at 8.89 -6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 34 smd rect (at 8.89 -8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D3-Pad2)"))
    (pad 35 smd rect (at 8.89 -11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad35)"))
    (pad 36 smd rect (at 8.89 -13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 V3_3))
    (pad 37 smd rect (at 8.89 -16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 8.89 -19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 39 smd rect (at 8.89 -21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at 8.89 -24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad39)"))
    (pad 20 smd rect (at -8.89 24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 35 /CPU/RS232_TXDATA))
    (pad 19 smd rect (at -8.89 21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 36 /CPU/RS232_RXCLK))
    (pad 18 smd rect (at -8.89 19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -8.89 16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 37 /CPU/RS232_RXDATA))
    (pad 16 smd rect (at -8.89 13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 38 /CPU/RS232_TXCLK))
    (pad 15 smd rect (at -8.89 11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 39 /CPU/RS232_CLKOUT))
    (pad 14 smd rect (at -8.89 8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 40 /CPU/RS232_ENABLE))
    (pad 13 smd rect (at -8.89 6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -8.89 3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at -8.89 1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at -8.89 -1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -8.89 -3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -8.89 -6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -8.89 -8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at -8.89 -11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at -8.89 -13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -8.89 -16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J4-Pad2)"))
    (pad 3 smd rect (at -8.89 -19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -8.89 -21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-Pad4)"))
    (pad 1 smd rect (at -8.89 -24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1-Pad5)"))
    (pad 40 thru_hole oval (at 8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad39)"))
    (pad 39 thru_hole oval (at 8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad39)"))
    (pad 38 thru_hole rect (at 8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 37 thru_hole oval (at 8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad37)"))
    (pad 36 thru_hole oval (at 8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (pad 35 thru_hole oval (at 8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad35)"))
    (pad 34 thru_hole oval (at 8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 41 "Net-(D3-Pad2)"))
    (pad 33 thru_hole rect (at 8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 32 thru_hole oval (at 8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (pad 31 thru_hole oval (at 8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 43 "Net-(D1-Pad2)"))
    (pad 30 thru_hole oval (at 8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad30)"))
    (pad 29 thru_hole oval (at 8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 121 "Net-(U1-Pad29)"))
    (pad 28 thru_hole rect (at 8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 27 thru_hole oval (at 8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 120 "Net-(U1-Pad27)"))
    (pad 26 thru_hole oval (at 8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 119 "Net-(U1-Pad26)"))
    (pad 25 thru_hole oval (at 8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 /CPU/IM_RXDATA))
    (pad 24 thru_hole oval (at 8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 /CPU/IM_ENABLE))
    (pad 23 thru_hole rect (at 8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 /CPU/IM_TXDATA))
    (pad 21 thru_hole oval (at 8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 123 "Net-(U1-Pad21)"))
    (pad 20 thru_hole oval (at -8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 /CPU/RS232_TXDATA))
    (pad 19 thru_hole oval (at -8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 /CPU/RS232_RXCLK))
    (pad 18 thru_hole rect (at -8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at -8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 /CPU/RS232_RXDATA))
    (pad 16 thru_hole oval (at -8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 /CPU/RS232_TXCLK))
    (pad 15 thru_hole oval (at -8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 /CPU/RS232_CLKOUT))
    (pad 14 thru_hole oval (at -8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 /CPU/RS232_ENABLE))
    (pad 13 thru_hole rect (at -8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at -8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 88 "Net-(U1-Pad12)"))
    (pad 11 thru_hole oval (at -8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad11)"))
    (pad 10 thru_hole oval (at -8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad10)"))
    (pad 9 thru_hole oval (at -8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad9)"))
    (pad 8 thru_hole rect (at -8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at -8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad7)"))
    (pad 6 thru_hole oval (at -8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 86 "Net-(U1-Pad6)"))
    (pad 5 thru_hole oval (at -8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 87 "Net-(U1-Pad5)"))
    (pad 4 thru_hole oval (at -8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad2)"))
    (pad 3 thru_hole rect (at -8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at -8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad4)"))
    (pad 1 thru_hole oval (at -8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad5)"))
    (model "${KIPRJMOD}/ddcmp_parts/Raspberry Pi Pico-R3.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module ddcmp_parts:AK_Design_9mm (layer F.Cu) (tedit 5EC6EF5E)
    (at 136.8806 124.9172)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value AK_Design_9mm (at 0 -0.5) (layer F.Fab) hide)
  )
  (module ddcmp_parts:Amphenol_DB25F_PCB (layer F.Cu) (tedit 60D9E921)
    (at 77.47 161.036)
    (descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm")
    (fp_text reference J6 (at -16.62 -2.8) (layer F.SilkS))
    (fp_text value DCE (at -16.62 20.81) (layer F.Fab))
    (fp_text user %R (at -16.62 16.225) (layer F.Fab))
    (pad 0 thru_hole circle (at 6.9 1.27) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at -40.14 1.27) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at -31.855 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(J6-Pad25)"))
    (pad 24 thru_hole circle (at -29.085 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(J6-Pad24)"))
    (pad 23 thru_hole circle (at -26.315 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "Net-(J6-Pad23)"))
    (pad 22 thru_hole circle (at -23.545 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 90 "/RS-232 I/O/RS232_0"))
    (pad 21 thru_hole circle (at -20.775 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(J6-Pad21)"))
    (pad 20 thru_hole circle (at -18.005 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(J6-Pad20)"))
    (pad 19 thru_hole circle (at -15.235 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(J6-Pad19)"))
    (pad 18 thru_hole circle (at -12.465 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(J6-Pad18)"))
    (pad 17 thru_hole circle (at -9.695 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 "/RS-232 I/O/CLKOUT"))
    (pad 16 thru_hole circle (at -6.925 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(J6-Pad16)"))
    (pad 15 thru_hole circle (at -4.155 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 "/RS-232 I/O/CLKOUT"))
    (pad 14 thru_hole circle (at -1.385 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(J6-Pad14)"))
    (pad 13 thru_hole circle (at -33.24 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(J6-Pad13)"))
    (pad 12 thru_hole circle (at -30.47 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(J6-Pad12)"))
    (pad 11 thru_hole circle (at -27.7 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(J6-Pad11)"))
    (pad 10 thru_hole circle (at -24.93 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(J6-Pad10)"))
    (pad 9 thru_hole circle (at -22.16 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(J6-Pad9)"))
    (pad 8 thru_hole circle (at -19.39 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad 7 thru_hole circle (at -16.62 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -13.85 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad 5 thru_hole circle (at -11.08 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad 4 thru_hole circle (at -8.31 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(J6-Pad4)"))
    (pad 3 thru_hole circle (at -5.54 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 82 "/RS-232 I/O/TXD"))
    (pad 2 thru_hole circle (at -2.77 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "/RS-232 I/O/RXD"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:Berg_40_pin_DEC_pinout (layer F.Cu) (tedit 60BA93D3)
    (at 142.0368 156.7688 270)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J8 (at -4.572 -2.7432 180) (layer F.SilkS))
    (fp_text value "To LU" (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad VV thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad UU thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad TT thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(J8-PadTT)"))
    (pad SS thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(J8-PadSS)"))
    (pad RR thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(J8-PadRR)"))
    (pad PP thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(J8-PadPP)"))
    (pad NN thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 "/Integral modem/IM_TXD"))
    (pad MM thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad LL thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(J8-PadLL)"))
    (pad KK thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(J8-PadKK)"))
    (pad JJ thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 152 "/Integral modem/IM_RXD"))
    (pad HH thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(J8-PadHH)"))
    (pad FF thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (pad EE thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J8-PadEE)"))
    (pad DD thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(J8-PadDD)"))
    (pad CC thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(J8-PadCC)"))
    (pad BB thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad AA thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J8-PadAA)"))
    (pad Z thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad Y thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(J8-PadY)"))
    (pad X thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "/RS-232 I/O/RS232_0"))
    (pad W thru_hole oval (at 2.54 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(J8-PadW)"))
    (pad V thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(J8-PadV)"))
    (pad U thru_hole oval (at 2.54 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(J8-PadU)"))
    (pad T thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad S thru_hole oval (at 2.54 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(J8-PadS)"))
    (pad R thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "/RS-232 I/O/CLKOUT"))
    (pad P thru_hole oval (at 2.54 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(J8-PadP)"))
    (pad N thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "/RS-232 I/O/CLKOUT"))
    (pad M thru_hole oval (at 2.54 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(J8-PadM)"))
    (pad L thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(J8-PadL)"))
    (pad K thru_hole oval (at 2.54 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(J8-PadK)"))
    (pad J thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "/RS-232 I/O/TXD"))
    (pad H thru_hole oval (at 2.54 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(J8-PadH)"))
    (pad F thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "/RS-232 I/O/RXD"))
    (pad E thru_hole oval (at 2.54 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(J8-PadE)"))
    (pad D thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(J8-PadD)"))
    (pad C thru_hole oval (at 2.54 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(J8-PadC)"))
    (pad B thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A thru_hole oval (at 2.54 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/ddcmp_parts/BERG_blue_40pin.step
      (offset (xyz -10.3 7.55 -3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module ddcmp_parts:Mini-Circuits_CD637_X65 (layer F.Cu) (tedit 60BE5F2D)
    (at 126.7714 128.016 180)
    (descr https://ww2.minicircuits.com/case_style/CD637.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference TR1 (at 0 -4.826) (layer F.SilkS))
    (fp_text value TT1-6-X65+ (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 3.81 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(R6-Pad2)"))
    (pad 5 thru_hole circle (at 3.81 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(TR1-Pad5)"))
    (pad 4 thru_hole circle (at 3.81 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(R6-Pad1)"))
    (pad 3 thru_hole circle (at -3.81 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 152 "/Integral modem/IM_RXD"))
    (pad 2 thru_hole circle (at -3.81 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(TR1-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (pad 6 smd rect (at 2.54 -2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at 2.54 0 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(TR1-Pad5)"))
    (pad 4 smd rect (at 2.54 2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R6-Pad1)"))
    (pad 3 smd rect (at -2.54 2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 152 "/Integral modem/IM_RXD"))
    (pad 2 smd rect (at -2.54 0 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(TR1-Pad2)"))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (model ${KIPRJMOD}/ddcmp_parts/CD637.step
      (offset (xyz -2.8 3.935 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 0 90))
    )
  )
  (module ddcmp_parts:Mini-Circuits_CD637_X65 (layer F.Cu) (tedit 60BE5F2D)
    (at 126.7968 141.2494 180)
    (descr https://ww2.minicircuits.com/case_style/CD637.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference TR2 (at 0.0254 5.08) (layer F.SilkS))
    (fp_text value TT1-6-X65+ (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 3.81 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(R7-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(TR2-Pad5)"))
    (pad 4 thru_hole circle (at 3.81 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(R7-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad 2 thru_hole circle (at -3.81 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(TR2-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 153 "/Integral modem/IM_TXD"))
    (pad 6 smd rect (at 2.54 -2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(R7-Pad1)"))
    (pad 5 smd rect (at 2.54 0 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(TR2-Pad5)"))
    (pad 4 smd rect (at 2.54 2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(R7-Pad2)"))
    (pad 3 smd rect (at -2.54 2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad 2 smd rect (at -2.54 0 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(TR2-Pad2)"))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 153 "/Integral modem/IM_TXD"))
    (model ${KIPRJMOD}/ddcmp_parts/CD637.step
      (offset (xyz -2.8 3.935 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 0 90))
    )
  )
  (module ddcmp_parts:Berg_40_pin_DEC_pinout (layer F.Cu) (tedit 60BA93D3)
    (at 141.986 166.9796 270)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J7 (at -3.8608 -2.9718 180) (layer F.SilkS))
    (fp_text value "To BC55" (at 1.27 50.59 270) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad VV thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad UU thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad TT thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(J7-PadTT)"))
    (pad SS thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(J7-PadSS)"))
    (pad RR thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(J7-PadRR)"))
    (pad PP thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(J7-PadPP)"))
    (pad NN thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 152 "/Integral modem/IM_RXD"))
    (pad MM thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (pad LL thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(J7-PadLL)"))
    (pad KK thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J7-PadKK)"))
    (pad JJ thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 "/Integral modem/IM_TXD"))
    (pad HH thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(J7-PadHH)"))
    (pad FF thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad EE thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(J7-PadEE)"))
    (pad DD thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad CC thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(J7-PadCC)"))
    (pad BB thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(J7-PadBB)"))
    (pad AA thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(J7-PadAA)"))
    (pad Z thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(J7-PadZ)"))
    (pad Y thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(J7-PadY)"))
    (pad X thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(J7-PadX)"))
    (pad W thru_hole oval (at 2.54 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(J7-PadW)"))
    (pad V thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad U thru_hole oval (at 2.54 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(J7-PadU)"))
    (pad T thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(J7-PadT)"))
    (pad S thru_hole oval (at 2.54 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(J7-PadS)"))
    (pad R thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "/RS-232 I/O/RXCLK"))
    (pad P thru_hole oval (at 2.54 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(J7-PadP)"))
    (pad N thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "/RS-232 I/O/TXCLK"))
    (pad M thru_hole oval (at 2.54 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(J7-PadM)"))
    (pad L thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(J7-PadL)"))
    (pad K thru_hole oval (at 2.54 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(J7-PadK)"))
    (pad J thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "/RS-232 I/O/RXD"))
    (pad H thru_hole oval (at 2.54 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(J7-PadH)"))
    (pad F thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "/RS-232 I/O/TXD"))
    (pad E thru_hole oval (at 2.54 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(J7-PadE)"))
    (pad D thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(J7-PadD)"))
    (pad C thru_hole oval (at 2.54 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(J7-PadC)"))
    (pad B thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A thru_hole oval (at 2.54 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/ddcmp_parts/BERG_blue_40pin.step
      (offset (xyz -10.3 7.55 -3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 70.993 131.445)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 4.699 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.937 -2.032) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 116.078 128.651 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C11 (at 5.207 -0.127) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 68.072 103.124 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C10 (at 5.334 0.508) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 60.96 123.19 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C9 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 60.96 116.84 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C8 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 60.96 110.49 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C7-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 73.66 103.124 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C6 (at -2.159 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 67.818 131.445 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 4.699 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 4.953 1.778) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C5-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 60.96 151.765 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 60.96 145.415 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 60B6D91F)
    (at 60.96 139.065 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (model ${KIPRJMOD}/ddcmp_parts/kemet_cap.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:Amphenol_DB25M_PCB (layer F.Cu) (tedit 60D9E936)
    (at 45.72 113.284 270)
    (descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm")
    (fp_text reference J5 (at 16.62 -2.8 90) (layer F.SilkS))
    (fp_text value DTE (at 16.62 20.64 90) (layer F.Fab))
    (fp_text user %R (at 16.62 16.14 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 40.14 1.27 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at -6.9 1.27 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at 31.855 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "Net-(J5-Pad25)"))
    (pad 24 thru_hole circle (at 29.085 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(J5-Pad24)"))
    (pad 23 thru_hole circle (at 26.315 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad23)"))
    (pad 22 thru_hole circle (at 23.545 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(J5-Pad22)"))
    (pad 21 thru_hole circle (at 20.775 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(J5-Pad21)"))
    (pad 20 thru_hole circle (at 18.005 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad 19 thru_hole circle (at 15.235 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(J5-Pad19)"))
    (pad 18 thru_hole circle (at 12.465 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 "Net-(J5-Pad18)"))
    (pad 17 thru_hole circle (at 9.695 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 "/RS-232 I/O/RXCLK"))
    (pad 16 thru_hole circle (at 6.925 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(J5-Pad16)"))
    (pad 15 thru_hole circle (at 4.155 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 85 "/RS-232 I/O/TXCLK"))
    (pad 14 thru_hole circle (at 1.385 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(J5-Pad14)"))
    (pad 13 thru_hole circle (at 33.24 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(J5-Pad13)"))
    (pad 12 thru_hole circle (at 30.47 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(J5-Pad12)"))
    (pad 11 thru_hole circle (at 27.7 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(J5-Pad11)"))
    (pad 10 thru_hole circle (at 24.93 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(J5-Pad10)"))
    (pad 9 thru_hole circle (at 22.16 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(J5-Pad9)"))
    (pad 8 thru_hole circle (at 19.39 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(J5-Pad8)"))
    (pad 7 thru_hole circle (at 16.62 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 13.85 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(J5-Pad6)"))
    (pad 5 thru_hole circle (at 11.08 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(J5-Pad5)"))
    (pad 4 thru_hole circle (at 8.31 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad 3 thru_hole circle (at 5.54 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "/RS-232 I/O/RXD"))
    (pad 2 thru_hole circle (at 2.77 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 82 "/RS-232 I/O/TXD"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Male_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 60D9E968)
    (at 77.47 111.125)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value TEST (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:LED_D3.0mm (layer F.Cu) (tedit 60A5A572)
    (at 112.268 108.331 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value TX (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(D3-Pad2)"))
    (model ${KIPRJMOD}/ddcmp_parts/LED_D3.0mm_red.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:LED_D3.0mm (layer F.Cu) (tedit 60A5A572)
    (at 112.268 114.681 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value RX (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(D2-Pad2)"))
    (model ${KIPRJMOD}/ddcmp_parts/LED_D3.0mm_yellow.step
      (at (xyz 0 0 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:LED_D3.0mm (layer F.Cu) (tedit 60A5A572)
    (at 112.268 121.031 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value SYN (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(D1-Pad2)"))
    (model ${KIPRJMOD}/ddcmp_parts/LED_D3.0mm_green.step
      (at (xyz 0 0 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 60D9E975)
    (at 53.848 117.348 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value UART (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:BNC_Molex_J_RA_PCB (layer F.Cu) (tedit 60A69344)
    (at 135.2042 140.97 270)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J3 (at -2.7 -1.2 90) (layer F.SilkS))
    (fp_text value TX (at 0 6 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.8 -7.8 270) (size 3.5 3.5) (drill 1.8) (layers *.Cu *.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad 2 thru_hole circle (at 3.8 -7.8 270) (size 3.5 3.5) (drill 1.8) (layers *.Cu *.Mask)
      (net 118 "/Integral modem/IM_TXD_N"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask)
      (net 153 "/Integral modem/IM_TXD"))
    (model ${KIPRJMOD}/ddcmp_parts/731000105.step
      (offset (xyz 0 12.58 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module ddcmp_parts:BNC_Molex_J_RA_PCB (layer F.Cu) (tedit 60A69344)
    (at 135.2042 113.03 270)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J2 (at -2.7 -1.2 90) (layer F.SilkS))
    (fp_text value RX (at 0 6 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.8 -7.8 270) (size 3.5 3.5) (drill 1.8) (layers *.Cu *.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (pad 2 thru_hole circle (at 3.8 -7.8 270) (size 3.5 3.5) (drill 1.8) (layers *.Cu *.Mask)
      (net 117 "/Integral modem/IM_RXD_N"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask)
      (net 152 "/Integral modem/IM_RXD"))
    (model ${KIPRJMOD}/ddcmp_parts/731000105.step
      (offset (xyz 0 12.58 3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module ddcmp_parts:DIP-18_W7.62mm (layer F.Cu) (tedit 60A51DA4)
    (at 65.405 106.68)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 9.779 -0.889) (layer F.SilkS))
    (fp_text value MAX3222 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /CPU/RS232_TXCLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C7-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C10-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /CPU/RS232_CLKOUT))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /CPU/RS232_RXCLK))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C8-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "/RS-232 I/O/RXCLK"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "/RS-232 I/O/CLKOUT"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "/RS-232 I/O/RS232_0"))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "/RS-232 I/O/TXCLK"))
    (pad 18 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /CPU/RS232_ENABLE))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:DIP-18_W7.62mm (layer F.Cu) (tedit 60A51DA4)
    (at 65.278 135.255)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 9.906 -0.762) (layer F.SilkS))
    (fp_text value MAX3222 (at 3.81 22.65) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U3-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /CPU/RS232_TXDATA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C5-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /CPU/RS232_ENABLE))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C2-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /CPU/RS232_RXDATA))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C3-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "/RS-232 I/O/RXD"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C3-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "/RS-232 I/O/RS232_1"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "/RS-232 I/O/TXD"))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U3-Pad9)"))
    (pad 18 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /CPU/RS232_ENABLE))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-18_W7.62mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ddcmp_parts:DIP-14_W7.62mm (layer F.Cu) (tedit 60A51DE1)
    (at 110.998 133.096)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value max3491ecpd (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CPU/IM_RXDATA))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(R7-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(R7-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /CPU/IM_ENABLE))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(R6-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /CPU/IM_TXDATA))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(R6-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 V3_3))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "To BC55" (at 126.0094 163.0172) (layer F.SilkS))
  (gr_text "To LU" (at 126.0094 152.4) (layer F.SilkS))
  (gr_text SYN (at 108.4072 122.2756) (layer F.SilkS))
  (gr_text "AK-005 A" (at 93.472 132.8674) (layer B.Cu))
  (gr_text "AK-005 A" (at 140.5382 128.5748) (layer F.Cu))
  (gr_text RX (at 108.4072 115.8748) (layer F.SilkS))
  (gr_text TX (at 108.4072 109.7026) (layer F.SilkS))
  (gr_text "DDCMP Framer\nPaul Koning, NI1D\nJuly 2021" (at 131.699 103.632) (layer F.SilkS))
  (gr_text TEST (at 77.978 116.332) (layer F.SilkS))
  (gr_text "Debug\nUART" (at 56.134 105.156) (layer F.SilkS))
  (gr_text TX (at 145.2372 147.9296) (layer F.SilkS))
  (gr_text RX (at 144.4498 120.0658) (layer F.SilkS))
  (gr_text DTE (at 50.038 135.128) (layer F.SilkS))
  (gr_text DCE (at 54.61 157.48) (layer F.SilkS))
  (gr_line (start 147.574 100.076) (end 33.02 100.076) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.574 173.736) (end 147.574 100.076) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 33.02 173.736) (end 147.574 173.736) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 33.02 100.076) (end 33.02 173.736) (layer Edge.Cuts) (width 0.05))
)
