(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 59)
    (tracks 730)
    (zones 0)
    (modules 101)
    (nets 119)
  )
  (page A3)
  (title_block
    (date "15 nov 2012")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.9)
    (via_drill 0.6)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (user_via 0.6 0.4)
    (uvia_size 0.5)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.1)
    (pcb_text_width 0.1)
    (pcb_text_size 0.75 0.75)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.1)
    (pad_size 3.96 3.96)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 200 150)
    (grid_origin 200 150)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 +5V)
  (net 3 GND)
  (net 4 "Net-(BT1-Pad1)")
  (net 5 +12V)
  (net 6 "Net-(C2-Pad1)")
  (net 7 +3.3VP)
  (net 8 "Net-(C7-Pad1)")
  (net 9 +5VP)
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C11-Pad1)")
  (net 12 "Net-(C11-Pad2)")
  (net 13 "Net-(C17-Pad2)")
  (net 14 "Net-(C17-Pad1)")
  (net 15 "Net-(C18-Pad1)")
  (net 16 /Vled)
  (net 17 "Net-(C19-Pad2)")
  (net 18 "Net-(D1-Pad1)")
  (net 19 "Net-(D1-Pad2)")
  (net 20 "Net-(D2-Pad2)")
  (net 21 /VALVE)
  (net 22 "Net-(D4-Pad2)")
  (net 23 "Net-(D4-Pad1)")
  (net 24 "Net-(FB1-Pad1)")
  (net 25 "Net-(FB2-Pad2)")
  (net 26 "Net-(FB3-Pad1)")
  (net 27 "Net-(FB4-Pad2)")
  (net 28 /LS1)
  (net 29 /LS2)
  (net 30 /SERVO_PWM)
  (net 31 /S4)
  (net 32 /S3)
  (net 33 /S2)
  (net 34 /S1)
  (net 35 "Net-(J2-Pad2)")
  (net 36 /SCL)
  (net 37 /SDA)
  (net 38 /FAN)
  (net 39 +12VA)
  (net 40 "Net-(P1-Pad6)")
  (net 41 "Net-(P1-Pad8)")
  (net 42 "Net-(P1-Pad9)")
  (net 43 "Net-(P1-Pad10)")
  (net 44 /LED_IND)
  (net 45 "Net-(P1-Pad14)")
  (net 46 /DRV_SLEEP)
  (net 47 /DRV_RESET)
  (net 48 /DRV_FAULT)
  (net 49 /STEP)
  (net 50 /DIR)
  (net 51 "Net-(P1-Pad27)")
  (net 52 "Net-(P1-Pad28)")
  (net 53 /FAN_GPIO)
  (net 54 "Net-(P1-Pad30)")
  (net 55 "Net-(P1-Pad31)")
  (net 56 /LED_PWM)
  (net 57 "Net-(P1-Pad34)")
  (net 58 /PWR_GPIO)
  (net 59 /VALVE_GPIO)
  (net 60 "Net-(Q1-Pad2)")
  (net 61 "Net-(Q2-Pad2)")
  (net 62 "Net-(Q3-Pad1)")
  (net 63 "Net-(Q4-Pad1)")
  (net 64 "Net-(R3-Pad2)")
  (net 65 /DRV_Vref)
  (net 66 /PGood_Pi_3V3)
  (net 67 /PGood_Pi_5V)
  (net 68 "Net-(R7-Pad2)")
  (net 69 "Net-(R8-Pad2)")
  (net 70 /PGood_LED_5V)
  (net 71 /PGood_LED_3V3)
  (net 72 "Net-(SW2-Pad4)")
  (net 73 "Net-(SW2-Pad5)")
  (net 74 "Net-(SW2-Pad6)")
  (net 75 "Net-(U1-Pad1)")
  (net 76 "Net-(U1-Pad3)")
  (net 77 "Net-(U1-Pad4)")
  (net 78 "Net-(U2-PadC1)")
  (net 79 "Net-(U2-PadE1)")
  (net 80 "Net-(U2-PadE2)")
  (net 81 "Net-(U2-PadE5)")
  (net 82 "Net-(U3-Pad19)")
  (net 83 "Net-(U3-Pad23)")
  (net 84 "Net-(U3-Pad27)")
  (net 85 "Net-(U4-PadE5)")
  (net 86 "Net-(U4-PadE2)")
  (net 87 "Net-(U4-PadE1)")
  (net 88 "Net-(U5-Pad3)")
  (net 89 "Net-(U5-Pad6)")
  (net 90 "Net-(P1-Pad24)")
  (net 91 "Net-(P1-Pad26)")
  (net 92 "Net-(P1-Pad19)")
  (net 93 "Net-(P1-Pad21)")
  (net 94 /R_VALVE)
  (net 95 /R_LS1)
  (net 96 /R_S1)
  (net 97 /R_S2)
  (net 98 /R_S4)
  (net 99 /R_S3)
  (net 100 /R_SERVO_PWM)
  (net 101 /R_LS2)
  (net 102 "Net-(J8-Pad1)")
  (net 103 "Net-(R23-Pad1)")
  (net 104 "Net-(R24-Pad1)")
  (net 105 /DRV_EN)
  (net 106 "Net-(P1-Pad23)")
  (net 107 "Net-(P1-Pad25)")
  (net 108 /INT)
  (net 109 /R_SCL)
  (net 110 /R_SDA)
  (net 111 /R_INT)
  (net 112 "Net-(P1-Pad13)")
  (net 113 "Net-(P1-Pad15)")
  (net 114 +R_12V)
  (net 115 R_GND)
  (net 116 +R_3V3)
  (net 117 +R_5V)
  (net 118 +3.3VA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.9)
    (via_drill 0.6)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net +3.3VA)
    (add_net +R_12V)
    (add_net +R_3V3)
    (add_net +R_5V)
    (add_net /DIR)
    (add_net /DRV_EN)
    (add_net /DRV_FAULT)
    (add_net /DRV_RESET)
    (add_net /DRV_SLEEP)
    (add_net /DRV_Vref)
    (add_net /FAN_GPIO)
    (add_net /INT)
    (add_net /LED_IND)
    (add_net /LS1)
    (add_net /LS2)
    (add_net /PGood_LED_3V3)
    (add_net /PGood_LED_5V)
    (add_net /PGood_Pi_3V3)
    (add_net /PGood_Pi_5V)
    (add_net /PWR_GPIO)
    (add_net /R_INT)
    (add_net /R_LS1)
    (add_net /R_LS2)
    (add_net /R_SCL)
    (add_net /R_SDA)
    (add_net /R_SERVO_PWM)
    (add_net /R_VALVE)
    (add_net /STEP)
    (add_net /VALVE)
    (add_net /VALVE_GPIO)
    (add_net /Vled)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad25)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad30)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad34)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(SW2-Pad4)")
    (add_net "Net-(SW2-Pad5)")
    (add_net "Net-(SW2-Pad6)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-PadC1)")
    (add_net "Net-(U2-PadE1)")
    (add_net "Net-(U2-PadE2)")
    (add_net "Net-(U2-PadE5)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U4-PadE1)")
    (add_net "Net-(U4-PadE2)")
    (add_net "Net-(U4-PadE5)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U5-Pad6)")
    (add_net R_GND)
  )
  (net_class Comms ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.9)
    (via_drill 0.6)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net /LED_PWM)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SERVO_PWM)
  )
  (net_class Motors ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.9)
    (via_drill 0.6)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net /FAN)
    (add_net /R_S1)
    (add_net /R_S2)
    (add_net /R_S3)
    (add_net /R_S4)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net /S4)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.7)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +12VA)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net +5V)
    (add_net +5VP)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(FB1-Pad1)")
    (add_net "Net-(FB2-Pad2)")
    (add_net "Net-(FB3-Pad1)")
    (add_net "Net-(FB4-Pad2)")
  )
  (module ulc-mm:L_Bourns_SRP1245A (layer B.Cu) (tedit 61AA65D1)
    (at 236.5506 136.411 90)
    (descr "Bourns SRP1245A series SMD inductor http://www.bourns.com/docs/Product-Datasheets/SRP1245A.pdf")
    (tags "Bourns SRP1245A SMD inductor")
    (attr smd)
    (fp_text reference L1 (at 8.2296 -0.381 180) (layer B.SilkS))
    (fp_text value "22 uH" (at 0 -7.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -5.625 0 90) (size 3.25 5) (layers B.Cu B.Paste B.Mask)
      (net 39 +12VA))
    (pad 2 smd rect (at 5.625 0 90) (size 3.25 5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRP1245A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Logos:logos (layer F.Cu) (tedit 0)
    (at 313.919 117.615 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Logos:logos (layer F.Cu) (tedit 0)
    (at 230.1498 146.2154)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module ulc-mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6193770F)
    (at 267.1322 131.4072 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 8.8138 180) (layer F.SilkS))
    (fp_text value 12V_WALL (at -0.0254 9.7536) (layer F.Fab))
    (fp_text user %R (at 0.0762 2.3622 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.48 2.48) (drill 1.78) (layers *.Cu *.Mask)
      (net 39 +12VA))
    (pad 2 thru_hole oval (at 0 6.35 180) (size 2.5 2.5) (drill 1.78) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/010844020.stp
      (offset (xyz 0 -3.25 7))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module ulc-mm:CP_EIA-3216-10_Kemet-I (layer B.Cu) (tedit 61930D00)
    (at 224.7904 139.6876)
    (descr "Tantalum Capacitor SMD Kemet-I (3216-10 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C7 (at -5.207 0 270) (layer B.SilkS))
    (fp_text value 150uF (at 0.1524 -4.4958) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -2.95 0) (size 2.3 6.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.185)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at 2.95 0) (size 2.3 6.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.185)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-10_Kemet-I.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mini-Fit_Jr_5566-02A_2x01_P4.20mm_Vertical (layer F.Cu) (tedit 5B781992)
    (at 209.0424 125.7938 180)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-02A, example for new mpn: 39-28-x02x, 1 Pins per row, Mounting:  (http://www.molex.com/pdm_docs/sd/039281043_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entry")
    (fp_text reference J13 (at 0.2032 -3.429 180) (layer F.SilkS))
    (fp_text value 12V_SWITCH (at 2.1 9.95) (layer F.Fab))
    (fp_text user %R (at 2.1 -1.55) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5.5 180) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.09259299999999999)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/039281023.stp
      (offset (xyz 0 -3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 261.5 97.5 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK2 (at 1.556 -3.478) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 208.37 98.77 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference P1 (at 2.208 1.512) (layer B.SilkS))
    (fp_text value RPi_Shield (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5VP))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /SDA))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5VP))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SCL))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /PWR_GPIO))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 /INT))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /LED_IND))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /LS2))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 +3.3VA))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /LS1))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P1-Pad21)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /VALVE_GPIO))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(P1-Pad23)"))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P1-Pad24)"))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(P1-Pad25)"))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P1-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P1-Pad27)"))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P1-Pad28)"))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /FAN_GPIO))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P1-Pad30)"))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P1-Pad31)"))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /SERVO_PWM))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /LED_PWM))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P1-Pad34)"))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /STEP))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /DRV_FAULT))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 /DRV_EN))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /DIR))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /DRV_SLEEP))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /DRV_RESET))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 261.5 146.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK4 (at -3.75 0 90) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 203.5 146.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK3 (at 4.0184 -0.0052 90) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 203.5 97.5 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK1 (at 0 -3.7 180) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module ulc-mm:Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles (layer F.Cu) (tedit 617336B9)
    (at 209.652 138.0112)
    (descr "Panasonic CR-1220/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D140.pdf")
    (tags "battery CR-1220 coin cell vertical")
    (fp_text reference BT1 (at 1.625 -4) (layer F.SilkS))
    (fp_text value CR1220 (at 0 3.2258) (layer F.Fab))
    (pad MP smd rect (at 0 0) (size 3.96 3.96) (layers F.Cu F.Paste F.Mask))
    (pad 2 thru_hole circle (at -6.6 0) (size 3.96 3.96) (drill 1.85) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 6.6 0) (size 3.96 3.96) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/Battery_CR1225.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer B.Cu) (tedit 5B301BBE)
    (at 213.5128 118.7326 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.3302 1.9558 90) (layer B.SilkS))
    (fp_text value "10 uF" (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 255.9308 114.9226)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.2352 0.127) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 266.04 106.4644 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.1524 -1.4732 90) (layer F.SilkS))
    (fp_text value "0.47 uF" (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3.3VP))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 211.6 114.8 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.2 -1.4 90) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 263.2 115.24 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.8956 0.0254 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 259.97 118.95 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at 0.603 3.5052 180) (layer F.SilkS))
    (fp_text value "47 uF" (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 217.272 114.3638 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 2.672 -0.0362 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +5VP))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer B.Cu) (tedit 5B301BBE)
    (at 233.4264 121.6282 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 3.8862 0.0254 270) (layer B.SilkS))
    (fp_text value "10 uF" (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 5 +12V))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 247.117 119.4946 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0.9906 1.651 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 216.7 105.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0.7 -1.3) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 257.8 141.65)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.0506 1.7822 180) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +5V))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 257.65 139.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -2.6 0 180) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 261.595 135.6744)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0.0254 -1.27) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C17-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 260.8 138.9002 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 1.7018 -1.2522 270) (layer F.SilkS))
    (fp_text value "82 nF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 257.5 130.05)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -3 -0.2 270) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(C19-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 /Vled))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 229.6672 141.6942 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 1.9812) (layer F.SilkS) hide)
    (fp_text value "E POWER" (at 0 1.8) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 229.7434 134.379 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.82) (layer F.SilkS) hide)
    (fp_text value "STATUS IND" (at -0.2 2) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMB (layer F.Cu) (tedit 58645DF3)
    (at 295.8215 118.6945)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D3 (at 4.3815 0 90) (layer F.SilkS))
    (fp_text value D (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 114 +R_12V))
    (pad 2 smd rect (at 2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /R_VALVE))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 229.6672 138.062 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 -1.82) (layer F.SilkS) hide)
    (fp_text value "RPi POWER" (at -0.2794 1.8034) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_Littelfuse-NANO2-451_453 (layer B.Cu) (tedit 5DA6DC9F)
    (at 214.7828 132.855 180)
    (descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
    (tags "Fuse Nano2")
    (attr smd)
    (fp_text reference F1 (at -0.127 2.3368) (layer B.SilkS))
    (fp_text value 10A (at 0 -2.7 180 unlocked) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.455 0 180) (size 1.96 3.15) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 2.455 0 180) (size 1.96 3.15) (layers B.Cu B.Paste B.Mask)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1812_4532Metric (layer B.Cu) (tedit 5B301BBE)
    (at 215.5702 114.2876 180)
    (descr "Inductor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at 3.6576 0.2032 270) (layer B.SilkS))
    (fp_text value 742792510 (at 0 -2.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 2.1375 0 180) (size 1.125 3.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 6 "Net-(C2-Pad1)"))
    (pad 1 smd roundrect (at -2.1375 0 180) (size 1.125 3.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 24 "Net-(FB1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ulc-mm:L_WE-PBF_7.8x4.75mm (layer B.Cu) (tedit 6154BAE1)
    (at 224.3078 115.8116)
    (descr "Shielded Power Inductors (https://www.bourns.com/docs/product-datasheets/srp7028a.pdf)")
    (tags "Shielded Inductors Bourns SMD SRP7028A")
    (attr smd)
    (fp_text reference FB2 (at 0 4.2) (layer B.SilkS))
    (fp_text value 7427932 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 3.65 0) (size 3 1.47) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(FB2-Pad2)"))
    (pad 1 smd rect (at -3.65 0) (size 3 1.47) (layers B.Cu B.Paste B.Mask)
      (net 9 +5VP))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRP7028A_7.3x6.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1812_4532Metric (layer B.Cu) (tedit 5B301BBE)
    (at 230.1244 120.9678 270)
    (descr "Inductor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB3 (at -4.4196 -0.4826 270) (layer B.SilkS))
    (fp_text value 742792510 (at 0 -2.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -2.1375 0 270) (size 1.125 3.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 26 "Net-(FB3-Pad1)"))
    (pad 2 smd roundrect (at 2.1375 0 270) (size 1.125 3.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.222222)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ulc-mm:L_WE-PBF_7.8x4.75mm (layer B.Cu) (tedit 6154BAE1)
    (at 247.498 120.3836 180)
    (descr "Shielded Power Inductors (https://www.bourns.com/docs/product-datasheets/srp7028a.pdf)")
    (tags "Shielded Inductors Bourns SMD SRP7028A")
    (attr smd)
    (fp_text reference FB4 (at 0 4.2) (layer B.SilkS))
    (fp_text value 7427932 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.65 0 180) (size 3 1.47) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 3.65 0 180) (size 3 1.47) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(FB4-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRP7028A_7.3x6.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 208.2 103.4)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at -0.2032 12.6238) (layer F.SilkS))
    (fp_text value MPR_Pressure_Breakout_Conn (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SCL))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53047-0210_1x02_P1.25mm_Vertical (layer F.Cu) (tedit 5B783167)
    (at 288.4555 100.216 180)
    (descr "Molex PicoBlade Connector System, 53047-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (fp_text reference J5 (at 0.7547 2.159 180) (layer F.SilkS))
    (fp_text value LIMIT_SWITCH_1 (at 0.62 2.35) (layer F.Fab))
    (fp_text user %R (at 0.62 -1.35) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.25 0 180) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 115 R_GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 95 /R_LS1))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/530470210.stp
      (offset (xyz 0.5 0.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53047-0210_1x02_P1.25mm_Vertical (layer F.Cu) (tedit 5B783167)
    (at 294.869 100.216 180)
    (descr "Molex PicoBlade Connector System, 53047-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (fp_text reference J7 (at 0.4699 2.1844 180) (layer F.SilkS))
    (fp_text value LIMIT_SWITCH_2 (at 0.62 2.35) (layer F.Fab))
    (fp_text user %R (at 0.62 -1.35) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 101 /R_LS2))
    (pad 2 thru_hole oval (at 1.25 0 180) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 115 R_GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/530470210.stp
      (offset (xyz 0.5 0.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 300.203 100.4065 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 2.3241 2.3241) (layer F.SilkS))
    (fp_text value SERVO_CONN (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 +R_5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 R_GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Pico-EZmate_78171-0002_1x02-1MP_P1.20mm_Vertical (layer F.Cu) (tedit 5B78AD88)
    (at 304.4575 117.996 90)
    (descr "Molex Pico-EZmate series connector, 78171-0002 (http://www.molex.com/pdm_docs/sd/781710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Pico-EZmate side entry")
    (attr smd)
    (fp_text reference J9 (at -0.3175 3.81 270) (layer F.SilkS))
    (fp_text value VALVE (at 0 3.72 90) (layer F.Fab))
    (fp_text user %R (at 0 0.27 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.6 -1.875 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 +R_12V))
    (pad 2 smd roundrect (at 0.6 -1.875 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /R_VALVE))
    (pad MP smd roundrect (at -1.75 1.9 90) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad MP smd roundrect (at 1.75 1.9 90) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/2026560021.stp
      (offset (xyz 1.75 1 0.25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53398-0471_1x04-1MP_P1.25mm_Vertical (layer F.Cu) (tedit 5B78AD88)
    (at 305.1814 108.8266 90)
    (descr "Molex PicoBlade series connector, 53398-0471 (http://www.molex.com/pdm_docs/sd/533980271_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (attr smd)
    (fp_text reference J10 (at 0 4.191 90) (layer F.SilkS))
    (fp_text value STEPPER (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0.4 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.875 -1.25 90) (size 0.8 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /R_S1))
    (pad 2 smd roundrect (at -0.625 -1.25 90) (size 0.8 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /R_S2))
    (pad 3 smd roundrect (at 0.625 -1.25 90) (size 0.8 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /R_S3))
    (pad 4 smd roundrect (at 1.875 -1.25 90) (size 0.8 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /R_S4))
    (pad MP smd roundrect (at -4.425 1.5 90) (size 2.1 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.119048))
    (pad MP smd roundrect (at 4.425 1.5 90) (size 2.1 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.119048))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_PicoBlade_53398-0471_1x04-1MP_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_CLIK-Mate_502443-0570_1x05-1MP_P2.00mm_Vertical (layer F.Cu) (tedit 5B78AD89)
    (at 285.6615 112.027 270)
    (descr "Molex CLIK-Mate series connector, 502443-0570 (http://www.molex.com/pdm_docs/sd/5024430270_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex CLIK-Mate side entry")
    (attr smd)
    (fp_text reference J11 (at -8.3058 -0.5588 180) (layer F.SilkS))
    (fp_text value ENCODER (at 0 5.15 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.98 90) (layer F.Fab))
    (pad 1 smd roundrect (at -4 2.5 270) (size 1 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 +R_3V3))
    (pad 2 smd roundrect (at -2 2.5 270) (size 1 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 110 /R_SDA))
    (pad 3 smd roundrect (at 0 2.5 270) (size 1 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 /R_SCL))
    (pad 4 smd roundrect (at 2 2.5 270) (size 1 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 /R_INT))
    (pad 5 smd roundrect (at 4 2.5 270) (size 1 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 115 R_GND))
    (pad MP smd roundrect (at -6.35 -2.15 270) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889))
    (pad MP smd roundrect (at 6.35 -2.15 270) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/5024430570.stp
      (offset (xyz 0 1 6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Connector_Molex:Molex_Pico-EZmate_78171-0002_1x02-1MP_P1.20mm_Vertical (layer F.Cu) (tedit 5B78AD88)
    (at 259.55 125.75)
    (descr "Molex Pico-EZmate series connector, 78171-0002 (http://www.molex.com/pdm_docs/sd/781710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Pico-EZmate side entry")
    (attr smd)
    (fp_text reference J12 (at -3.2128 -0.8509 90) (layer F.SilkS))
    (fp_text value LED (at 0 3.72) (layer F.Fab))
    (fp_text user %R (at 0 0.27) (layer F.Fab))
    (pad 1 smd roundrect (at -0.6 -1.875) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /Vled))
    (pad 2 smd roundrect (at 0.6 -1.875) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C19-Pad2)"))
    (pad MP smd roundrect (at -1.75 1.9) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad MP smd roundrect (at 1.75 1.9) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/2026560021.stp
      (offset (xyz 1.75 1 0.4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Inductor_SMD:L_Wuerth_WE-PDF_Handsoldering (layer B.Cu) (tedit 5D8D15D5)
    (at 252.35 131.65 90)
    (descr "Shielded Power Inductor, Wuerth Elektronik, WE-PDF, SMD, Handsoldering, https://katalog.we-online.de/pbs/datasheet/7447797022.pdf")
    (tags "Choke Shielded Power Inductor WE-PDF Wuerth Handsoldering")
    (attr smd)
    (fp_text reference L2 (at 0 6.35 90) (layer B.SilkS))
    (fp_text value "11 uH" (at 0 -6.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -5.1 0 90) (size 4.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C17-Pad2)"))
    (pad 2 smd rect (at 5.1 0 90) (size 4.4 3.4) (layers B.Cu B.Paste B.Mask)
      (net 16 /Vled))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_WE-PDF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 224.1046 129.1466 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 2.2466 0.1524) (layer B.SilkS))
    (fp_text value ZVN3306F (at 0 -2.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 215.9766 126.4288 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.4384 0 270) (layer B.SilkS))
    (fp_text value ZVN3306F (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 239.751 117.615)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.286 -0.127) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 /VALVE_GPIO))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 239.624 115.837 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.286 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 /VALVE_GPIO))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 266.04 104.788 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.2606 0.0254 270) (layer B.SilkS))
    (fp_text value 499 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 +3.3VP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 264.804 113.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.125 -0.04 270) (layer F.SilkS))
    (fp_text value 4.02k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /DRV_Vref))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 213.3604 122.822 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0.127 -1.6764 90) (layer B.SilkS))
    (fp_text value 10.2k (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 /PGood_Pi_3V3))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 67 /PGood_Pi_5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 217.5 122.8 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.794 -0.0254 270) (layer B.SilkS))
    (fp_text value 19.6k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 /PGood_Pi_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 257.3405 115.964 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.248 1.2435) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 262.738 102.756)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0.0254 -1.2954) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 +3.3VP))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 48 /DRV_FAULT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 229.1084 125.7176 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 10.2k (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 /PGood_LED_5V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 /PGood_LED_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 231.5214 128.5116)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.8194 -0.0254) (layer B.SilkS))
    (fp_text value 19.6k (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 /PGood_LED_3V3))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 244.748 111.361 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0.1595 1.5435 270) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 /FAN_GPIO))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 245.248 108.761)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.3) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 /FAN_GPIO))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 263.3476 138.4938 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -0.25 -1.5) (layer F.SilkS))
    (fp_text value 910 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C18-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 227.1 129.2 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -2.8194 0.0254 90) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 /PGood_LED_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 228.95 129.0196 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 2.5654 -0.0254 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 /PGood_LED_3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 260.65 131.55 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -0.15 -1.5 270) (layer F.SilkS))
    (fp_text value 400m (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C19-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 215.4 122.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 3.2004 0.0762 90) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(Q4-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 /PGood_Pi_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 213.208 126.1748 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -0.127 1.397 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 /PGood_Pi_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3266W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 268.834 103.518 270)
    (descr "Potentiometer, vertical, Bourns 3266W, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266W")
    (fp_text reference RV1 (at -2.286 4.3942 270) (layer F.SilkS))
    (fp_text value 10k (at -2.54 4.73 90) (layer F.Fab))
    (fp_text user %R (at -3.175 1.23 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(R3-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /DRV_Vref))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /DRV_Vref))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile (layer F.Cu) (tedit 5A4E1404)
    (at 247.244 109.9315 90)
    (descr "SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile")
    (tags "SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile")
    (attr smd)
    (fp_text reference SW2 (at 6.5786 -0.0508 180) (layer F.SilkS))
    (fp_text value "DIP SWITCH" (at 0 5.65 90) (layer F.Fab))
    (fp_text user %R (at 2.58 0) (layer F.Fab))
    (fp_text user on (at 0.4275 -3.8825 90) (layer F.Fab))
    (pad 1 smd rect (at -4.305 -2.54 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (pad 4 smd rect (at 4.305 2.54 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(SW2-Pad4)"))
    (pad 2 smd rect (at -4.305 0 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (pad 5 smd rect (at 4.305 0 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(SW2-Pad5)"))
    (pad 3 smd rect (at -4.305 2.54 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP))
    (pad 6 smd rect (at 4.305 -2.54 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(SW2-Pad6)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 210.1854 146.1138 90)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP1 (at -2.794 0) (layer F.SilkS) hide)
    (fp_text value 12V (at -2.7686 0.0254 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 +12V))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 268.834 111.138 90)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP6 (at -5.08 -0.508 90) (layer F.SilkS))
    (fp_text value DRV_VREF (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 65 /DRV_Vref))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 203.45 109.5 90)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP4 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value SDA (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 37 /SDA))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 214.5542 146.1392 180)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP2 (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value 5V (at 0.0254 -2.6924) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 203.45 104.65 90)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP5 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value SCL (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 36 /SCL))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 251.0794 145.7328 270)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP7 (at 0.1016 -2.5654 270) (layer F.SilkS))
    (fp_text value VLED (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 16 /Vled))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 218.9484 146.19 180)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP3 (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value 3.3V (at 0.0508 -2.667) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 223.2664 146.0884 180)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP8 (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -2.7686) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 216.8656 106.566)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 6.1) (layer B.SilkS))
    (fp_text value DS3231M (at 0 -6.1) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -4.65 4.445) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -4.65 3.175) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 3 smd roundrect (at -4.65 1.905) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at -4.65 0.635) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U1-Pad4)"))
    (pad 5 smd roundrect (at -4.65 -0.635) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 6 smd roundrect (at -4.65 -1.905) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 7 smd roundrect (at -4.65 -3.175) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 8 smd roundrect (at -4.65 -4.445) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 9 smd roundrect (at 4.65 -4.445) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 10 smd roundrect (at 4.65 -3.175) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 11 smd roundrect (at 4.65 -1.905) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 12 smd roundrect (at 4.65 -0.635) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 13 smd roundrect (at 4.65 0.635) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 14 smd roundrect (at 4.65 1.905) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(BT1-Pad1)"))
    (pad 15 smd roundrect (at 4.65 3.175) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 /SDA))
    (pad 16 smd roundrect (at 4.65 4.445) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 /SCL))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_RECOM_RPMx.x-x.0 (layer F.Cu) (tedit 5C6321BD)
    (at 220.5232 122.822)
    (descr https://www.recom-power.com/pdf/Innoline/RPM-6.0.pdf)
    (tags "dc-dc recom buck lga-25 pitch 2.29mm")
    (attr smd)
    (fp_text reference U2 (at 0.0254 -7.0104) (layer F.SilkS))
    (fp_text value RPM5.0-6.0 (at 0 8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad A1 smd rect (at -4.58 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(FB1-Pad1)"))
    (pad B1 smd rect (at -4.58 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C1 smd rect (at -4.58 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U2-PadC1)"))
    (pad D1 smd rect (at -4.58 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 67 /PGood_Pi_5V))
    (pad E1 smd rect (at -4.58 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U2-PadE1)"))
    (pad A2 smd rect (at -2.29 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(FB1-Pad1)"))
    (pad B2 smd rect (at -2.29 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C2 smd rect (at -2.29 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D2 smd rect (at -2.29 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E2 smd rect (at -2.29 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U2-PadE2)"))
    (pad A3 smd rect (at 0 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad B3 smd rect (at 0 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C3 smd rect (at 0 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D3 smd rect (at 0 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E3 smd rect (at 0 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A4 smd rect (at 2.29 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad B4 smd rect (at 2.29 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C4 smd rect (at 2.29 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D4 smd rect (at 2.29 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E4 smd rect (at 2.29 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A5 smd rect (at 4.58 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(FB2-Pad2)"))
    (pad B5 smd rect (at 4.58 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(FB2-Pad2)"))
    (pad C5 smd rect (at 4.58 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(FB2-Pad2)"))
    (pad D5 smd rect (at 4.58 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E5 smd rect (at 4.58 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U2-PadE5)"))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/RPM5.0-6.0--3DModel-STEP-363165.STEP
      (offset (xyz -6.5 -6 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_RECOM_RPMx.x-x.0 (layer F.Cu) (tedit 5C6321BD)
    (at 236.3474 122.8728)
    (descr https://www.recom-power.com/pdf/Innoline/RPM-6.0.pdf)
    (tags "dc-dc recom buck lga-25 pitch 2.29mm")
    (attr smd)
    (fp_text reference U4 (at -0.2474 -6.8728) (layer F.SilkS))
    (fp_text value RPM5.0-6.0 (at 0 8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad E5 smd rect (at 4.58 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U4-PadE5)"))
    (pad D5 smd rect (at 4.58 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C5 smd rect (at 4.58 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(FB4-Pad2)"))
    (pad B5 smd rect (at 4.58 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(FB4-Pad2)"))
    (pad A5 smd rect (at 4.58 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(FB4-Pad2)"))
    (pad E4 smd rect (at 2.29 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D4 smd rect (at 2.29 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C4 smd rect (at 2.29 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad B4 smd rect (at 2.29 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A4 smd rect (at 2.29 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E3 smd rect (at 0 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D3 smd rect (at 0 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C3 smd rect (at 0 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad B3 smd rect (at 0 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A3 smd rect (at 0 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad E2 smd rect (at -2.29 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U4-PadE2)"))
    (pad D2 smd rect (at -2.29 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C2 smd rect (at -2.29 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad B2 smd rect (at -2.29 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A2 smd rect (at -2.29 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(FB3-Pad1)"))
    (pad E1 smd rect (at -4.58 4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U4-PadE1)"))
    (pad D1 smd rect (at -4.58 2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 70 /PGood_LED_5V))
    (pad C1 smd rect (at -4.58 0) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 58 /PWR_GPIO))
    (pad B1 smd rect (at -4.58 -2.29) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A1 smd rect (at -4.58 -4.58) (size 1.06 1.06) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(FB3-Pad1)"))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/RPM5.0-6.0--3DModel-STEP-363165.STEP
      (offset (xyz -6.5 -6 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP1.05x1.75mm (layer F.Cu) (tedit 5EA4BCEE)
    (at 216.7 107.8 90)
    (descr "DFN8 2x2, 0.5P; CASE 506CN (see ON Semiconductor 506CN.PDF)")
    (tags "DFN 0.5")
    (clearance 0.1)
    (attr smd)
    (fp_text reference U5 (at -1.9808 0.1 180) (layer F.SilkS))
    (fp_text value SHT3x (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -0.75 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /SDA))
    (pad 2 smd rect (at -0.9 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -0.9 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U5-Pad3)"))
    (pad 4 smd rect (at -0.9 0.75 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /SCL))
    (pad 5 smd rect (at 0.9 0.75 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 6 smd rect (at 0.9 0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U5-Pad6)"))
    (pad 7 smd rect (at 0.9 -0.25 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 0.9 -0.75 90) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd rect (at 0 0 90) (size 1.05 1.75) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad "" smd rect (at 0 0.4375 90) (size 0.85 0.65) (layers F.Paste))
    (pad "" smd rect (at 0 -0.4375 90) (size 0.85 0.65) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_P0.5mm_EP1.05x1.75mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 258.05 137)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U6 (at 0 -2.4) (layer F.SilkS))
    (fp_text value TPS54200DDCT (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C17-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C18-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R24-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer B.Cu) (tedit 5A02FF57)
    (at 236.449 116.98 270)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q1 (at 2.45 -0.4) (layer B.SilkS))
    (fp_text value BSS214NWH6327XTSA1 (at -0.05 -2.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.45 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1 -0.65) (size 0.45 0.7) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -1 0.65) (size 0.45 0.7) (layers B.Cu B.Paste B.Mask)
      (net 21 /VALVE))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer B.Cu) (tedit 5A02FF57)
    (at 242.291 111.392 270)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q2 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value BSS214NWH6327XTSA1 (at -0.05 -2.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.65) (size 0.45 0.7) (layers B.Cu B.Paste B.Mask)
      (net 38 /FAN))
    (pad 2 smd rect (at -1 -0.65) (size 0.45 0.7) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.45 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 277.0954 100.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK5 (at -0.0508 3.81) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 277.0954 118.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK6 (at 0 -3.7) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 321.0954 100.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK7 (at 0 3.81) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 321.0954 118.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK8 (at 0 -3.7) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x08_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 230.7975 107.709 180)
    (descr "surface-mounted straight pin header, 2x08, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x08 1.27mm double row")
    (attr smd)
    (fp_text reference J1 (at -1.2065 -6.14) (layer F.SilkS))
    (fp_text value "REMOTE CONNECTOR" (at 0 6.14) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 1.95 4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 15 smd rect (at -1.95 4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 28 /LS1))
    (pad 14 smd rect (at 1.95 3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 118 +3.3VA))
    (pad 13 smd rect (at -1.95 3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 29 /LS2))
    (pad 12 smd rect (at 1.95 1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 37 /SDA))
    (pad 11 smd rect (at -1.95 1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 30 /SERVO_PWM))
    (pad 10 smd rect (at 1.95 0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd rect (at -1.95 0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1.95 -0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 36 /SCL))
    (pad 7 smd rect (at -1.95 -0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 31 /S4))
    (pad 6 smd rect (at 1.95 -1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 21 /VALVE))
    (pad 5 smd rect (at -1.95 -1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 32 /S3))
    (pad 4 smd rect (at 1.95 -3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 108 /INT))
    (pad 3 smd rect (at -1.95 -3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 33 /S2))
    (pad 2 smd rect (at 1.95 -4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (pad 1 smd rect (at -1.95 -4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 34 /S1))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x08_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_PicoBlade_53047-0210_1x02_P1.25mm_Vertical (layer F.Cu) (tedit 5B783167)
    (at 239.6875 108.0265 270)
    (descr "Molex PicoBlade Connector System, 53047-0210, 2 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (fp_text reference J3 (at 4.0005 1.3335 90) (layer F.SilkS))
    (fp_text value FAN (at 0.62 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0.62 -1.35 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 +12V))
    (pad 2 thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 /FAN))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/530470210.stp
      (offset (xyz 0.5 0.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x08_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 296.0755 110.0585 180)
    (descr "surface-mounted straight pin header, 2x08, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x08 1.27mm double row")
    (attr smd)
    (fp_text reference J6 (at 0.127 6.2865) (layer F.SilkS))
    (fp_text value "SHIELD CONNECTOR" (at 0 6.14) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 96 /R_S1))
    (pad 2 smd rect (at 1.95 -4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 114 +R_12V))
    (pad 3 smd rect (at -1.95 -3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 97 /R_S2))
    (pad 4 smd rect (at 1.95 -3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 111 /R_INT))
    (pad 5 smd rect (at -1.95 -1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 99 /R_S3))
    (pad 6 smd rect (at 1.95 -1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 94 /R_VALVE))
    (pad 7 smd rect (at -1.95 -0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 98 /R_S4))
    (pad 8 smd rect (at 1.95 -0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 109 /R_SCL))
    (pad 9 smd rect (at -1.95 0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 115 R_GND))
    (pad 10 smd rect (at 1.95 0.635 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 115 R_GND))
    (pad 11 smd rect (at -1.95 1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 100 /R_SERVO_PWM))
    (pad 12 smd rect (at 1.95 1.905 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 110 /R_SDA))
    (pad 13 smd rect (at -1.95 3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 101 /R_LS2))
    (pad 14 smd rect (at 1.95 3.175 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 116 +R_3V3))
    (pad 15 smd rect (at -1.95 4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 95 /R_LS1))
    (pad 16 smd rect (at 1.95 4.445 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 117 +R_5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x08_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 261.9125 115.9005)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 1.397 -180) (layer B.SilkS))
    (fp_text value 10 (at 0 -1.43 -180) (layer B.Fab))
    (fp_text user %R (at 0 0 -180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TSSOP-28-1EP_W4.40mm (layer F.Cu) (tedit 5D28ACA9)
    (at 259.494 108.48)
    (descr http://www.ti.com/lit/ds/symlink/tlc5940.pdf)
    (attr smd)
    (fp_text reference U3 (at 0.2 -5.37) (layer F.SilkS))
    (fp_text value DRV8825 (at 0.06 5.64) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 29 smd rect (at 0 -1.45) (size 6.17 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin -0.25))
    (pad 29 smd rect (at 0 1.45) (size 6.17 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin -0.25))
    (pad 29 smd rect (at -3.9225 0) (size 1.675 3.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin -0.8375))
    (pad 1 smd rect (at -4.225 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -3.575 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C11-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -2.925 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)") (solder_mask_margin 0.07))
    (pad 4 smd rect (at -2.275 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V) (solder_mask_margin 0.07))
    (pad 5 smd rect (at -1.625 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /S1) (solder_mask_margin 0.07))
    (pad 6 smd rect (at -0.975 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R7-Pad2)") (solder_mask_margin 0.07))
    (pad 7 smd rect (at -0.325 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /S2) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 0.325 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /S4) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 0.975 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R8-Pad2)") (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.625 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /S3) (solder_mask_margin 0.07))
    (pad 11 smd rect (at 2.275 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V) (solder_mask_margin 0.07))
    (pad 12 smd rect (at 2.925 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 /DRV_Vref) (solder_mask_margin 0.07))
    (pad 13 smd rect (at 3.575 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 /DRV_Vref) (solder_mask_margin 0.07))
    (pad 14 smd rect (at 4.225 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 15 smd rect (at 4.225 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +3.3VP) (solder_mask_margin 0.07))
    (pad 16 smd rect (at 3.575 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /DRV_RESET) (solder_mask_margin 0.07))
    (pad 17 smd rect (at 2.925 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /DRV_SLEEP) (solder_mask_margin 0.07))
    (pad 18 smd rect (at 2.275 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /DRV_FAULT) (solder_mask_margin 0.07))
    (pad 19 smd rect (at 1.625 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U3-Pad19)") (solder_mask_margin 0.07))
    (pad 20 smd rect (at 0.975 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /DIR) (solder_mask_margin 0.07))
    (pad 21 smd rect (at 0.325 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 105 /DRV_EN) (solder_mask_margin 0.07))
    (pad 22 smd rect (at -0.325 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(R23-Pad1)") (solder_mask_margin 0.07))
    (pad 23 smd rect (at -0.975 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U3-Pad23)") (solder_mask_margin 0.07))
    (pad 24 smd rect (at -1.625 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(SW2-Pad6)") (solder_mask_margin 0.07))
    (pad 25 smd rect (at -2.275 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(SW2-Pad5)") (solder_mask_margin 0.07))
    (pad 26 smd rect (at -2.925 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(SW2-Pad4)") (solder_mask_margin 0.07))
    (pad 27 smd rect (at -3.575 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U3-Pad27)") (solder_mask_margin 0.07))
    (pad 28 smd rect (at -4.225 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.07))
    (pad 29 smd rect (at 0 0) (size 6.17 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0001))
    (pad 29 smd rect (at 3.9225 0) (size 1.675 3.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin -0.8375))
    (pad 29 thru_hole circle (at 0 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0001))
    (pad 29 thru_hole circle (at 1.3 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0001))
    (pad 29 thru_hole circle (at 2.6 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0001))
    (pad 29 thru_hole circle (at -1.3 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0001))
    (pad 29 thru_hole circle (at -2.6 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0001))
    (pad 29 thru_hole circle (at -3.9 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at -2.6 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at -1.3 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 0 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 1.3 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 2.6 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 3.9 -1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at -3.9 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at -3.9 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at -2.6 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at -1.3 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 0 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 1.3 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 2.6 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 3.9 1.3) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (pad 29 thru_hole circle (at 3.9 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin -0.15))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 255.91 116.49 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.22 -0.02) (layer F.SilkS))
    (fp_text value "4.7 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 253.34 110.86368 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -2.6289 -0.0508 90) (layer F.SilkS))
    (fp_text value "0.01 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 225.1968 135.776 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /LED_IND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 225.2984 138.6716)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -0.0508 1.4732) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 225.273 141.5418)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -0.0255 1.4986) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 252.2732 102.1972 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 1.3462) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(R23-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /STEP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 264.6684 136.7158)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at -0.5842 -1.2192) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /LED_PWM))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(R24-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 301.1428 105.042 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 "Net-(J8-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /R_SERVO_PWM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 253.64 113.93 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0.32 -1.2 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +12V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 255.93 113.38)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 2.57 0.17) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 72.0344 (width 0.12) (layer Dwgs.User)
    (gr_text "72.034 mm" (at 235.9918 87.512) (layer Dwgs.User))
    (feature1 (pts (xy 272.009 97.1426) (xy 272.009 87.945579)))
    (feature2 (pts (xy 199.9746 97.1426) (xy 199.9746 87.945579)))
    (crossbar (pts (xy 199.9746 88.532) (xy 272.009 88.532)))
    (arrow1a (pts (xy 272.009 88.532) (xy 270.882496 89.118421)))
    (arrow1b (pts (xy 272.009 88.532) (xy 270.882496 87.945579)))
    (arrow2a (pts (xy 199.9746 88.532) (xy 201.101104 89.118421)))
    (arrow2b (pts (xy 199.9746 88.532) (xy 201.101104 87.945579)))
  )
  (dimension 25 (width 0.12) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 328.4732 109.4838 270) (layer Dwgs.User))
    (feature1 (pts (xy 321.57 121.9838) (xy 327.789621 121.9838)))
    (feature2 (pts (xy 321.57 96.9838) (xy 327.789621 96.9838)))
    (crossbar (pts (xy 327.2032 96.9838) (xy 327.2032 121.9838)))
    (arrow1a (pts (xy 327.2032 121.9838) (xy 326.616779 120.857296)))
    (arrow1b (pts (xy 327.2032 121.9838) (xy 327.789621 120.857296)))
    (arrow2a (pts (xy 327.2032 96.9838) (xy 326.616779 98.110304)))
    (arrow2b (pts (xy 327.2032 96.9838) (xy 327.789621 98.110304)))
  )
  (dimension 51 (width 0.12) (layer Dwgs.User)
    (gr_text "51.000 mm" (at 299.0954 93.1548) (layer Dwgs.User))
    (feature1 (pts (xy 324.5954 100) (xy 324.5954 93.838379)))
    (feature2 (pts (xy 273.5954 100) (xy 273.5954 93.838379)))
    (crossbar (pts (xy 273.5954 94.4248) (xy 324.5954 94.4248)))
    (arrow1a (pts (xy 324.5954 94.4248) (xy 323.468896 95.011221)))
    (arrow1b (pts (xy 324.5954 94.4248) (xy 323.468896 93.838379)))
    (arrow2a (pts (xy 273.5954 94.4248) (xy 274.721904 95.011221)))
    (arrow2b (pts (xy 273.5954 94.4248) (xy 274.721904 93.838379)))
  )
  (gr_circle (center 271.8846 111.8676) (end 272.1386 111.8676) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 271.8846 110.8676) (end 272.1386 110.8676) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 271.8846 109.8676) (end 272.1386 109.8676) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 272.7874 108.8852) (end 273.5748 108.8852) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 272 113) (end 272 147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 272 97) (end 272 108.8852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 273.5748 113) (end 273.5748 119) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 273.5748 108.8852) (end 273.5748 100) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 272.7874 113) (end 272 113) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_text "Bioengineering Platform\nChan Zuckerberg Biohub\nLabel Free Malaria Scope\n5-0006 Remote Board\nEmily Huynh\n12/2021 - pcb - V1" (at 314.173 113.5764 90) (layer F.SilkS))
  (gr_text "Bioengineering Platform\nChan Zuckerberg Biohub\nLabel Free Malaria Scope\n5-0005 RPi 4B Hat\nEmily Huynh\n12/2021 - pcb - V1" (at 234.0106 146.698) (layer F.SilkS))
  (gr_arc (start 321.5748 119) (end 324.5748 119) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 321.5748 100) (end 321.5748 97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 324.5748 100) (end 324.5748 119) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 276.5748 122) (end 321.5748 122) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 276.5748 119) (end 276.5748 122) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 276.5748 100) (end 273.5748 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 276.5748 97) (end 321.5748 97) (layer Edge.Cuts) (width 0.1))
  (dimension 56 (width 0.12) (layer Dwgs.User)
    (gr_text "56.000 mm" (at 193.6091 122 270) (layer Dwgs.User))
    (feature1 (pts (xy 203.0861 150) (xy 194.292679 150)))
    (feature2 (pts (xy 203.0861 94) (xy 194.292679 94)))
    (crossbar (pts (xy 194.8791 94) (xy 194.8791 150)))
    (arrow1a (pts (xy 194.8791 150) (xy 194.292679 148.873496)))
    (arrow1b (pts (xy 194.8791 150) (xy 195.465521 148.873496)))
    (arrow2a (pts (xy 194.8791 94) (xy 194.292679 95.126504)))
    (arrow2b (pts (xy 194.8791 94) (xy 195.465521 95.126504)))
  )
  (gr_text USB (at 278.232 102.248) (layer Dwgs.User))
  (gr_arc (start 269 97) (end 269 94) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244 146) (end 244 131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 246 131) (end 246 146) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 245 131) (end 244 131) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 245 146) (end 246 146) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 200.5 131) (end 200 131) (angle 89.9) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 204.5 130) (end 205 130) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 200.5 113) (end 200.5 113.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 204.5 114) (end 204.5 113.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 97) (end 200 113) (layer Edge.Cuts) (width 0.1))
  (gr_text DISPLAY (at 202.5 122 90) (layer Dwgs.User))
  (gr_text RJ45 (at 276.2 139.84) (layer Dwgs.User))
  (gr_text USB (at 277.724 121.552) (layer Dwgs.User))
  (gr_arc (start 269 147) (end 272 147) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 203 147) (end 203 150) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 203 97) (end 200 97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 269 94) (end 203 94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.5 130.5) (end 200.5 130.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 205 114) (end 205 130) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.5 113.5) (end 204.5 113.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 203 150) (end 269 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 131) (end 200 147) (layer Edge.Cuts) (width 0.1))
  (gr_text "RASPBERRY-PI 40-PIN ADDON BOARD\nVIEW FROM TOP\nNOTE: P1 SHOULD BE FITTED ON THE REVERSE OF THE BOARD\n\nADD EDGE CUTS FROM CAMERA AND DISPLAY PORTS AS REQUIRED" (at 201.1684 165.1892) (layer Dwgs.User))
  (zone (net 3) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 272.136 150.5588) (xy 199.746 150.4064) (xy 199.8476 93.612) (xy 272.2884 93.6882)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 239.5605 124.219) (xy 241.9354 124.219) (xy 241.9354 126.1494) (xy 239.5859 126.1494) (xy 239.5859 128.3465)
        (xy 235.3949 128.3465) (xy 235.3949 126.0478) (xy 233.1343 126.0605) (xy 233.1216 121.552) (xy 230.8483 121.552)
        (xy 230.8483 119.6216) (xy 235.4584 119.6216) (xy 235.4584 117.3737) (xy 239.5605 117.3737)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.7617 124.2444) (xy 226.1366 124.2444) (xy 226.1366 126.1748) (xy 223.7871 126.1748) (xy 223.7871 128.3719)
        (xy 219.5961 128.3719) (xy 219.5961 126.0732) (xy 217.3355 126.0859) (xy 217.3228 121.5774) (xy 215.0495 121.5774)
        (xy 215.0495 119.647) (xy 219.6596 119.647) (xy 219.6596 117.3991) (xy 223.7617 117.3991)
      )
    )
  )
  (zone (net 26) (net_name "Net-(FB3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.6583 118.8469) (xy 230.1117 118.8469) (xy 230.1117 116.6371) (xy 234.6583 116.6371)
      )
    )
  )
  (zone (net 24) (net_name "Net-(FB1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 218.8341 118.7961) (xy 214.2875 118.7961) (xy 214.2875 116.5863) (xy 218.8341 116.5863)
      )
    )
  )
  (zone (net 27) (net_name "Net-(FB4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 242.61125 123.6) (xy 240.207725 123.58145) (xy 240.192275 116.61855) (xy 242.5704 116.6371)
      )
    )
  )
  (zone (net 25) (net_name "Net-(FB2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.81125 123.6) (xy 224.410187 123.611775) (xy 224.389813 116.588226) (xy 226.765476 116.576451)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 257.4 142.75) (xy 250.5 142.75) (xy 250.45 138.8) (xy 254.95 138.8) (xy 255.95 137.8)
        (xy 257.45 137.8)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 261.55 134.8) (xy 258.35 134.85) (xy 258.3762 139.1029) (xy 262.4262 139.1039) (xy 262.4 142.8)
        (xy 257.925 142.8) (xy 257.875 136.4) (xy 255.95 136.4) (xy 255.9375 132.22) (xy 261.5375 132.22)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C17-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.775 136.7) (xy 257.35 136.7) (xy 257.35 137.3) (xy 255.5 137.3) (xy 254.7 138)
        (xy 250.45 138) (xy 250.45 136.1) (xy 255.025 136.1)
      )
    )
  )
  (zone (net 17) (net_name "Net-(C19-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 262.75 131.3) (xy 258.05 131.25) (xy 258.05 128.8) (xy 262.75 128.8)
      )
    )
  )
  (zone (net 16) (net_name /Vled) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 256.833858 131.3945) (xy 250.583858 131.3945) (xy 250.583858 123.801219) (xy 256.833858 123.851219)
      )
    )
  )
  (zone (net 5) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 257.404 112.0905) (xy 257.4294 113.1954) (xy 257.404 118.185875) (xy 261.49725 118.187125) (xy 262.23 113.424)
        (xy 261.6585 112.2175) (xy 261.6585 110.68) (xy 261.994 110.68) (xy 261.976 112.281) (xy 262.738 113.2335)
        (xy 262.738 117.9325) (xy 265.0875 117.9325) (xy 265.0875 119.74225) (xy 256.515 119.7105) (xy 256.515 116.1545)
        (xy 256.9468 112.8652) (xy 257.023 112.281) (xy 257.044 110.63) (xy 257.404 110.63)
      )
    )
  )
  (zone (net 7) (net_name +3.3VP) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 268.58 106.312) (xy 263.519 106.38) (xy 263.519 104.88) (xy 268.58 104.8)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 261.2775 115.76) (xy 257.7115 115.76) (xy 257.7265 117.742) (xy 261.2725 117.742)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.626 106.312) (xy 253.975 106.312) (xy 253.975 107.074) (xy 263.627 107.074) (xy 263.627 106.82)
        (xy 266.675 106.82) (xy 266.675 122.441) (xy 253.213 122.441) (xy 253.213 119.266) (xy 250.419 119.266)
        (xy 250.419 103.391) (xy 255.626 103.391)
      )
    )
    (polygon
      (pts
        (xy 253.975 110.122) (xy 253.975 112.408) (xy 252.197 112.408) (xy 252.197 115.456) (xy 254.356 115.456)
        (xy 254.356 119.9645) (xy 265.405 119.9645) (xy 265.405 112.408) (xy 263.627 112.408) (xy 263.627 110.122)
      )
    )
  )
  (zone (net 115) (net_name R_GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 324.8283 122.3775) (xy 272.945625 122.482275) (xy 272.850375 96.694925) (xy 324.98705 96.64095)
      )
    )
  )
)
