(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 66)
    (zones 0)
    (modules 3)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /FOOT_DOWN_A)
  (net 3 /HEAD_DOWN_A)
  (net 4 /HEAD_UP_A)
  (net 5 /FOOT_UP_A)
  (net 6 /FOOT_POSITION_A)
  (net 7 /HEAD_POSITION_A)
  (net 8 /FOOT_DOWN_B)
  (net 9 /HEAD_DOWN_B)
  (net 10 /HEAD_UP_B)
  (net 11 /FOOT_UP_B)
  (net 12 /FOOT_POSITION_B)
  (net 13 /HEAD_POSITION_B)
  (net 14 "Net-(J1-Pad8)")
  (net 15 "Net-(J2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /FOOT_DOWN_A)
    (add_net /FOOT_DOWN_B)
    (add_net /FOOT_POSITION_A)
    (add_net /FOOT_POSITION_B)
    (add_net /FOOT_UP_A)
    (add_net /FOOT_UP_B)
    (add_net /HEAD_DOWN_A)
    (add_net /HEAD_DOWN_B)
    (add_net /HEAD_POSITION_A)
    (add_net /HEAD_POSITION_B)
    (add_net /HEAD_UP_A)
    (add_net /HEAD_UP_B)
    (add_net GND)
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad8)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 131 79.8)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J3 (at 5.5 -1) (layer F.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at -1.2 52) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 90) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HEAD_DOWN_B))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /FOOT_DOWN_B))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HEAD_UP_B))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /FOOT_POSITION_B))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HEAD_POSITION_B))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /FOOT_UP_B))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /HEAD_DOWN_A))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /FOOT_DOWN_A))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HEAD_UP_A))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /FOOT_POSITION_A))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HEAD_POSITION_A))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /FOOT_UP_A))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:RJ45_Amphenol_RJHSE5080 (layer F.Cu) (tedit 5F30B693)
    (at 149.9 116.3 90)
    (fp_text reference J2 (at -9.2 3.7 180) (layer F.SilkS))
    (fp_text value RJ45 (at 0 -11 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6.35 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.555 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (pad 7 thru_hole circle (at -2.565 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -1.545 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 /FOOT_DOWN_B))
    (pad 5 thru_hole circle (at -0.525 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 /HEAD_DOWN_B))
    (pad 4 thru_hole circle (at 0.495 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 10 /HEAD_UP_B))
    (pad 3 thru_hole circle (at 1.515 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 11 /FOOT_UP_B))
    (pad 2 thru_hole circle (at 2.535 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 12 /FOOT_POSITION_B))
    (pad 1 thru_hole circle (at 3.555 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 13 /HEAD_POSITION_B))
  )
  (module local_footprints:RJ45_Amphenol_RJHSE5080 (layer F.Cu) (tedit 5F30B693)
    (at 149.9 91.5 90)
    (fp_text reference J1 (at -9.3 3.7 180) (layer F.SilkS))
    (fp_text value RJ45 (at 0 -11 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6.35 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.555 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at -2.565 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -1.545 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 /FOOT_DOWN_A))
    (pad 5 thru_hole circle (at -0.525 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 /HEAD_DOWN_A))
    (pad 4 thru_hole circle (at 0.495 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 /HEAD_UP_A))
    (pad 3 thru_hole circle (at 1.515 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 /FOOT_UP_A))
    (pad 2 thru_hole circle (at 2.535 -4.32 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 /FOOT_POSITION_A))
    (pad 1 thru_hole circle (at 3.555 -2.54 90) (size 1.6 1.6) (drill 0.89) (layers *.Cu *.Mask)
      (net 7 /HEAD_POSITION_A))
  )
  (gr_text "Populate J3 on Backside" (at 136.5 103.8 90) (layer F.SilkS))
  (gr_text FOOT (at 147.2 106.9) (layer F.SilkS))
  (gr_text HEAD (at 147 82) (layer F.SilkS))
  (gr_line (start 128.5 130.5) (end 128.5 77.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155 130.5) (end 128.5 130.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155 77.3) (end 155 130.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.5 77.3) (end 155 77.3) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155 130.5) (xy 128.5 130.5) (xy 128.5 77.3) (xy 155 77.3)
      )
    )
  )
)
