<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="63.5" y2="0" width="0" layer="20"/>
<hole x="2.54" y="2.54" drill="2"/>
<hole x="63.5" y="2.54" drill="2"/>
<hole x="63.5" y="34.925" drill="2"/>
<hole x="2.54" y="34.925" drill="2"/>
<wire x1="66.04" y1="2.54" x2="66.04" y2="35.56" width="0" layer="20"/>
<wire x1="0" y1="35.56" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0" layer="20" curve="-90"/>
<wire x1="66.04" y1="2.54" x2="63.5" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="38.1" x2="63.5" y2="38.1" width="0" layer="20"/>
<wire x1="63.5" y1="38.1" x2="66.04" y2="35.56" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="35.56" x2="2.54" y2="38.1" width="0" layer="20" curve="-90"/>
<text>aka.farm
lilygo-surf v0</text>
<text>3v3</text>
<text>GND</text>
<text>0</text>
<text>12</text>
<text>27</text>
<text>26</text>
<text>3v3</text>
<text>3v3</text>
<text>25</text>
<text>33</text>
<text>32</text>
<text>34</text>
<text>RST</text>
<text>VP</text>
<text>GND</text>
<text>SDA</text>
<text>TXD</text>
<text>RXD</text>
<text>SCL</text>
<text>19</text>
<text>14</text>
<text>2</text>
<text>13</text>
<text>15</text>
<text>5v</text>
<text>VBAT</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X13_LOCK">
<description>&lt;h3&gt;Plated Through Hole -13 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X04_1MM_RA" value="Qwiic Right Angle">
<attribute name="PROD_ID" value="CONN-13729"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_1MM_RA" value="Qwiic Right Angle">
<attribute name="PROD_ID" value="CONN-13729"/>
</element>
<element name="FUCKTHIS" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCHSIDE" library="SparkFun-Connectors" package="1X13_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCHSIDE1" library="SparkFun-Connectors" package="1X13_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USBSIDE" library="SparkFun-Connectors" package="1X13_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="USBSIDE1" library="SparkFun-Connectors" package="1X13_LOCK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="PIN_0">
<contactref element="USBSIDE1" pad="12"/>
<contactref element="USBSIDE" pad="12"/>
</signal>
<signal name="VP">
<contactref element="USBSIDE1" pad="1"/>
<contactref element="USBSIDE" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="USBSIDE1" pad="2"/>
<contactref element="USBSIDE" pad="2"/>
</signal>
<signal name="RST">
<contactref element="USBSIDE1" pad="3"/>
<contactref element="USBSIDE" pad="3"/>
</signal>
<signal name="PIN_34">
<contactref element="USBSIDE1" pad="4"/>
<contactref element="USBSIDE" pad="4"/>
</signal>
<signal name="PIN_32">
<contactref element="USBSIDE1" pad="6"/>
<contactref element="USBSIDE" pad="6"/>
</signal>
<signal name="PIN_33">
<contactref element="USBSIDE1" pad="7"/>
<contactref element="USBSIDE" pad="7"/>
</signal>
<signal name="PIN_25">
<contactref element="USBSIDE1" pad="8"/>
<contactref element="USBSIDE" pad="8"/>
</signal>
<signal name="PIN_26">
<contactref element="USBSIDE1" pad="9"/>
<contactref element="USBSIDE" pad="9"/>
</signal>
<signal name="PIN_27">
<contactref element="USBSIDE1" pad="10"/>
<contactref element="USBSIDE" pad="10"/>
</signal>
<signal name="TXD">
<contactref element="SWITCHSIDE" pad="4"/>
<contactref element="SWITCHSIDE1" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="SWITCHSIDE" pad="5"/>
<contactref element="SWITCHSIDE1" pad="5"/>
</signal>
<signal name="PIN_19">
<contactref element="SWITCHSIDE" pad="7"/>
<contactref element="SWITCHSIDE1" pad="7"/>
</signal>
<signal name="PIN_14">
<contactref element="SWITCHSIDE" pad="8"/>
<contactref element="SWITCHSIDE1" pad="8"/>
</signal>
<signal name="PIN_02">
<contactref element="SWITCHSIDE" pad="9"/>
<contactref element="SWITCHSIDE1" pad="9"/>
</signal>
<signal name="PIN_15">
<contactref element="SWITCHSIDE" pad="10"/>
<contactref element="SWITCHSIDE1" pad="10"/>
</signal>
<signal name="PIN_13">
<contactref element="SWITCHSIDE" pad="11"/>
<contactref element="SWITCHSIDE1" pad="11"/>
</signal>
<signal name="5V">
<contactref element="SWITCHSIDE" pad="12"/>
<contactref element="SWITCHSIDE1" pad="12"/>
</signal>
<signal name="VBAT">
<contactref element="SWITCHSIDE" pad="13"/>
<contactref element="SWITCHSIDE1" pad="13"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="SWITCHSIDE" pad="3"/>
<contactref element="SWITCHSIDE1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="SWITCHSIDE" pad="6"/>
<contactref element="SWITCHSIDE1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="USBSIDE1" pad="13"/>
<contactref element="USBSIDE" pad="13"/>
<contactref element="SWITCHSIDE" pad="2"/>
<contactref element="SWITCHSIDE1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="USBSIDE1" pad="5"/>
<contactref element="USBSIDE" pad="5"/>
<contactref element="SWITCHSIDE" pad="1"/>
<contactref element="SWITCHSIDE1" pad="1"/>
</signal>
<signal name="PIN_12">
<contactref element="USBSIDE1" pad="11"/>
<contactref element="USBSIDE" pad="11"/>
</signal>
<signal name="1">
<contactref element="FUCKTHIS" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="2">
<contactref element="FUCKTHIS" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="3">
<contactref element="FUCKTHIS" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="J5" pad="3"/>
<contactref element="J6" pad="3"/>
<contactref element="J7" pad="3"/>
<contactref element="J8" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
