(kicad_pcb (version 4) (host pcbnew 4.0.7-e1-6374~58~ubuntu16.04.1)
  (general
    (links 134)
    (no_connects 0)
    (area 116.764999 93.904999 155.015001 111.835001)
    (thickness 1.6)
    (drawings 53)
    (tracks 474)
    (zones 0)
    (modules 43)
    (nets 35)
  )
  (page A4)
  (layers
    (0 Top signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 Bottom signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (trace_clearance 0.1225)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1225)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.441)
    (via_drill 0.245)
    (via_min_size 0.441)
    (via_min_drill 0.245)
    (user_via 0.6615 0.3185)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 0.5 0.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.3 0.3)
    (mod_text_width 0.05)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.025)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(BATT+1-Pad1)")
  (net 2 "Net-(BATT-1-Pad1)")
  (net 3 GND)
  (net 4 3.3v)
  (net 5 vtest)
  (net 6 "Net-(C33-Pad1)")
  (net 7 5v)
  (net 8 "Net-(IC3-Pad10)")
  (net 9 "Net-(LED1-Pad1)")
  (net 10 "Net-(LED2-Pad1)")
  (net 11 "Net-(LED3-Pad1)")
  (net 12 "Net-(Q3-Pad2)")
  (net 13 amp_en)
  (net 14 SDA)
  (net 15 SCL)
  (net 16 sd_en)
  (net 17 miso)
  (net 18 sclk)
  (net 19 mosi)
  (net 20 "Net-(SP+1-Pad1)")
  (net 21 "Net-(SP-1-Pad1)")
  (net 22 INT)
  (net 23 "Net-(IC3-Pad3)")
  (net 24 "Net-(Q4-Pad2)")
  (net 25 "Net-(Q5-Pad2)")
  (net 26 "Net-(Q6-Pad2)")
  (net 27 "Net-(LED4-Pad1)")
  (net 28 "Net-(LED5-Pad1)")
  (net 29 "Net-(LED6-Pad1)")
  (net 30 CH1)
  (net 31 CH2)
  (net 32 I2S_BCLK)
  (net 33 I2S_DATA)
  (net 34 I2S_LRCLK)
  (net_class Default "This is the default net class."
    (clearance 0.1225)
    (trace_width 0.1225)
    (via_dia 0.441)
    (via_drill 0.245)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3v)
    (add_net CH1)
    (add_net CH2)
    (add_net I2S_BCLK)
    (add_net I2S_DATA)
    (add_net I2S_LRCLK)
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(IC3-Pad10)")
    (add_net "Net-(IC3-Pad3)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(Q6-Pad2)")
  )
  (net_class POWER ""
    (clearance 0.1225)
    (trace_width 1.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(BATT-1-Pad1)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(LED4-Pad1)")
    (add_net "Net-(LED5-Pad1)")
    (add_net "Net-(LED6-Pad1)")
  )
  (net_class medium ""
    (clearance 0.1225)
    (trace_width 0.5)
    (via_dia 0.441)
    (via_drill 0.245)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5v)
    (add_net GND)
    (add_net "Net-(BATT+1-Pad1)")
    (add_net "Net-(SP+1-Pad1)")
    (add_net "Net-(SP-1-Pad1)")
  )
  (net_class narrow ""
    (clearance 0.1225)
    (trace_width 0.1225)
    (via_dia 0.441)
    (via_drill 0.245)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net INT)
    (add_net "Net-(Q3-Pad2)")
    (add_net SCL)
    (add_net SDA)
    (add_net amp_en)
    (add_net miso)
    (add_net mosi)
    (add_net sclk)
    (add_net sd_en)
    (add_net vtest)
  )
  (module lightsaber_footprints:teensy32-2.5 (layer Top) (tedit 597C27D1)
    (at 135.89 102.87)
    (fp_text reference U0 (at -0.254 12.319) (layer F.SilkS))
    (fp_text value Teensy_3.2 (at -0.635 -10.541) (layer F.Fab))
    (pad 9 thru_hole circle (at 7.62 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 I2S_BCLK))
    (pad 10 thru_hole circle (at 10.16 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 CH2))
    (pad 6 thru_hole circle (at 0 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 30 CH1))
    (pad 5 thru_hole circle (at -2.54 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Q6-Pad2)"))
    (pad 4 thru_hole circle (at -5.08 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(Q5-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(Q4-Pad2)"))
    (pad 0 thru_hole circle (at -15.24 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 sd_en))
    (pad 2 thru_hole circle (at -10.16 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 22 INT))
    (pad 1 thru_hole circle (at -12.7 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 amp_en))
    (pad 11 thru_hole circle (at 12.7 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 mosi))
    (pad 12 thru_hole circle (at 15.24 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 miso))
    (pad 13 thru_hole circle (at 15.24 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 sclk))
    (pad 14 thru_hole circle (at 12.7 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 vtest))
    (pad 18 thru_hole circle (at 2.54 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 SDA))
    (pad 19 thru_hole circle (at 0 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 SCL))
    (pad 21 thru_hole circle (at -5.08 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(Q3-Pad2)"))
    (pad 22 thru_hole circle (at -7.62 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 I2S_DATA))
    (pad 23 thru_hole circle (at -10.16 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 I2S_LRCLK))
    (pad 24 thru_hole circle (at -12.7 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 3.3v))
    (pad 25 thru_hole circle (at -15.24 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at -17.78 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 5v))
    (pad 27 thru_hole circle (at -17.78 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module lightsaber_footprints:fiduciary (layer Top) (tedit 57F463E7)
    (at 130.556 100.076)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.6) (clearance 0.5))
  )
  (module modules:DM3D-SF (layer Top) (tedit 57DDA3BF)
    (at 121.1326 102.743 270)
    (descr "Micro SD")
    (tags "Micro SD")
    (solder_mask_margin 0.1)
    (solder_paste_margin -0.05)
    (fp_text reference SD1 (at 0 -12.0904 270) (layer F.SilkS))
    (fp_text value microsd_socket (at 1.5 -7 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.25 270) (layer F.Fab) hide)
    (pad 8 smd rect (at -4.5 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask))
    (pad 9 smd rect (at -5.7 0.75 270) (size 1.3 1.5) (layers Top F.Paste F.Mask))
    (pad 10 smd rect (at -5.95 -6.85 270) (size 0.8 1.5) (layers Top F.Paste F.Mask))
    (pad B smd rect (at -5.625 -8.35 270) (size 1.45 1) (layers Top F.Paste F.Mask))
    (pad 11 smd rect (at 6 -7.5 270) (size 0.8 1.4) (layers Top F.Paste F.Mask))
    (pad 7 smd rect (at -3.4 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 17 miso))
    (pad 6 smd rect (at -2.3 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at -1.2 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 18 sclk))
    (pad 4 smd rect (at -0.1 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 3 smd rect (at 1 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 19 mosi))
    (pad 2 smd rect (at 2.1 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 16 sd_en))
    (pad 1 smd rect (at 3.2 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask))
    (pad 12 smd rect (at 5.65 0.75 270) (size 1.5 1.5) (layers Top F.Paste F.Mask))
    (pad A smd rect (at 5.6 -9.8 270) (size 1 1.55) (layers Top F.Paste F.Mask))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA295)
    (at 153.67 110.49)
    (fp_text reference BATT+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.048 0.127) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BATT+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA298)
    (at 153.67 107.95)
    (fp_text reference BATT-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.048 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(BATT-1-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57DD92C6)
    (at 134.62 105.918 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C32 (at -0.762 -0.889 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.635 -0.889 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57DD92FF)
    (at 140.97 104.14 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C33 (at 1.651 -0.381 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 0.127 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:2520 (layer Top) (tedit 597B58C6)
    (at 138.303 107.696 270)
    (fp_text reference L1 (at 1.778 0.762 360) (layer F.SilkS))
    (fp_text value "4.7 uH 1.2A" (at 1.778 -1.016 360) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 0.8 2) (layers Top F.Paste F.Mask)
      (net 23 "Net-(IC3-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 0.8 2) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2A8)
    (at 153.67 105.41)
    (fp_text reference LED1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.175 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(LED1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2A3)
    (at 153.67 102.87)
    (fp_text reference LED2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.175 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(LED2-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA29B)
    (at 153.67 100.33)
    (fp_text reference LED3 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.175 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(LED3-Pad1)"))
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DD9291)
    (at 136.144 108.204 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at -0.381 -0.889 90) (layer F.SilkS))
    (fp_text value 2M (at 0.508 -0.889 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DD931C)
    (at 142.748 103.759)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at -0.381 -0.889) (layer F.SilkS))
    (fp_text value 2M (at 0.635 -0.889) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 8 "Net-(IC3-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DD92B3)
    (at 136.144 105.918 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 1.397 0 90) (layer F.SilkS))
    (fp_text value 220k (at 1.524 0.508 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57FACC0E)
    (at 144.907 104.14)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 1.397 -0.254) (layer F.SilkS))
    (fp_text value 220k (at 1.524 0.254) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 8 "Net-(IC3-Pad10)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA363)
    (at 153.67 97.79)
    (fp_text reference SP+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SP+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2D3)
    (at 153.67 95.25)
    (fp_text reference SP-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SP-1-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57DDA08C)
    (at 133.858 99.568 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0.762 -0.762 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.381 -0.762 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DDA075)
    (at 134.366 97.282)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at -0.508 -0.889) (layer F.SilkS))
    (fp_text value 2.2k (at 0.635 -0.889) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 14 SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DDA03D)
    (at 137.668 97.028 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 1.143 -0.254 270) (layer F.SilkS))
    (fp_text value 2.2k (at 1.143 0.889 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 15 SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:LGA-14L (layer Top) (tedit 57DDA060)
    (at 136.652 99.568)
    (fp_text reference U2 (at 0 0.127) (layer F.SilkS))
    (fp_text value LSM6DS3H (at 1.905 0.254 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.25 -0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.25 0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -1.25 0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 22 INT))
    (pad 5 smd rect (at -0.5 1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 6 smd rect (at 0 1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 0.5 1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1.25 0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 9 smd rect (at 1.25 0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask))
    (pad 10 smd rect (at 1.25 -0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask))
    (pad 11 smd rect (at 1.25 -0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask))
    (pad 12 smd rect (at 0.5 -1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 13 smd rect (at 0 -1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 15 SCL))
    (pad 14 smd rect (at -0.5 -1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 14 SDA))
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 57FACC07)
    (at 145.923 106.426 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0.0635 -1.016 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.016 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:PAD (layer Bottom) (tedit 57F330B7)
    (at 124.46 103.9495 180)
    (fp_text reference LED4 (at 0.635 -0.508 450) (layer B.SilkS))
    (fp_text value Pad (at 0 0.5 180) (layer B.Fab) hide)
    (pad 1 connect rect (at 0 0 180) (size 1.5 3) (layers Bottom B.Mask)
      (net 27 "Net-(LED4-Pad1)"))
  )
  (module lightsaber_footprints:PAD (layer Bottom) (tedit 57F330B7)
    (at 128.397 104.013)
    (fp_text reference LED5 (at 0.635 -0.508 270) (layer B.SilkS))
    (fp_text value Pad (at 0 0.5) (layer B.Fab) hide)
    (pad 1 connect rect (at 0 0) (size 1.5 3) (layers Bottom B.Mask)
      (net 28 "Net-(LED5-Pad1)"))
  )
  (module lightsaber_footprints:PAD (layer Bottom) (tedit 57F330B7)
    (at 132.461 104.013)
    (fp_text reference LED6 (at 0.635 -0.508 270) (layer B.SilkS))
    (fp_text value Pad (at 0 0.5) (layer B.Fab) hide)
    (pad 1 connect rect (at 0 0) (size 1.5 3) (layers Bottom B.Mask)
      (net 29 "Net-(LED6-Pad1)"))
  )
  (module lightsaber_footprints:SOT-23F (layer Bottom) (tedit 57F339F1)
    (at 124.46 107.569 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at -0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 24 "Net-(Q4-Pad2)"))
    (pad 3 smd rect (at 0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 1 smd rect (at 0 0.99822 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 27 "Net-(LED4-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOT-23F (layer Bottom) (tedit 57F339F1)
    (at 128.397 107.569 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at -0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 25 "Net-(Q5-Pad2)"))
    (pad 3 smd rect (at 0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 1 smd rect (at 0 0.99822 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 28 "Net-(LED5-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOT-23F (layer Bottom) (tedit 57F339F1)
    (at 132.3975 107.569 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at -0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 26 "Net-(Q6-Pad2)"))
    (pad 3 smd rect (at 0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 1 smd rect (at 0 0.99822 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 29 "Net-(LED6-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57FACCD8)
    (at 137.414 102.108 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0.508 -0.762 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.762 -0.762 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 597B5810)
    (at 140.208 99.441 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -0.635 1.016 90) (layer F.SilkS))
    (fp_text value 10uF (at 0.762 0.889 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:QFN-10-PAD (layer Top) (tedit 58AFB0F7)
    (at 142.24 106.934 270)
    (descr 9)
    (fp_text reference IC3 (at 1.5 1 360) (layer F.SilkS))
    (fp_text value TPS61200 (at 0 -0.5 270) (layer F.Fab))
    (pad 15 smd rect (at 1.524 0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.25))
    (pad 14 smd rect (at 1.524 -0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.25))
    (pad 13 smd rect (at -1.524 0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.25))
    (pad 11 smd rect (at 0 0 270) (size 2.4 1.65) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin -0.14))
    (pad 9 smd oval (at -0.5 -1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd oval (at 1 1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 6 smd oval (at 1 -1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 4 smd oval (at 0.5 1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd oval (at 0 1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 23 "Net-(IC3-Pad3)"))
    (pad 1 smd oval (at -1 1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C33-Pad1)"))
    (pad 2 smd oval (at -0.5 1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 7 smd oval (at 0.5 -1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (pad 8 smd oval (at 0 -1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 10 smd oval (at -1 -1.5 270) (size 0.28 0.8) (layers Top F.Paste F.Mask)
      (net 8 "Net-(IC3-Pad10)"))
    (pad 12 smd rect (at -1.524 -0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.25))
  )
  (module lightsaber_footprints:DMG7430LFG (layer Top) (tedit 597B58E5)
    (at 150.622 99.314 270)
    (fp_text reference Q3 (at 0 0.889 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 12 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer Top) (tedit 597B58E9)
    (at 150.622 102.87 270)
    (fp_text reference Q2 (at 0 0.889 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 31 CH2))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)") (solder_paste_margin -0.1))
  )
  (module lightsaber_footprints:DMG7430LFG (layer Top) (tedit 597B58ED)
    (at 150.622 106.426 270)
    (fp_text reference Q1 (at 0 0.889 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 30 CH1))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)") (solder_paste_margin -0.1))
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58B1128B)
    (at 138.303 103.632 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.762 360) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58B11283)
    (at 138.303 105.156 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.762 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:fiduciary locked (layer Top) (tedit 57F463E7)
    (at 124.46 108.204)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.6) (clearance 0.5))
  )
  (module lightsaber_footprints:fiduciary locked (layer Top) (tedit 57F463E7)
    (at 118.11 97.536)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.6) (clearance 0.5))
  )
  (module lightsaber_footprints:fiduciary locked (layer Bottom) (tedit 57F463E7)
    (at 118.11 106.426)
    (fp_text reference "" (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0.5) (layer B.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers Bottom B.Mask)
      (solder_mask_margin 0.6) (clearance 0.5))
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer Top) (tedit 597B5890)
    (at 135.001 103.505 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0.508 1.524 180) (layer F.SilkS))
    (fp_text value 10k (at -0.635 1.524 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.5 -0.75 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -0.5 0.25 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.5 -0.25 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -0.5 0.75 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 7 smd rect (at 0.5 -0.25 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 25 "Net-(Q5-Pad2)"))
    (pad 8 smd rect (at 0.5 -0.75 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 26 "Net-(Q6-Pad2)"))
    (pad 6 smd rect (at 0.5 0.25 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 24 "Net-(Q4-Pad2)"))
    (pad 5 smd rect (at 0.5 0.75 180) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 16 sd_en))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer Top) (tedit 597B5851)
    (at 145.669 102.362 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at -0.762 -1.524 270) (layer F.SilkS))
    (fp_text value 10k (at 0.762 -1.524 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 12 "Net-(Q3-Pad2)"))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 13 amp_en))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 31 CH2))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.32) (layers Top F.Paste F.Mask)
      (net 30 CH1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 597B581A)
    (at 141.986 99.187 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0.635 -0.635 90) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.762 -0.635 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm_ThermalVias (layer Top) (tedit 597C0C52)
    (at 144.526 98.298)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 2.159 -1.27) (layer F.SilkS))
    (fp_text value MAX98357A_TQFN (at 0.127 2.286) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 33 I2S_DATA))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 13 amp_en))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 20 "Net-(SP+1-Pad1)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 21 "Net-(SP-1-Pad1)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers Top F.Paste F.Mask))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 34 I2S_LRCLK))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers Top F.Paste F.Mask)
      (net 32 I2S_BCLK))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at 0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 17 thru_hole circle (at -0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 143.256 111.76) (end 153.67 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.541 109.982) (end 141.732 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.017 111.76) (end 133.604 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 93.98) (end 153.67 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text ID (at 133.35 96.52) (layer B.SilkS))
  (gr_text "LED6-\n" (at 133.731 104.9655 90) (layer B.SilkS))
  (gr_text "LED5-\n" (at 129.667 104.9655 90) (layer B.SilkS))
  (gr_text "LED4-\n" (at 125.7935 104.902 90) (layer B.SilkS))
  (gr_line (start 133.604 111.76) (end 125.984 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.033 110.49) (end 137.033 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.541 110.49) (end 137.033 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136.017 110.744) (end 137.033 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 93.98) (end 118.11 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.112 95.758) (end 132.588 95.758) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 95.758) (end 140.208 95.758) (layer Edge.Cuts) (width 0.15))
  (gr_text buttons (at 143.7005 97.2185) (layer B.SilkS))
  (gr_text 3 (at 141.732 96.52) (layer B.SilkS))
  (gr_text 2 (at 143.764 96.52) (layer B.SilkS))
  (gr_text 1 (at 145.796 96.52) (layer B.SilkS))
  (gr_text SPKR+ (at 151.384 98.425) (layer B.SilkS))
  (gr_text "SPKR-\n" (at 151.892 96.774 45) (layer B.SilkS))
  (gr_text "BATT+\n" (at 151.892 108.966 315) (layer B.SilkS))
  (gr_text "BATT-\n" (at 151.511 107.188) (layer B.SilkS))
  (gr_text "LED3-\n" (at 151.384 100.711) (layer B.SilkS))
  (gr_text "LED2-\n" (at 151.384 102.997) (layer B.SilkS))
  (gr_text LED1- (at 151.384 105.283) (layer B.SilkS))
  (gr_text GND (at 118.11 108.331 90) (layer B.SilkS))
  (gr_text "TeensySaber V3.0, by Fredrik Hubinette\nhttp://fredrik.hubbe.net/lightsaber/v3/\n" (at 145.7325 100.1395) (layer B.SilkS))
  (gr_line (start 116.84 110.49) (end 116.84 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.11 110.49) (end 118.11 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.11 95.25) (end 116.84 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 110.49) (end 142.24 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 95.25) (end 147.32 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 94.996) (end 139.7 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141.732 110.49) (end 141.732 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.812 95.25) (end 147.32 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.208 95.25) (end 140.208 95.758) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 93.98) (end 138.684 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 93.98) (end 148.336 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 95.25) (end 154.94 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.256 110.744) (end 143.256 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 110.49) (end 154.94 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 95.25) (end 153.67 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.336 94.996) (end 147.32 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.684 94.996) (end 138.684 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 95.25) (end 132.08 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 94.996) (end 134.62 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135.636 94.996) (end 134.62 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.112 95.25) (end 134.62 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.588 95.25) (end 132.588 95.758) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.064 94.996) (end 131.064 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.636 93.98) (end 138.43 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.984 111.76) (end 118.11 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.383 91.059) (xy 151.003 90.678) (xy 158.623 94.996) (xy 158.623 106.426) (xy 151.765 115.8875)
        (xy 115.189 115.189) (xy 114.935 91.44) (xy 132.207 90.551)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.903 86.233) (xy 148.082 86.106) (xy 148.209 119.253) (xy 112.903 119.253)
      )
    )
  )
  (zone (net 10) (net_name "Net-(LED2-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.686 101.727) (xy 154.686 103.886) (xy 150.876 103.886) (xy 150.876 101.727)
      )
    )
  )
  (zone (net 9) (net_name "Net-(LED1-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.686 104.394) (xy 152.781 104.394) (xy 152.146 104.648) (xy 150.622 104.648) (xy 150.114 105.156)
        (xy 150.114 107.315) (xy 152.273 107.315) (xy 153.035 106.807) (xy 154.686 106.553)
      )
    )
  )
  (zone (net 11) (net_name "Net-(LED3-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.289 98.933) (xy 154.559 99.187) (xy 154.686 99.314) (xy 154.686 101.219) (xy 152.527 101.219)
        (xy 151.892 101.092) (xy 151.257 100.965) (xy 150.495 100.457) (xy 150.495 98.298) (xy 152.273 98.298)
      )
    )
  )
  (zone (net 10) (net_name "Net-(LED2-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.686 101.727) (xy 154.686 103.886) (xy 150.876 103.886) (xy 150.876 101.727)
      )
    )
  )
  (zone (net 9) (net_name "Net-(LED1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.686 104.394) (xy 152.781 104.394) (xy 152.146 104.648) (xy 150.622 104.648) (xy 150.114 105.156)
        (xy 150.114 107.315) (xy 152.273 107.315) (xy 153.035 106.807) (xy 154.686 106.553)
      )
    )
  )
  (zone (net 11) (net_name "Net-(LED3-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.289 98.933) (xy 154.559 99.187) (xy 154.686 99.314) (xy 154.686 101.219) (xy 152.527 101.219)
        (xy 151.892 101.092) (xy 151.257 100.965) (xy 150.495 100.457) (xy 150.495 98.298) (xy 152.273 98.298)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.812 93.345) (xy 146.812 113.665) (xy 160.401 113.665) (xy 160.401 93.345) (xy 159.639 93.345)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 97.79) (xy 149.225 99.822) (xy 147.32 99.822) (xy 147.32 97.79)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 103.378) (xy 147.32 103.378) (xy 147.32 101.092) (xy 149.225 101.092)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 106.934) (xy 147.32 106.934) (xy 147.32 104.648) (xy 149.225 104.648)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.304 93.345) (xy 146.304 113.665) (xy 112.141 113.665) (xy 112.141 93.345) (xy 113.411 93.345)
      )
    )
  )
)
