(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 95)
    (zones 0)
    (modules 2)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad16)")
  (net 2 "Net-(J1-Pad15)")
  (net 3 "Net-(J1-Pad14)")
  (net 4 "Net-(J1-Pad13)")
  (net 5 "Net-(J1-Pad12)")
  (net 6 "Net-(J1-Pad11)")
  (net 7 "Net-(J1-Pad10)")
  (net 8 "Net-(J1-Pad9)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad7)")
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J1-Pad5)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad2)")
  (net 16 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module "Coil Library:SLW16R-1C7LF" (layer F.Cu) (tedit 0)
    (at 110.991001 91.948001)
    (fp_text reference J1 (at 7.5 0) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 7.5 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 16 thru_hole circle (at 15.000001 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad16)"))
    (pad 15 thru_hole circle (at 14 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at 13 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at 11.999999 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at 11.000001 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at 10 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 10 thru_hole circle (at 9 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 9 thru_hole circle (at 7.999999 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at 6.999999 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at 6.000001 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at 5 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 4 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 2.999999 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 2.000001 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 1.000001 -2.000001) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 151.1808 89.7382 270)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad12)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad13)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad14)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad15)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 104.14 104.14) (end 104.14 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.94 104.14) (end 104.14 104.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.94 78.74) (end 154.94 104.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.14 78.74) (end 154.94 78.74) (layer Edge.Cuts) (width 0.05))
)
