(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 64)
    (zones 0)
    (modules 8)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VTarget)
  (net 2 /SWDIO)
  (net 3 /SWCLK)
  (net 4 /SWO)
  (net 5 "Net-(J1-Pad7)")
  (net 6 "Net-(J1-Pad8)")
  (net 7 /RESET)
  (net 8 "Net-(J1-Pad11)")
  (net 9 "Net-(J1-Pad12)")
  (net 10 "Net-(J1-Pad13)")
  (net 11 "Net-(J1-Pad14)")
  (net 12 "Net-(J1-Pad16)")
  (net 13 "Net-(J1-Pad18)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RESET)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /VTarget)
    (add_net GND)
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 112.776 100.076 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference TP5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SWO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PearlGecko_EDT:PinHeader_2x10_P1.27mm_Vertical_Mirrored (layer B.Cu) (tedit 5E471A56)
    (at 102.108 105.791)
    (descr "Through hole straight pin header, 2x10, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 1.27mm double row")
    (fp_text reference J1 (at 3.556 0.381 270) (layer B.SilkS))
    (fp_text value Conn_02x10_Odd_Even (at 0.635 -13.125 180) (layer B.Fab))
    (fp_text user %R (at 0.635 -5.842 90) (layer B.Fab))
    (pad 20 thru_hole oval (at 0 -11.557) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 1.27 -11.557) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 18 thru_hole oval (at 0 -10.287) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 1.27 -10.287) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 16 thru_hole oval (at 0 -9.017) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 1.27 -9.017) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 14 thru_hole oval (at 0 -7.747) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 1.27 -7.747) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -6.477) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 1.27 -6.477) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -5.207) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 9 thru_hole oval (at 1.27 -5.207) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 8 thru_hole oval (at 0 -3.937) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 1.27 -3.937) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -2.667) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /SWO))
    (pad 5 thru_hole oval (at 1.27 -2.667) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 4 thru_hole oval (at 0 -1.397) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 3 thru_hole oval (at 1.27 -1.397) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 2 thru_hole oval (at 0 -0.127) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /SWDIO))
    (pad 1 thru_hole rect (at 1.27 -0.127) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 /VTarget))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 119.38 97.79)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at -1.524 -3.048 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SWO))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SWDIO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VTarget))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.966 100.076 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference TP1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.966 103.886 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference TP2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VTarget))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.966 96.266 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference TP3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /SWCLK))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 112.776 103.886 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference TP4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SWDIO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 112.776 96.266 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference TP6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 99.568 108.966) (end 99.568 91.186) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.968 108.966) (end 99.568 108.966) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.968 91.186) (end 124.968 108.966) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.568 91.186) (end 124.968 91.186) (layer Edge.Cuts) (width 0.05))
  (dimension 17.78 (width 0.15) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 129.316 100.076 90) (layer Dwgs.User))
    (feature1 (pts (xy 124.968 91.186) (xy 128.602421 91.186)))
    (feature2 (pts (xy 124.968 108.966) (xy 128.602421 108.966)))
    (crossbar (pts (xy 128.016 108.966) (xy 128.016 91.186)))
    (arrow1a (pts (xy 128.016 91.186) (xy 128.602421 92.312504)))
    (arrow1b (pts (xy 128.016 91.186) (xy 127.429579 92.312504)))
    (arrow2a (pts (xy 128.016 108.966) (xy 128.602421 107.839496)))
    (arrow2b (pts (xy 128.016 108.966) (xy 127.429579 107.839496)))
  )
  (gr_text "Sid Price Design (C) 2020\nEDT DBG Adapter" (at 115.824 106.934) (layer F.SilkS))
  (gr_text RST (at 115.062 96.266 90) (layer F.SilkS))
  (gr_text SWO (at 115.062 99.822 90) (layer F.SilkS))
  (gr_text SWDIO (at 115.062 103.632 90) (layer F.SilkS))
  (gr_text VTG (at 106.68 103.886 90) (layer F.SilkS))
  (gr_text GND (at 106.68 100.076 90) (layer F.SilkS))
  (gr_text SWCLK (at 106.68 96.266 90) (layer F.SilkS))
  (zone (net 15) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.822 91.44) (xy 124.714 91.44) (xy 124.714 108.712) (xy 99.822 108.712)
      )
    )
  )
  (zone (net 15) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.822 91.44) (xy 124.714 91.44) (xy 124.714 108.712) (xy 99.822 108.712)
      )
    )
  )
)
