(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 19)
    (no_connects 0)
    (area 154.229999 83.744999 175.335001 119.455001)
    (thickness 1.6)
    (drawings 7)
    (tracks 49)
    (zones 0)
    (modules 10)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GNDD)
  (net 3 /VCC_LINE)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 +12V)
  (net 7 "Net-(U1-Pad1)")
  (net 8 "Net-(U1-Pad3)")
  (net 9 "Net-(U1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /VCC_LINE)
    (add_net GNDD)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
  )
  (module Housings_SSOP:MSOP-8-1EP_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 162.645 108.655 90)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -2.55 90) (layer F.SilkS))
    (fp_text value LTC4071 (at 0 2.55 90) (layer F.Fab))
    (pad 1 smd rect (at -2.105 -0.975 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.105 -0.325 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC_LINE))
    (pad 3 smd rect (at -2.105 0.325 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.105 0.975 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 2.105 0.975 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC_LINE))
    (pad 6 smd rect (at 2.105 0.325 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 7 smd rect (at 2.105 -0.325 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 8 smd rect (at 2.105 -0.975 90) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC_LINE))
    (pad 9 smd rect (at 0.42 0.47 90) (size 0.84 0.94) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.42 -0.47 90) (size 0.84 0.94) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.42 0.47 90) (size 0.84 0.94) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.42 -0.47 90) (size 0.84 0.94) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD) (solder_paste_margin_ratio -0.2))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 163.83 100.965 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDD))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC_LINE))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads_:SolderWirePad_2x_2mmDrill_30mmWide (layer F.Cu) (tedit 574F4CDA)
    (at 157.48 101.36 270)
    (fp_text reference BT1 (at 0 0 270) (layer F.SilkS))
    (fp_text value Battery (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -15 0 270) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 270) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDD))
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 0)
    (at 170.18 101.6 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference D1 (at 0.254 -2.413 90) (layer F.SilkS))
    (fp_text value LED (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDD))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Handsoldering (layer F.Cu) (tedit 552FF1AB)
    (at 163.83 88.9 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 0 -2.85 90) (layer F.SilkS))
    (fp_text value D (at 0.05 4.4 90) (layer F.Fab))
    (fp_text user K (at -3.25 2.9 90) (layer F.SilkS))
    (fp_text user A (at 3.05 2.85 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.49936 0 90) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.49936 0 90) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
    (model Diodes_SMD.3dshapes/SMA_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 170.18 86.36)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 2.54) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 +12V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 170.18 116.84)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.54) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Oddities:NetTie-I (layer F.Cu) (tedit 0)
    (at 170.18 91.44)
    (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC. Make connection between 1 and 2 by yourself.")
    (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC. Make connection between 1 and 2 by yourself.")
    (fp_text reference R3 (at 0 0) (layer F.SilkS))
    (fp_text value Photores (at 0 -3.048) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VCC_LINE))
    (pad 2 thru_hole rect (at 2.54 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 170.18 93.98 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC_LINE))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 162.56 95.885 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC_LINE))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Milkyware\n @>%---\n   - H&G" (at 165.1 101.6 90) (layer B.SilkS))
  (gr_line (start 154.305 119.38) (end 154.94 119.38) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.305 83.82) (end 154.305 119.38) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 83.82) (end 154.305 83.82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 119.38) (end 175.26 119.38) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 83.82) (end 154.94 83.82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 119.38) (end 175.26 83.82) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.26 119.38) (xy 175.26 83.82) (xy 154.94 83.82) (xy 154.94 119.38)
      )
    )
  )
)
