(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 188)
    (zones 0)
    (modules 22)
    (nets 22)
  )
  (page A4)
  (title_block
    (title "Mad Cat Backpack")
    (date 2018-10-17)
    (rev V0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.3556)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.69)
    (via_drill 0.33)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFDDF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(D5-Pad1)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 "Net-(D6-Pad1)")
  (net 12 "Net-(D6-Pad2)")
  (net 13 "Net-(D7-Pad1)")
  (net 14 "Net-(D7-Pad2)")
  (net 15 "Net-(D8-Pad1)")
  (net 16 "Net-(D8-Pad2)")
  (net 17 GND)
  (net 18 +5V)
  (net 19 "Net-(J2-Pad5)")
  (net 20 "Net-(J2-Pad4)")
  (net 21 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.69)
    (via_drill 0.33)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E61B)
    (at 153.3525 119.4435 90)
    (fp_text reference D8 (at 4.3815 -1.2065) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 90) (layer F.Fab))
    (fp_text user - (at 2.4765 2.667 90) (layer F.SilkS) hide)
    (fp_text user + (at -2.3495 2.667 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D8-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E64D)
    (at 128.905 109.2835)
    (fp_text reference D1 (at 4.445 -1.3335) (layer F.SilkS))
    (fp_text value LED (at 0 3.556) (layer F.Fab))
    (fp_text user - (at 2.413 -2.6035) (layer F.SilkS) hide)
    (fp_text user + (at -2.413 -2.6035) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -2.4 0) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E631)
    (at 148.082 109.474 180)
    (fp_text reference D2 (at 4.572 1.27 180) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 180) (layer F.Fab))
    (fp_text user - (at 2.413 2.54 180) (layer F.SilkS) hide)
    (fp_text user + (at -2.413 2.54 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 180) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -2.4 0 180) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E5B0)
    (at 123.952 119.3165 90)
    (fp_text reference D3 (at 4.2545 1.524) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 90) (layer F.Fab))
    (fp_text user - (at 2.4765 -2.921 90) (layer F.SilkS) hide)
    (fp_text user + (at -2.4765 -2.921 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E5C2)
    (at 128.9685 124.1425 90)
    (fp_text reference D4 (at 2.4765 -2.4765 90) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 90) (layer F.Fab))
    (fp_text user - (at 2.4765 -2.6035 90) (layer F.SilkS) hide)
    (fp_text user + (at -2.3495 -2.6035 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E5DF)
    (at 135.636 125.73 90)
    (fp_text reference D5 (at 4.318 1.524 180) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 90) (layer F.Fab))
    (fp_text user - (at 2.413 -2.667 90) (layer F.SilkS) hide)
    (fp_text user + (at -2.413 -2.667 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E5EF)
    (at 142.1765 125.476 90)
    (fp_text reference D6 (at 4.318 1.3335) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 90) (layer F.Fab))
    (fp_text user - (at 2.413 -2.7305 90) (layer F.SilkS) hide)
    (fp_text user + (at -2.413 -2.7305 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D6-Pad2)"))
  )
  (module customparts:LED_OSRAM_TOPLED_LxT776 (layer F.Cu) (tedit 5BC7E605)
    (at 148.3995 124.333 90)
    (fp_text reference D7 (at 4.445 1.4605) (layer F.SilkS))
    (fp_text value LED (at 0 3.556 90) (layer F.Fab))
    (fp_text user - (at 2.413 -2.7305 90) (layer F.SilkS) hide)
    (fp_text user + (at -2.413 -2.7305 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at -2.4 0 90) (size 1.2 2.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D7-Pad2)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5B261024)
    (at 123.952 120.062 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.08 -1.778 90) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module badgelife:Badgelife-Shitty-2x2 (layer F.Cu) (tedit 5BC7E66D)
    (at 147.0025 135.6995)
    (descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x02 2.54mm double row")
    (fp_text reference X1 (at 0 0) (layer F.Fab))
    (fp_text value Badgelife_shitty_connector (at 0 4.2) (layer F.Fab))
    (fp_text user SDA (at 1.5 -3) (layer B.SilkS))
    (fp_text user SCL (at 3.3655 0.9525) (layer B.SilkS))
    (fp_text user GND (at -3.4925 0.9525) (layer B.SilkS))
    (fp_text user VCC (at -1.5 -3) (layer B.SilkS))
    (pad 4 thru_hole circle (at 1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole oval (at -1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_Mini_B_Female_UJ2-MBH-1-SMT-TR (layer B.Cu) (tedit 59D259DB)
    (at 130.642 137.836 180)
    (fp_text reference J1 (at 4.658 10.074 180) (layer B.SilkS))
    (fp_text value USB_B_Mini (at 0.225 -2.65 180) (layer B.Fab))
    (fp_text user %R (at 0.025 1.35 180) (layer B.Fab))
    (pad 6 smd rect (at 4.36 2.37 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 6 smd rect (at -4.36 2.37 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 6 smd rect (at -4.36 7.85 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 6 smd rect (at 4.36 7.85 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 1 smd rect (at -1.6 7.85 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 2 smd rect (at -0.8 7.85 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 0 7.85 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 0.8 7.85 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.6 7.85 180) (size 0.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 6 thru_hole circle (at -2.2 4.74 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 6 thru_hole circle (at 2.2 4.74 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 128.524 118.618 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 2.54 -1.016 180) (layer F.SilkS))
    (fp_text value PicKit (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 127.936 109.22 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.778 180) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.844 109.474)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 153.416 120.222 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.336 125.222 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 142.24 126.238 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 135.636 125.556 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 129.032 124.968 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 200 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 58CC8F64)
    (at 138.43 112.522 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -4.318 4.064) (layer B.SilkS))
    (fp_text value PIC16F1503 (at 0 -5.375 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 14 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 13 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J2-Pad4)"))
    (pad 12 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 9 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 8 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D6-Pad1)"))
    (pad 7 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 6 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D8-Pad1)"))
    (pad 5 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D7-Pad1)"))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 131.826 111.76 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 GND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS-icons:metroid (layer B.Cu) (tedit 5A0106A6)
    (at 143.002 134.366 270)
    (fp_text reference icon1 (at 0 -2.54 270) (layer B.Fab) hide)
    (fp_text value Metroid (at 0 2.54 270) (layer B.SilkS) hide)
    (pad "" smd circle (at -0.635 0 270) (size 0.635 0.635) (layers B.Cu B.Paste B.Mask))
    (pad "" smd circle (at 0.635 0 270) (size 0.635 0.635) (layers B.Cu B.Paste B.Mask))
    (pad "" smd circle (at 0 0.635 270) (size 0.635 0.635) (layers B.Cu B.Paste B.Mask))
  )
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 198.12 175.514) (layer F.SilkS))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 198.12 175.514) (layer F.Cu))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 198.12 175.514) (layer B.Cu))
  (gr_text "Mad Cat Backpack\nPJS 17Oct2018 V0\nMIT license" (at 151.384 129.286 90) (layer B.SilkS))
  (gr_line (start 151.384 137.16) (end 150.114 138.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 133.096) (end 151.384 137.16) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 128.016) (end 155.448 133.096) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 109.728) (end 155.448 128.016) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.908 107.188) (end 155.448 109.728) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 107.188) (end 152.908 107.188) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 109.728) (end 124.46 107.188) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.224 137.922) (end 142.748 137.414) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.714 132.334) (end 124.714 137.922) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.714 128.27) (end 124.714 132.334) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 124.206) (end 124.714 128.27) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 109.728) (end 121.92 124.206) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 138.43) (end 150.114 138.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.748 137.414) (end 143.764 138.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.714 137.922) (end 141.224 137.922) (layer Edge.Cuts) (width 0.15))
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 106.426) (xy 156.21 106.426) (xy 156.21 138.43) (xy 121.92 138.43)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 106.426) (xy 156.21 106.426) (xy 156.21 138.43) (xy 121.92 138.43)
      )
    )
  )
)
