<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="49" y2="0" width="0.1524" layer="20"/>
<wire x1="49" y1="0" x2="49" y2="58" width="0.1524" layer="20"/>
<wire x1="49" y1="58" x2="0" y2="58" width="0.1524" layer="20"/>
<wire x1="0" y1="58" x2="0" y2="0" width="0.1524" layer="20"/>
<hole x="3" y="3" drill="3.2"/>
<hole x="3" y="55" drill="3.2"/>
<hole x="46" y="3" drill="3.2"/>
<hole x="46" y="55" drill="3.2"/>
<text>GPIO1</text>
<text>GPIO2</text>
<text>!DRDY</text>
<text>MISO</text>
<text>SCK</text>
<text>MOSI</text>
<text>!CS</text>
<text>START</text>
<text>CLK</text>
<text>CLKSEL</text>
<text>EXTERNAL</text>
<text>INTERNAL</text>
<text>RLD REROUTE/
READ</text>
<text>!PWDN!/!RESET!</text>
<text>DVDD</text>
<text>DVDD</text>
<text>DGND</text>
<text>DGND</text>
<text>AGND</text>
<text>AVDD</text>
<text>AVDD</text>
<text>AGND</text>
<text>INT_CLK</text>
<text>EXT_CLK</text>
<text>First Order
Low Pass Filter</text>
<text>Common Mode &amp;
Differential
EMI/RFI Filter</text>
<text>Channel Disable Pullups</text>
</plain>
<libraries>
<library name="Alex's Corrected Parts">
<packages>
<package name="TQFP32(5X5,AAA)">
<description>32-lead, 5 x 5 mm Body Size, 1.00 mm Body Thickness, 0.5 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP) &lt;p&gt;

&lt;b&gt; Based on JEDEC MS-026 variation AAA &lt;/b&gt; &lt;p&gt;

Silk Screen reflects nominal dimensions of TQFP44 Package, as detailed in JEDEC MS-026, variation AAA&lt;p&gt;

Pads are design to add .03mm to Max pin condition (in between spacing) and .30mm to the nominal pin length, both as detailed in JEDEC MS-026 variation AAA&lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; J. Alex Heller (2013/11/20) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/01/16) &lt;br&gt;</description>
</package>
<package name="TP(C)-1.5">
<description>&lt;b&gt;TEST POINT (TP)&lt;/b&gt;, 1.5mmØ&lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; J. Alex Heller (2013/12/30) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/07) &lt;p&gt;

&lt;b&gt; Change Log:&lt;/b&gt;&lt;br&gt;
2014/11/07 - Changed font size and removed cream.</description>
</package>
<package name="C0805(M2012)_TANT">
<description>&lt;b&gt;CAPACITOR, Polizarized Tantalum&lt;/b&gt;, 0805 Size (Metric 2012), 2.00mm x 1.25mm, &lt;u&gt; Reflow Soldering&lt;/u&gt;&lt;p&gt;

Sizes (Case Code):&lt;br&gt;
AVX: N, R, P &lt;br&gt;
Kemet: R &lt;p&gt;

&lt;b&gt;Source(s):&lt;/b&gt; http://www.kemet.com/kemet/web/homepage/kechome.nsf/file/KEM_TC101_STD.pdf/$file/KEM_TC101_STD.pdf, http://www.tortai-tech.com/upload/download/2011102023233369053.pdf, http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Tantalum_Capacitors.pdf&lt;p&gt;

Based on Samsung's suggested Land Pattern, Kemet's KEM TC101 STD, and IPC-SM-782. &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; J. Alex Heller (2013/12/09) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03)&lt;br&gt;</description>
</package>
<package name="R0805(M2012)">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;, 0805 Size (Metric 2012), 2.00mm x 1.25mm, &lt;u&gt;Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03) &lt;br&gt;</description>
</package>
<package name="C0805(M2012)">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;, 0805 Size (Metric 2012), 2.00mm x 1.25mm,&lt;u&gt; Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

Samsung datasheet is for Chip Resistors; this package uses the same land patterns for Chip Capacitors &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03) &lt;br&gt;</description>
</package>
<package name="C0603(M1608)">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;, 0603 Size (Metric 1608), 1.60mm x 0.80mm,&lt;u&gt; Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

Samsung datasheet is for Chip Resistors; this package uses the same land patterns for Chip Capacitors &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03) &lt;br&gt;</description>
</package>
<package name="C0402(M1005)">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;, 0402 Size (Metric 1005), 1.00mm x 0.50mm,&lt;u&gt; Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

Samsung datasheet is for Chip Resistors; this package uses the same land patterns for Chip Capacitors &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03) &lt;br&gt;</description>
</package>
<package name="R0603(M1608)">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;, 0603 Size (Metric 1608), 1.60mm x 0.80mm,&lt;u&gt; Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03) &lt;br&gt;</description>
</package>
<package name="R0402(M1005)">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;, 0402 Size (Metric 1005), 1.00mm x 0.50mm,&lt;u&gt; Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2014/11/03) &lt;br&gt;</description>
</package>
<package name="U.FL-R-SMT-1">
<description>Connector, Jack, Male Pin, U.FL (Ultra Miniature Coax), 50Ω Impedance, Snap-On, 2.6mm x 2.6mm Body Size, 1.25mm Body Thickness, Surface Mount&lt;p&gt;

&lt;b&gt;Layout for:&lt;/b&gt; Hirose U.FL-R-SMT-1 &lt;p&gt;

Silk Screen reflects nominal dimensions of part, as detailed in Hirose provided spec: https://www.hirose.com/product/en/download_file/key_name/U.FL-R-SMT-1%2832%29/category/Drawing%20(2D)/doc_file_id/37630/?file_category_id=6&amp;item_id=03310472232&amp;is_series=&lt;p&gt;

Pads are design to reflect the suggested pad layout, as detailed in Hirose provided spec&lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; J. Alex Heller (2016/04/01) &lt;br&gt;
&lt;b&gt;Last Edited  By (on):&lt;/b&gt; J. Alex Heller (2016/04/01) &lt;br&gt;</description>
</package>
</packages>
</library>
<library name="ADuCM350 Breakout Board Pins">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Capacitors">
<packages>
<package name="C0402(M1005)">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;, 0402 Size (Metric 1005), 1.00mm x 0.50mm, &lt;u&gt;Reflow Soldering&lt;/u&gt;&lt;p&gt;

Source: http://www.samsungsem.com/servlet/FileDownload?filename=productcatalog/pdf/Chip_Resistor.pdf &lt;p&gt;

Based on Samsung's suggested Land Pattern for Reflow Soldering for this package size&lt;/b&gt;, details on Page 5 under Example Land Patterns. &lt;p&gt;

Samsung datasheet is for Chip Resistors; this package uses the same land patterns for Chip Capacitors &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt; Philip Chung (2013/11/01) &lt;br&gt;
&lt;b&gt;Last Edited By (on):&lt;/b&gt; J. Alex Heller (2017/01/27) &lt;p&gt;

&lt;b&gt;Change Log: &lt;/b&gt;&lt;br&gt;
2017/01/27 - Changed tStop for pins to be 0.05mm clearance past the pads</description>
</package>
</packages>
</library>
<library name="Pins">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER 2 x 5&lt;/b&gt;</description>
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Logos">
<packages>
<package name="4MM-FILLED-SILK-IRL">
<description>&lt;b&gt;IRL Logo&lt;/b&gt;, Filled, Slik Screen, 4mm x 7.3mm &lt;p&gt;

&lt;b&gt;Made By (on):&lt;/b&gt;Andrew M. Carek (2018/08/06) &lt;br&gt;
&lt;b&gt;Last Edited By (on):&lt;/b&gt; Andrew M. Carek (2018/08/06) &lt;p&gt;

&lt;b&gt;Change Log: &lt;/b&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="Alex's Corrected Parts" package="TQFP32(5X5,AAA)" value="ADS1292-PBS(S-PQFP-G32)">
<attribute name="NAME"/>
</element>
<element name="TP1" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="C2" library="Alex's Corrected Parts" package="C0805(M2012)_TANT" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="Alex's Corrected Parts" package="C0603(M1608)" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="Alex's Corrected Parts" package="C0402(M1005)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="Alex's Corrected Parts" package="C0402(M1005)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="Alex's Corrected Parts" package="C0402(M1005)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="Alex's Corrected Parts" package="C0402(M1005)" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="Alex's Corrected Parts" package="C0402(M1005)" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="Alex's Corrected Parts" package="C0805(M2012)" value="NP">
<attribute name="NAME"/>
</element>
<element name="C10" library="Alex's Corrected Parts" package="C0805(M2012)" value="NP">
<attribute name="NAME"/>
</element>
<element name="R1" library="Alex's Corrected Parts" package="R0402(M1005)" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="R2" library="Alex's Corrected Parts" package="R0402(M1005)" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="R3" library="Alex's Corrected Parts" package="R0402(M1005)" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="R4" library="Alex's Corrected Parts" package="R0402(M1005)" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="R5" library="Alex's Corrected Parts" package="R0402(M1005)" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="TP2" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP3" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP4" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP5" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP6" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP7" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP8" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP9" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP10" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP11" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP12" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP13" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP14" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="R6" library="Alex's Corrected Parts" package="R0402(M1005)" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R7" library="Alex's Corrected Parts" package="R0402(M1005)" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="JP10" library="ADuCM350 Breakout Board Pins" package="2X03" value="RLDIN/RLDREF"/>
<element name="R9" library="Alex's Corrected Parts" package="R0402(M1005)" value="10kΩ (NP)">
<attribute name="NAME"/>
</element>
<element name="R10" library="Alex's Corrected Parts" package="R0402(M1005)" value="10kΩ (NP)">
<attribute name="NAME"/>
</element>
<element name="R11" library="Alex's Corrected Parts" package="R0402(M1005)" value="10kΩ (NP)">
<attribute name="NAME"/>
</element>
<element name="R12" library="Alex's Corrected Parts" package="R0402(M1005)" value="10kΩ (NP)">
<attribute name="NAME"/>
</element>
<element name="TP15" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP16" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP17" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP18" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="Alex's Corrected Parts" package="C0603(M1608)" value="4.7nF">
<attribute name="NAME"/>
</element>
<element name="C12" library="Alex's Corrected Parts" package="C0603(M1608)" value="4.7nF">
<attribute name="NAME"/>
</element>
<element name="TP19" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP20" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP21" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP22" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP23" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP24" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="C14" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="R8" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="R13" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="TP25" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="IN1N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="IN1P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="RLDOUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X6" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="IN2N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="IN2P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="IN3N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="Alex's Corrected Parts" package="U.FL-R-SMT-1" value="IN3P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="R14" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="R15" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="C16" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="R16" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="R17" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="C17" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="C18" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="TP26" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="Alex's Corrected Parts" package="C0603(M1608)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="Alex's Corrected Parts" package="R0603(M1608)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="Alex's Corrected Parts" package="R0402(M1005)" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="C20" library="Alex's Corrected Parts" package="C0402(M1005)" value="1.5nF">
<attribute name="NAME"/>
</element>
<element name="R20" library="Alex's Corrected Parts" package="R0603(M1608)" value=""/>
<element name="TP27" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP28" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP29" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP30" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP31" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="TP32" library="Alex's Corrected Parts" package="TP(C)-1.5" value=""/>
<element name="R21" library="Alex's Corrected Parts" package="R0402(M1005)" value="0Ω/NP">
<attribute name="NAME"/>
</element>
<element name="R22" library="Alex's Corrected Parts" package="R0402(M1005)" value="0Ω/NP">
<attribute name="NAME"/>
</element>
<element name="JP2" library="ADuCM350 Breakout Board Pins" package="1X04" value="ANALOG PWR (2.7-5.25V)"/>
<element name="JP4" library="ADuCM350 Breakout Board Pins" package="1X05" value="DIGITAL PWR (1.7-3.6V)"/>
<element name="R30" library="Alex's Corrected Parts" package="R0805(M2012)" value="0Ω/NP">
<attribute name="NAME"/>
</element>
<element name="R23" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="TP33" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP34" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="R24" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="C23" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="C24" library="Alex's Corrected Parts" package="C0603(M1608)" value="??pF">
<attribute name="NAME"/>
</element>
<element name="TP35" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP36" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP37" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP38" library="Alex's Corrected Parts" package="TP(C)-1.5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="R26" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="R27" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="R28" library="Alex's Corrected Parts" package="R0603(M1608)" value="??kΩ">
<attribute name="NAME"/>
</element>
<element name="C25" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="C26" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="C27" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="C28" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="C29" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="C30" library="Alex's Corrected Parts" package="C0603(M1608)" value="??nF">
<attribute name="NAME"/>
</element>
<element name="C1" library="Capacitors" package="C0402(M1005)" value="1uF"/>
<element name="JP8" library="Pins" package="2X03" value="RLDIN/RLDREF"/>
<element name="U$1" library="Logos" package="4MM-FILLED-SILK-IRL" value="IRL"/>
<element name="JP9" library="Pins" package="2X06" value="2X06">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Pins" package="2X02" value=""/>
<element name="JP5" library="Pins" package="2X02" value=""/>
</elements>
<signals>
<signal name="CLK">
<contactref element="IC1" pad="17"/>
<contactref element="TP7" pad="TP"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="!CS">
<contactref element="TP6" pad="TP"/>
<contactref element="IC1" pad="18"/>
<contactref element="R3" pad="1"/>
<contactref element="JP9" pad="9"/>
<contactref element="JP9" pad="10"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="19"/>
<contactref element="TP5" pad="TP"/>
<contactref element="JP9" pad="7"/>
<contactref element="JP9" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="20"/>
<contactref element="TP4" pad="TP"/>
<contactref element="JP9" pad="5"/>
<contactref element="JP9" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="21"/>
<contactref element="TP3" pad="TP"/>
<contactref element="JP9" pad="3"/>
<contactref element="JP9" pad="4"/>
</signal>
<signal name="START">
<contactref element="IC1" pad="16"/>
<contactref element="R2" pad="2"/>
<contactref element="TP9" pad="TP"/>
<contactref element="JP9" pad="11"/>
<contactref element="JP9" pad="12"/>
</signal>
<signal name="!PWDN!/!RESET!">
<contactref element="IC1" pad="15"/>
<contactref element="R1" pad="1"/>
<contactref element="TP13" pad="TP"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="CLKSEL">
<contactref element="IC1" pad="14"/>
<contactref element="TP14" pad="TP"/>
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="1"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="2"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="27"/>
<contactref element="TP12" pad="TP"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="C2" pad="-"/>
<contactref element="C10" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="C6" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="X5" pad="G2"/>
<contactref element="X4" pad="G1"/>
<contactref element="X5" pad="G1"/>
<contactref element="X4" pad="G2"/>
<contactref element="X1" pad="G2"/>
<contactref element="X1" pad="G1"/>
<contactref element="X2" pad="G2"/>
<contactref element="X2" pad="G1"/>
<contactref element="X3" pad="G2"/>
<contactref element="X3" pad="G1"/>
<contactref element="X6" pad="G2"/>
<contactref element="X6" pad="G1"/>
<contactref element="X7" pad="G2"/>
<contactref element="X7" pad="G1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C24" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="11"/>
<contactref element="C2" pad="+"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="DVDD">
<contactref element="C9" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="23"/>
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="AVDD">
<contactref element="C10" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="C6" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="DGND">
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="IC1" pad="24"/>
<contactref element="C5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP4" pad="4"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="9"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="!DRDY">
<contactref element="IC1" pad="22"/>
<contactref element="TP2" pad="TP"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="GPIO1">
<contactref element="IC1" pad="26"/>
<contactref element="TP11" pad="TP"/>
<contactref element="R4" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GPIO2">
<contactref element="IC1" pad="25"/>
<contactref element="TP10" pad="TP"/>
<contactref element="R5" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="IN3P">
<contactref element="IC1" pad="31"/>
<contactref element="R6" pad="1"/>
<contactref element="TP19" pad="TP"/>
<contactref element="R28" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C28" pad="1"/>
</signal>
<signal name="RLDIN/RLDREF">
<contactref element="IC1" pad="29"/>
<contactref element="JP10" pad="3"/>
<contactref element="TP30" pad="TP"/>
<contactref element="JP10" pad="5"/>
<contactref element="JP10" pad="2"/>
<contactref element="JP8" pad="3"/>
<contactref element="JP8" pad="5"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="RLDIN/RLDREF_EXT">
<contactref element="TP29" pad="TP"/>
<contactref element="JP10" pad="6"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="RLDINV">
<contactref element="IC1" pad="28"/>
<contactref element="R19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="TP31" pad="TP"/>
</signal>
<signal name="IN3N">
<contactref element="IC1" pad="32"/>
<contactref element="R7" pad="2"/>
<contactref element="TP20" pad="TP"/>
<contactref element="R27" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C28" pad="2"/>
</signal>
<signal name="IN1N">
<contactref element="IC1" pad="3"/>
<contactref element="TP23" pad="TP"/>
<contactref element="R10" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="IN1P">
<contactref element="IC1" pad="4"/>
<contactref element="TP24" pad="TP"/>
<contactref element="R9" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="C25" pad="2"/>
</signal>
<signal name="IN2N">
<contactref element="IC1" pad="5"/>
<contactref element="TP22" pad="TP"/>
<contactref element="R11" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="IN2P">
<contactref element="IC1" pad="6"/>
<contactref element="TP21" pad="TP"/>
<contactref element="R12" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="7"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="8"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="RARM">
<contactref element="X4" pad="SIG"/>
<contactref element="R13" pad="2"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="LARM">
<contactref element="R8" pad="2"/>
<contactref element="TP16" pad="TP"/>
<contactref element="X5" pad="SIG"/>
</signal>
<signal name="N$19">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="X6" pad="SIG"/>
<contactref element="TP17" pad="TP"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="X7" pad="SIG"/>
<contactref element="TP18" pad="TP"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="X2" pad="SIG"/>
<contactref element="R16" pad="2"/>
<contactref element="TP26" pad="TP"/>
</signal>
<signal name="RLEG">
<contactref element="X1" pad="SIG"/>
<contactref element="R18" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="TP27" pad="TP"/>
</signal>
<signal name="RLDOUT">
<contactref element="R18" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="TP28" pad="TP"/>
<contactref element="TP32" pad="TP"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R20" pad="2"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$20">
</signal>
<signal name="N$22">
<contactref element="X3" pad="SIG"/>
<contactref element="R17" pad="2"/>
<contactref element="TP25" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="C16" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="TP33" pad="TP"/>
</signal>
<signal name="N$21">
<contactref element="TP34" pad="TP"/>
<contactref element="C15" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="C13" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="TP36" pad="TP"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="C14" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="TP35" pad="TP"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="C17" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="TP38" pad="TP"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="C18" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="TP37" pad="TP"/>
<contactref element="R27" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
