(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 37)
    (zones 0)
    (modules 12)
    (nets 36)
  )
  (page A4)
  (title_block
    (date "lun. 30 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 110.998 126.365)
    (grid_origin 110.998 126.365)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /IOREF)
  (net 2 /Reset)
  (net 3 +5V)
  (net 4 GND)
  (net 5 /Vin)
  (net 6 /A0)
  (net 7 /A1)
  (net 8 /A2)
  (net 9 /A3)
  (net 10 /AREF)
  (net 11 "/9(**)")
  (net 12 /8)
  (net 13 /7)
  (net 14 "/6(**)")
  (net 15 "/5(**)")
  (net 16 /4)
  (net 17 "/3(**)")
  (net 18 /2)
  (net 19 "/1(Tx)")
  (net 20 "/0(Rx)")
  (net 21 "Net-(P5-Pad1)")
  (net 22 "Net-(P6-Pad1)")
  (net 23 "Net-(P7-Pad1)")
  (net 24 "Net-(P8-Pad1)")
  (net 25 "/13(SCK)")
  (net 26 "/10(**/SS)")
  (net 27 "Net-(P1-Pad1)")
  (net 28 +3V3)
  (net 29 "/12(MISO)")
  (net 30 "/11(**/MOSI)")
  (net 31 "Net-(J1-Pad8)")
  (net 32 "Net-(J1-Pad10)")
  (net 33 "Net-(J1-Pad2)")
  (net 34 /A5)
  (net 35 /A4)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/0(Rx)")
    (add_net "/1(Tx)")
    (add_net "/10(**/SS)")
    (add_net "/11(**/MOSI)")
    (add_net "/12(MISO)")
    (add_net "/13(SCK)")
    (add_net /2)
    (add_net "/3(**)")
    (add_net /4)
    (add_net "/5(**)")
    (add_net "/6(**)")
    (add_net /7)
    (add_net /8)
    (add_net "/9(**)")
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /IOREF)
    (add_net /Reset)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer F.Cu) (tedit 5C9B30E6)
    (at 157.353 114.935)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd custom (at -0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 5 /Vin)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 33 "Net-(J1-Pad2)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5C9B30E0)
    (at 149.733 114.935 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 1.9 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 33 "Net-(J1-Pad2)"))
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59DE0611)
    (at 165.608 104.14 180)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 1.27 -6.604 180) (layer F.SilkS))
    (fp_text value TLC (at 1.27 16.764 180) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "/13(SCK)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "/11(**/MOSI)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "/10(**/SS)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "/9(**)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "/3(**)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 552168D2)
    (at 138.938 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 8.89 -2.54) (layer F.SilkS))
    (fp_text value Power (at 8.89 -4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /IOREF))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Reset))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 +3V3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /Vin))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x06 locked (layer F.Cu) (tedit 552168D6)
    (at 161.798 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 6.604 -2.54) (layer F.SilkS))
    (fp_text value Analog (at 6.604 -4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /A4))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /A5))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x06.wrl
      (offset (xyz 6.349999904632568 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x10 locked (layer F.Cu) (tedit 552168BF)
    (at 129.794 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 11.43 2.794) (layer F.SilkS))
    (fp_text value Digital (at 11.43 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /A5))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /A4))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /AREF))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "/13(SCK)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "/12(MISO)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "/11(**/MOSI)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "/10(**/SS)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "/9(**)"))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /8))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x10.wrl
      (offset (xyz 11.42999982833862 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 552168C7)
    (at 156.718 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 8.89 2.794) (layer F.SilkS))
    (fp_text value Digital (at 8.89 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /7))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "/6(**)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "/5(**)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /4))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "/3(**)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /2))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "/1(Tx)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "/0(Rx)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC39)
    (at 124.968 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P5-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC4A)
    (at 177.038 118.745)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P6-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC2F)
    (at 126.238 75.565)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P7-Pad1)"))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5524FC41)
    (at 177.038 90.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P8-Pad1)"))
  )
  (module Symbol:OSHW-Logo_11.4x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 125.603 97.155)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text larsskj-002-01 (at 126.238 106.68) (layer F.SilkS))
  (gr_text 1 (at 138.938 121.285 90) (layer F.SilkS))
  (gr_line (start 177.038 74.549) (end 175.514 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 85.979) (end 177.038 74.549) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 88.519) (end 177.038 85.979) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 121.285) (end 179.578 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 123.825) (end 179.578 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 126.365) (end 177.038 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 126.365) (end 177.038 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 73.025) (end 110.998 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 73.025) (end 110.998 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.998 73.025) (xy 175.133 73.025) (xy 177.038 74.93) (xy 177.038 86.36) (xy 179.578 88.9)
        (xy 179.578 121.285) (xy 177.038 123.825) (xy 177.038 126.365) (xy 110.998 126.365)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.998 73.025) (xy 175.768 73.025) (xy 177.038 74.93) (xy 177.038 85.725) (xy 179.578 88.9)
        (xy 179.578 121.285) (xy 177.038 123.825) (xy 177.038 126.365) (xy 110.998 126.365) (xy 110.998 73.66)
      )
    )
  )
)
