(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 79)
    (no_connects 0)
    (area 136.8726 91.5286 173.355001 117.419067)
    (thickness 1.6)
    (drawings 9)
    (tracks 363)
    (zones 0)
    (modules 43)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 1.778)
    (pad_drill 1.5494)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C51-Pad1)")
  (net 4 "Net-(C121-Pad1)")
  (net 5 /RF_P)
  (net 6 "Net-(C122-Pad1)")
  (net 7 "Net-(C123-Pad1)")
  (net 8 "Net-(C124-Pad2)")
  (net 9 "Net-(C125-Pad1)")
  (net 10 /RF_N)
  (net 11 /SCLK)
  (net 12 /MISO)
  (net 13 /GDO2)
  (net 14 /GDO0)
  (net 15 /CSN)
  (net 16 "Net-(IC1-Pad17)")
  (net 17 /MOSI)
  (net 18 /CSN_CON)
  (net 19 /P1)
  (net 20 /P2)
  (net 21 /TX)
  (net 22 /RX)
  (net 23 /SCL)
  (net 24 /SDA)
  (net 25 /P3)
  (net 26 /P4)
  (net 27 /P5)
  (net 28 /P6)
  (net 29 /P7)
  (net 30 /P8)
  (net 31 /P9)
  (net 32 /P10)
  (net 33 "Net-(C81-Pad1)")
  (net 34 "Net-(C101-Pad1)")
  (net 35 "Net-(C127-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CSN)
    (add_net /CSN_CON)
    (add_net /GDO0)
    (add_net /GDO2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /P1)
    (add_net /P10)
    (add_net /P2)
    (add_net /P3)
    (add_net /P4)
    (add_net /P5)
    (add_net /P6)
    (add_net /P7)
    (add_net /P8)
    (add_net /P9)
    (add_net /RF_N)
    (add_net /RF_P)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SCLK)
    (add_net /SDA)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C121-Pad1)")
    (add_net "Net-(C122-Pad1)")
    (add_net "Net-(C123-Pad1)")
    (add_net "Net-(C124-Pad2)")
    (add_net "Net-(C125-Pad1)")
    (add_net "Net-(C127-Pad1)")
    (add_net "Net-(C51-Pad1)")
    (add_net "Net-(C81-Pad1)")
    (add_net "Net-(IC1-Pad17)")
    (add_net VDD)
  )
  (module ekoeppen_parts:M1x10_stackable (layer F.Cu) (tedit 586D4D22)
    (at 152.4 93.98)
    (fp_text reference P1 (at -11.36 0.23) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at -7.366 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at -12.7 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole circle (at -10.16 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -7.62 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 21 /TX))
    (pad 4 thru_hole circle (at -5.08 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 22 /RX))
    (pad 5 thru_hole circle (at -2.54 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 23 /SCL))
    (pad 6 thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 24 /SDA))
    (pad 7 thru_hole circle (at 2.54 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 /MISO))
    (pad 8 thru_hole circle (at 5.08 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 17 /MOSI))
    (pad 9 thru_hole circle (at 7.62 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 /SCLK))
    (pad 10 thru_hole circle (at 10.16 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 18 /CSN_CON))
  )
  (module ekoeppen_parts:M1x10_stackable (layer F.Cu) (tedit 586D4D65)
    (at 152.4 111.76)
    (fp_text reference P2 (at -11.43 0.254) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at -7.366 -1.524) (layer F.Fab))
    (pad 1 thru_hole circle (at -12.7 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 19 /P1))
    (pad 2 thru_hole circle (at -10.16 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 20 /P2))
    (pad 3 thru_hole circle (at -7.62 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 25 /P3))
    (pad 4 thru_hole circle (at -5.08 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 26 /P4))
    (pad 5 thru_hole circle (at -2.54 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 27 /P5))
    (pad 6 thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 28 /P6))
    (pad 7 thru_hole circle (at 2.54 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 29 /P7))
    (pad 8 thru_hole circle (at 5.08 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 30 /P8))
    (pad 9 thru_hole circle (at 7.62 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 31 /P9))
    (pad 10 thru_hole circle (at 10.16 2.54) (size 1.8 1.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 32 /P10))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D50F6)
    (at 144.78 99.06)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W1 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 /TX))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D50F2)
    (at 147.32 99.06)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W2 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 /RX))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D50ED)
    (at 149.86 99.06)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W3 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 /SCL))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D50EA)
    (at 152.4 99.06)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W4 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 /SDA))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DB6)
    (at 144.78 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W5 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 25 /P3))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DB9)
    (at 147.32 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W6 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 26 /P4))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DBC)
    (at 149.86 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W7 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 27 /P5))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DBF)
    (at 152.4 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W8 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 28 /P6))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DC2)
    (at 154.94 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W9 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 29 /P7))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DC5)
    (at 157.48 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W10 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 30 /P8))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DC8)
    (at 160.02 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W11 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 31 /P9))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 586D4DCC)
    (at 162.56 111.125)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference W12 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 32 /P10))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 161.8 98.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference J1 (at 0.5608 -1.3474 180) (layer B.SilkS))
    (fp_text value SOLDER_JUMPER (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 18 /CSN_CON))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 /CSN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 139.7 111.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference J2 (at 2.1086 1.1938 90) (layer B.SilkS))
    (fp_text value SOLDER_JUMPER (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 19 /P1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 14 /GDO0))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 142.2 111.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference J3 (at 2.134 1.31 90) (layer B.SilkS))
    (fp_text value SOLDER_JUMPER (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 20 /P2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 /GDO2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ekoeppen_parts:CRYSTAL_3225 (layer F.Cu) (tedit 5970308E)
    (at 144.91 109.9)
    (fp_text reference X1 (at 0.09 -3.1) (layer F.SilkS) hide)
    (fp_text value 26MHz (at 0.01 -4.4) (layer F.Fab))
    (pad 3 smd rect (at -1.1 -0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.1 -0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at -1.1 0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C81-Pad1)"))
    (pad 3 smd rect (at 1.1 0.8) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 140.5 105.3 270)
    (attr smd)
    (fp_text reference C41 (at -0.8044 1.5366 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 140.5 106.5 270)
    (attr smd)
    (fp_text reference C51 (at -0.1248 1.5874 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C51-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 141.5 111 270)
    (attr smd)
    (fp_text reference C81 (at 0.0488 1.6476 270) (layer F.SilkS))
    (fp_text value 15p (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C81-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 140.5 107.7 270)
    (attr smd)
    (fp_text reference C91 (at 0.4278 1.5874 270) (layer F.SilkS))
    (fp_text value 10n (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 148.1 110.1)
    (attr smd)
    (fp_text reference C101 (at 1.9378 -0.0926) (layer F.SilkS))
    (fp_text value 15p (at 0 0 90) (layer F.Fab))
    (fp_text user REF** (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C101-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 148.3 105.7 90)
    (attr smd)
    (fp_text reference C111 (at -1.6404 1.56 90) (layer F.SilkS))
    (fp_text value 220p (at 0 0 180) (layer F.Fab))
    (fp_text user REF** (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 152.654 105.4354 270)
    (attr smd)
    (fp_text reference C121 (at 1.1684 -1.524 360) (layer F.SilkS))
    (fp_text value 3p9 (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C121-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /RF_P) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 156.0068 102.3112 180)
    (attr smd)
    (fp_text reference C122 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 8p2 (at 0 0 270) (layer F.Fab))
    (fp_text user REF** (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C122-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 158.8516 102.2604 180)
    (attr smd)
    (fp_text reference C123 (at 0.0508 1.6256 180) (layer F.SilkS))
    (fp_text value 5p6 (at 0 0 270) (layer F.Fab))
    (fp_text user REF** (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C123-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 153.9494 108.1278 270)
    (attr smd)
    (fp_text reference C124 (at 1.2192 -0.5842 360) (layer F.SilkS))
    (fp_text value 220p (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C124-Pad2)") (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 160.951 104.2162 270)
    (attr smd)
    (fp_text reference C125 (at 1.2446 0.0928 360) (layer F.SilkS))
    (fp_text value 220p (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C125-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C123-Pad1)") (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 162.1282 102.362)
    (attr smd)
    (fp_text reference C126 (at -0.0762 -1.7272) (layer F.SilkS))
    (fp_text value 0 (at 0 0 90) (layer F.Fab))
    (fp_text user REF** (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C125-Pad1)") (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 163.3474 104.2162 270)
    (attr smd)
    (fp_text reference C127 (at 1.1938 0.0254 360) (layer F.SilkS))
    (fp_text value 0 (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C127-Pad1)") (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C125-Pad1)") (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 163.9316 102.362)
    (attr smd)
    (fp_text reference C128 (at 0.508 -1.7272) (layer F.SilkS))
    (fp_text value 0 (at 0 0 90) (layer F.Fab))
    (fp_text user REF** (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C127-Pad1)") (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 152.1206 102.3366 180)
    (attr smd)
    (fp_text reference C131 (at 0.0762 1.8034 180) (layer F.SilkS))
    (fp_text value 3p9 (at 0 0 270) (layer F.Fab))
    (fp_text user REF** (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 /RF_N) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 148.1836 103.7082 90)
    (attr smd)
    (fp_text reference C141 (at 0.0254 1.6764 90) (layer F.SilkS))
    (fp_text value 220p (at 0 0 180) (layer F.Fab))
    (fp_text user REF** (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 148.1836 102.5144 90)
    (attr smd)
    (fp_text reference C151 (at 1.4732 1.651 90) (layer F.SilkS))
    (fp_text value 10n (at 0 0 180) (layer F.Fab))
    (fp_text user REF** (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:CAPC1005X60N (layer F.Cu) (tedit 0)
    (at 143.7386 100.076 270)
    (attr smd)
    (fp_text reference C181 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value 220p (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.025))
    (pad 2 smd rect (at 0 0.5 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.025))
    (model CAPC1005X60N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:INDC1005X55N (layer F.Cu) (tedit 0)
    (at 152.0698 107.5436 180)
    (attr smd)
    (fp_text reference L121 (at 0.3556 -1.5748 180) (layer F.SilkS))
    (fp_text value 27n (at 0 0 270) (layer F.Fab))
    (fp_text user REF** (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.45 180) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C124-Pad2)") (solder_mask_margin 0.001))
    (pad 2 smd rect (at 0 0.45 180) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /RF_P) (solder_mask_margin 0.001))
    (model INDC1005X55N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:INDC1005X55N (layer F.Cu) (tedit 0)
    (at 155.448 104.2162 270)
    (attr smd)
    (fp_text reference L122 (at 1.143 -0.1524 360) (layer F.SilkS))
    (fp_text value 22n (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.45 270) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C122-Pad1)") (solder_mask_margin 0.001))
    (pad 2 smd rect (at 0 0.45 270) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C121-Pad1)") (solder_mask_margin 0.001))
    (model INDC1005X55N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:INDC1005X55N (layer F.Cu) (tedit 0)
    (at 158.3182 104.2162 270)
    (attr smd)
    (fp_text reference L123 (at 1.2192 0 360) (layer F.SilkS))
    (fp_text value 27n (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.45 270) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C123-Pad1)") (solder_mask_margin 0.001))
    (pad 2 smd rect (at 0 0.45 270) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C122-Pad1)") (solder_mask_margin 0.001))
    (model INDC1005X55N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:INDC1005X55N (layer F.Cu) (tedit 0)
    (at 152.654 104.2162 270)
    (attr smd)
    (fp_text reference L131 (at -0.0254 1.6256 450) (layer F.SilkS))
    (fp_text value 27n (at 0 0 360) (layer F.Fab))
    (fp_text user REF** (at 0 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.45 270) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C121-Pad1)") (solder_mask_margin 0.001))
    (pad 2 smd rect (at 0 0.45 270) (size 0.75 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /RF_N) (solder_mask_margin 0.001))
    (model INDC1005X55N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_0402:RESC1005X40N (layer F.Cu) (tedit 0)
    (at 145.8468 100.1014 90)
    (attr smd)
    (fp_text reference R171 (at 0.1016 1.4986 90) (layer F.SilkS))
    (fp_text value 56k (at 0 0 180) (layer F.Fab))
    (fp_text user REF** (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.45 90) (size 0.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad17)") (solder_mask_margin 0.05))
    (pad 2 smd rect (at 0 0.45 90) (size 0.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.05))
    (model RESC1005X40N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ekoeppen_parts:QLP20 (layer F.Cu) (tedit 59703073)
    (at 144.275 104.505)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference IC1 (at -3.3812 -1.6096) (layer F.SilkS) hide)
    (fp_text value CC1101 (at -0.025 -4.635) (layer F.SilkS))
    (pad 21 smd rect (at 0 0) (size 2.4 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.02))
    (pad 1 smd rect (at -1.78 -1) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCLK) (solder_mask_margin 0.02))
    (pad 2 smd rect (at -1.78 -0.5) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO) (solder_mask_margin 0.02))
    (pad 3 smd rect (at -1.78 0) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 /GDO2) (solder_mask_margin 0.02))
    (pad 4 smd rect (at -1.78 0.5) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.02))
    (pad 5 smd rect (at -1.78 1) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C51-Pad1)") (solder_mask_margin 0.02))
    (pad 6 smd rect (at -1 1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 14 /GDO0) (solder_mask_margin 0.02))
    (pad 7 smd rect (at -0.5 1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 15 /CSN) (solder_mask_margin 0.02))
    (pad 8 smd rect (at 0 1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C81-Pad1)") (solder_mask_margin 0.02))
    (pad 9 smd rect (at 0.5 1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.02))
    (pad 10 smd rect (at 1 1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C101-Pad1)") (solder_mask_margin 0.02))
    (pad 11 smd rect (at 1.78 1) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.02))
    (pad 12 smd rect (at 1.78 0.5) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 /RF_P) (solder_mask_margin 0.02))
    (pad 13 smd rect (at 1.78 0) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 10 /RF_N) (solder_mask_margin 0.02))
    (pad 14 smd rect (at 1.78 -0.5) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.02))
    (pad 15 smd rect (at 1.78 -1) (size 0.76 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.02))
    (pad 16 smd rect (at 1 -1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.02))
    (pad 17 smd rect (at 0.5 -1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad17)") (solder_mask_margin 0.02))
    (pad 18 smd rect (at 0 -1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD) (solder_mask_margin 0.02))
    (pad 19 smd rect (at -0.5 -1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.02))
    (pad 20 smd rect (at -1 -1.78) (size 0.28 0.76) (layers F.Cu F.Paste F.Mask)
      (net 17 /MOSI) (solder_mask_margin 0.02))
  )
  (module ekoeppen_parts:SMA_PTH (layer F.Cu) (tedit 586D1006)
    (at 169.0718 104.3432)
    (fp_text reference P3 (at 0.13 -2) (layer F.SilkS))
    (fp_text value SMA (at 0 -3.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask)
      (net 35 "Net-(C127-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.778 1.778) (drill 1.5494) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text 20170719 (at 166.59 109.04) (layer B.SilkS))
  (gr_arc (start 171.45 114.3) (end 173.228 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171.45 96.52) (end 171.45 94.742) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.7 114.3) (end 139.7 116.078) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.7 96.52) (end 137.922 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 116.078) (end 139.7 116.078) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.228 96.52) (end 173.228 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 94.742) (end 171.45 94.742) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.922 114.3) (end 137.922 96.52) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 137.9982 94.7674) (xy 173.355 94.7674) (xy 173.228 116.1034) (xy 137.9982 116.0526)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 137.97 94.78) (xy 173.3 94.82) (xy 173.21 116.12) (xy 137.99 116.05)
      )
    )
  )
)
