(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 86)
    (tracks 171)
    (zones 0)
    (modules 37)
    (nets 32)
  )
  (page USLetter)
  (title_block
    (title "Sidewinder HUD v3.1 (ATTiny)")
    (date 2023-06-02)
    (rev A)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 86.28 120.13)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/Users/andrewpitkin/Library/Mobile Documents/com~apple~CloudDocs/Documents/SeeedStudio/Sidewinder HUD v1_0/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 /S0)
  (net 4 /S1)
  (net 5 /S2)
  (net 6 /S3)
  (net 7 "Net-(J4-Pad1)")
  (net 8 "Net-(J6-Pad1)")
  (net 9 "Net-(J7-Pad1)")
  (net 10 "Net-(J8-Pad1)")
  (net 11 "Net-(J10-Pad1)")
  (net 12 "Net-(J11-Pad1)")
  (net 13 "Net-(J12-Pad1)")
  (net 14 "Net-(J13-Pad1)")
  (net 15 "Net-(J14-Pad1)")
  (net 16 "Net-(J16-Pad1)")
  (net 17 "Net-(J17-Pad1)")
  (net 18 "Net-(J18-Pad1)")
  (net 19 "Net-(J19-Pad1)")
  (net 20 "Net-(R1-Pad1)")
  (net 21 "Net-(R2-Pad1)")
  (net 22 "Net-(R3-Pad1)")
  (net 23 "Net-(R10-Pad2)")
  (net 24 "Net-(R11-Pad2)")
  (net 25 "Net-(R12-Pad2)")
  (net 26 "Net-(R13-Pad2)")
  (net 27 "Net-(U1-Pad8)")
  (net 28 "Net-(U1-Pad12)")
  (net 29 "Net-(U1-Pad13)")
  (net 30 "Net-(U1-Pad14)")
  (net 31 "Net-(U1-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /S0)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J19-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad8)")
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm locked (layer F.Cu) (tedit 5A0F774F)
    (at 109.1 127.61)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J5 (at 0 -2.398) (layer F.SilkS) hide)
    (fp_text value B- (at 0 2.55) (layer F.SilkS))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm locked (layer F.Cu) (tedit 5A0F774F)
    (at 109.1 108.71)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.398) (layer F.SilkS) hide)
    (fp_text value B+ (at -0.22 -2.78) (layer F.SilkS))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
  )
  (module ADP_CustomFootprints:SSOP-20_5.3x7.2mm_P0.65mm_edited (layer F.Cu) (tedit 62E71691)
    (at 109.96 118.14)
    (descr "SSOP, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001800C.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (attr smd)
    (fp_text reference U1 (at 0 -4.55) (layer F.SilkS))
    (fp_text value ATTiny3226-X (at 0 4.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.5 -2.925) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at -3.5 -2.275) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R11-Pad2)"))
    (pad 3 smd roundrect (at -3.5 -1.625) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J11-Pad1)"))
    (pad 4 smd roundrect (at -3.5 -0.975) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R1-Pad1)"))
    (pad 5 smd roundrect (at -3.5 -0.325) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(R2-Pad1)"))
    (pad 6 smd roundrect (at -3.5 0.325) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R3-Pad1)"))
    (pad 7 smd roundrect (at -3.5 0.975) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R10-Pad2)"))
    (pad 8 smd roundrect (at -3.5 1.625) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad8)"))
    (pad 9 smd roundrect (at -3.5 2.275) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R13-Pad2)"))
    (pad 10 smd roundrect (at -3.5 2.925) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J18-Pad1)"))
    (pad 11 smd roundrect (at 3.5 2.925) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R12-Pad2)"))
    (pad 12 smd roundrect (at 3.5 2.275) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(U1-Pad12)"))
    (pad 13 smd roundrect (at 3.5 1.625) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(U1-Pad13)"))
    (pad 14 smd roundrect (at 3.5 0.975) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(U1-Pad14)"))
    (pad 15 smd roundrect (at 3.5 0.325) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J16-Pad1)"))
    (pad 16 smd roundrect (at 3.5 -0.325) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(J10-Pad1)"))
    (pad 17 smd roundrect (at 3.5 -0.975) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(U1-Pad17)"))
    (pad 18 smd roundrect (at 3.5 -1.625) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(J14-Pad1)"))
    (pad 19 smd roundrect (at 3.5 -2.275) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J13-Pad1)"))
    (pad 20 smd roundrect (at 3.5 -2.925) (size 1.9 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-20_5.3x7.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 87.48 134.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.98 135.03)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 1.2 1.6) (layer F.SilkS))
    (fp_text value 680 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(J19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 99.98 138.03)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 2.2 1.6) (layer F.SilkS))
    (fp_text value 680 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(J17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.98 132.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 3.2 0) (layer F.SilkS))
    (fp_text value 680 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.88 130.03)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 3.1 0.1) (layer F.SilkS))
    (fp_text value "100k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.08 120.43)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "100k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R3-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.08 109.73 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.5 -0.1) (layer F.SilkS))
    (fp_text value "100k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(R2-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.58 98.63 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "10k 1%" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /S3))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 89.58 98.73 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "10k 1%" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /S2))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 94.58 98.83 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "10k 1%" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /S1))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.88 126.93 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0.3 1.4) (layer F.SilkS))
    (fp_text value "4.7k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /S3))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.08 117.33 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.4) (layer F.SilkS))
    (fp_text value "4.7k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /S2))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.08 112.73 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.5 0) (layer F.SilkS))
    (fp_text value "4.7k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /S1))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 101.08 106.63 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.5 -0.1) (layer F.SilkS))
    (fp_text value "4.7k 1%" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /S0))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 113.58 108.83)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value Si2333 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 93 141.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J19 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 3 (at 2.1 0.6) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J19-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 98 141.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J18 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 4 (at 2.2 0.6) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J18-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 95.25 137.9)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J17 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 5 (at 1.8 -2) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J17-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 85.5 137.9)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J16 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 7 (at 1 -2) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J16-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 114.38 129.26)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J15 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value SW- (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 114.38 124.91)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J14 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value SW+ (at -2.8 -1.48) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J14-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 90.5 137.9)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J13 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 6 (at 1.3 -2.1) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J13-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 83 141.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J12 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 1 (at 2.2 0.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J12-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 88 141.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J11 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value 2 (at 2.2 0.5) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J11-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 112.45 133.48)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J10 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Prg (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 99.6 93.13)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J9 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value A0 (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /S0))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 84.6 93.13)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value A3 (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J8-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 89.6 93.13)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J7 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value A2 (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J7-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 94.6 93.13)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J6 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value A1 (at 0 2.05) (layer F.SilkS))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J6-Pad1)"))
  )
  (module ADP_CustomFootprints:SMB_Vertical_Elevated (layer F.Cu) (tedit 63DAD88A)
    (at 94.58 130.23 90)
    (descr "SMB mounted elevated on PCB")
    (tags "SMB elevated")
    (fp_text reference J3 (at 0 -4.85 90) (layer F.SilkS) hide)
    (fp_text value S3 (at 4.4 -0.1 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.24 2.24) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /S3))
    (model "${KISYS3DMOD}/ADP_Custom.3dshapes/SMB straight THT.stp"
      (offset (xyz 0 0 -1.72))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module ADP_CustomFootprints:SMB_Vertical_Elevated (layer F.Cu) (tedit 63DAD88A)
    (at 94.58 120.13 90)
    (descr "SMB mounted elevated on PCB")
    (tags "SMB elevated")
    (fp_text reference J2 (at 0 -4.85 90) (layer F.SilkS) hide)
    (fp_text value S2 (at 4.4 0.1 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.24 2.24) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /S2))
    (model "${KISYS3DMOD}/ADP_Custom.3dshapes/SMB straight THT.stp"
      (offset (xyz 0 0 -1.72))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module ADP_CustomFootprints:SMB_Vertical_Elevated (layer F.Cu) (tedit 63DAD88A)
    (at 94.58 110.03 90)
    (descr "SMB mounted elevated on PCB")
    (tags "SMB elevated")
    (fp_text reference J1 (at 0 -4.85 90) (layer F.SilkS) hide)
    (fp_text value S1 (at 4.4 -0.1 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.74 2.74) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /S0))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.24 2.24) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /S1))
    (model "${KISYS3DMOD}/ADP_Custom.3dshapes/SMB straight THT.stp"
      (offset (xyz 0 0 -1.72))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module "Artwork:Fathom logo" (layer F.Cu) (tedit 0)
    (at 100.73 100.15)
    (fp_text reference G1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FathomDiveSystemsLogo (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 106.68 113.23)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "100n 6.3V" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Sidewinder head\nHUD Rev A 060323" (at 90.17 102.88) (layer F.SilkS))
  (gr_arc (start 112.4099 146.028239) (end 112.421346 137.278726) (angle -59.97388763) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 102.68 140.3) (end 102.68 142.84) (angle -58.1857613) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.600599 142.839315) (end 102.68 142.84) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 112.39982 133.278226) (end 112.421346 137.278726) (angle -89.67715318) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.400378 133.279242) (end 116.400378 120) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 82.600599 140.299315) (end 80.060599 140.299315) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.060599 139.188428) (end 80.060599 140.299315) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 70.393359 120) (end 89.951357 120) (angle -54.53808168) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 112.4 93.957258) (end 103.637 93.957258) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.637 93.957258) (end 103.637 93.83) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.060599 100.811572) (end 80.060599 93.83) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 84.061099 139.188428) (end 81.740162 135.930016) (angle -54.53808168) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 70.393359 120) (end 81.740162 135.930016) (angle -54.53808168) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 84.061099 100.811572) (end 80.060599 100.811572) (angle -54.53808168) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 112.399878 106.720758) (end 116.400378 106.720758) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.400378 106.720758) (end 116.400378 120) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 82.600599 93.83) (end 82.600599 91.29) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 101.097 93.83) (end 103.637 93.83) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.600599 91.29) (end 101.097 91.29) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.4 102.720258) (end 112.399878 102.720258) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.28 143.13) (xy 79.28 143.13) (xy 79.28 90.13) (xy 117.28 90.13)
      )
    )
  )
)
