(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5")
	(title_block
		(date "2025-09-04")
		(rev "1.1")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "manufacturing/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "/POW_B")
	(net 3 "/5V")
	(net 4 "/POW_A")
	(net 5 "Net-(D2-K)")
	(net 6 "/12V")
	(net 7 "Net-(C1-Pad2)")
	(footprint "asl_footprints:1206_reverse_smd"
		(layer "F.Cu")
		(at 105.85 57.42502)
		(property "Reference" "D1"
			(at 0.00482 -1.80482 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0.635 -1.905 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP655R-IW-2897/9650105?s=N4IgTCBcDaIIwFY4DYC0cDMyAcIC6AvkA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 2.3 2.3)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -1.625 0 90)
			(size 1.7 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/POW_A")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.625 0 90)
			(size 1.7 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/3d/reverse_LED.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 109.6 72.4 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -3.25 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "120Ω"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/vishay-dale/CRCW1206120RFKEAHP/2227652"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 104.55 76.5 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -0.05 1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-6AEB101V/1465724"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 2 "/POW_B")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "asl_footprints:D_SOD-123F"
		(layer "F.Cu")
		(at 105.85 73.5202 180)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D2"
			(at 3 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819HW-7-F"
			(at 0 2.1 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/diodes-incorporated/1N5819HW-7-F/815283"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.127 -1.905 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.4 0 180)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/POW_B")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "asl_footprints:vibration_motor_12k_smd"
		(layer "F.Cu")
		(at 105.85 65.325 -90)
		(property "Reference" "M1"
			(at -2.5 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "VZ43FM1B8230001L"
			(at 0.3952 3.387 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/vybronics-inc/VZ43FM1B8230001L/12323592"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*P2.54mm* TerminalBlock*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd)
		(fp_rect
			(start -5.08 -1.524)
			(end -0.90424 1.524)
			(fill no)
			(layer "Edge.Cuts")
		)
		(pad "1" smd rect
			(at 5.55 -1.65 90)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D2-K)")
			(pinfunction "+")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 5.55 1.65 90)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/POW_B")
			(pinfunction "-")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -0.325 -0.85)
			(size 1 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -0.325 0.85)
			(size 1 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 2.15 0 270)
			(size 4.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 5.05 0 90)
			(size 1.5 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/3d/VZ43FM1B8230001L.stp"
			(offset
				(xyz 5.85 0 1.9)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 112.8 72.4 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 1.95 90)
			(layer "F.SilkS")
		)
		(property "Value" "120Ω"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/vishay-dale/CRCW1206120RFKEAHP/2227652"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 3 "/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 1 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 107.1 76.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/kemet/C0805C104K5RACTU/411169"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "asl_footprints:board_to_board_joint_4"
		(layer "B.Cu")
		(at 105.85 76.92046)
		(property "Reference" "J1"
			(at 3 -1.006 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -2.54 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "top.kicad_sch")
		(attr smd exclude_from_bom)
		(pad "1" smd rect
			(at -4.7625 1.373)
			(size 1.905 2.7432)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "/POW_B")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.5875 1.373)
			(size 1.905 2.7432)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "/12V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.5875 1.373)
			(size 1.905 2.7432)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/POW_A")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 4.7625 1.373)
			(size 1.905 2.7432)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "/5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 92.684009 70.488373)
		(end 99.85 79.9202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.983949 55.76329)
		(end 113.537613 65.542234)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.716051 55.76329)
		(mid 100.054404 55.159662)
		(end 100.703664 54.9202)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.537613 65.542234)
		(mid 113.546897 65.620445)
		(end 113.55 65.699144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.703664 54.9202)
		(end 110.996336 54.9202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113.55 67.9202)
		(end 113.55 65.699144)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 110.996336 54.9202)
		(mid 111.645581 55.159651)
		(end 111.983949 55.76329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.15 67.9202)
		(end 116.15 66.6202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.55 65.6202)
		(end 93.48026 65.6202)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.15 66.6202)
		(mid 116.442893 65.913093)
		(end 117.15 65.6202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.15 67.9202)
		(end 98.15 65.699144)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 94.55 65.6202)
		(mid 95.257107 65.913093)
		(end 95.55 66.6202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.162387 65.542234)
		(end 99.716051 55.76329)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.48026 66.6202)
		(mid 92.773157 65.913114)
		(end 93.48026 65.6202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.48026 66.6202)
		(end 92.48026 69.883407)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.21974 65.6202)
		(end 117.15 65.6202)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.15 67.9202)
		(mid 96.85 69.2202)
		(end 95.55 67.9202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.85 79.9202)
		(end 111.85 79.9202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.21974 66.6202)
		(end 119.21974 69.883407)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.21974 69.883407)
		(mid 119.167435 70.202585)
		(end 119.015991 70.488373)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.15 65.699144)
		(mid 98.153105 65.620445)
		(end 98.162387 65.542234)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.55 67.9202)
		(end 95.55 66.6202)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.21974 65.6202)
		(mid 118.926821 65.913107)
		(end 119.21974 66.6202)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.015991 70.488373)
		(end 111.85 79.9202)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.15 67.9202)
		(mid 114.85 69.2202)
		(end 113.55 67.9202)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.684009 70.488373)
		(mid 92.532569 70.202584)
		(end 92.48026 69.883407)
		(layer "Edge.Cuts")
	)
	(gr_text "PA"
		(at 107.55 79.8202 -0)
		(layer "F.SilkS")
	)
	(gr_text "Sep 2025"
		(at 99.65 65.1202 270)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 108.05 56.7202 -90)
		(layer "F.SilkS")
	)
	(gr_text "v${REVISION}"
		(at 112.25 65.1202 270)
		(layer "F.SilkS")
	)
	(gr_text "PB"
		(at 101.05 79.8202 -0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 102.35 58.0202 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 110.65 79.7202 -0)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 104.25 79.8202 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 110.5 76.5 0)
		(layer "B.SilkS")
	)
	(gr_text "12V"
		(at 104.2 76.4 0)
		(layer "B.SilkS")
	)
	(gr_text "PA"
		(at 107.4 76.4 0)
		(layer "B.SilkS")
	)
	(gr_text "PB"
		(at 101 76.5 0)
		(layer "B.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 92.48026 69.883407) (xy 119.21974 69.8834)
		)
		(height 12.916593)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 1)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "26.7 mm"
			(at 105.85 82.8 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Cmts.User")
		(pts
			(xy 100.703664 54.92025) (xy 99.85 79.9202)
		)
		(height -10.303664)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 1)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "25.0 mm"
			(at 90.4 67.420225 90)
			(layer "Cmts.User")
		)
	)
	(embedded_fonts no)
)
