(kicad_pcb (version 4) (host pcbnew 4.0.2-2.fc24-product)
  (general
    (links 316)
    (no_connects 0)
    (area 163.244999 112.744999 257.255001 144.755001)
    (thickness 1.6)
    (drawings 122)
    (tracks 919)
    (zones 0)
    (modules 147)
    (nets 136)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3.3)
    (pad_to_mask_clearance 0.15)
    (solder_mask_min_width 0.15)
    (aux_axis_origin 0 0)
    (grid_origin 244.25 123.75)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 "Net-(D5-Pad2)")
  (net 7 "Net-(D6-Pad2)")
  (net 8 "Net-(D7-Pad2)")
  (net 9 "Net-(D8-Pad2)")
  (net 10 "Net-(D9-Pad2)")
  (net 11 "Net-(D10-Pad2)")
  (net 12 "Net-(D11-Pad2)")
  (net 13 "Net-(D12-Pad2)")
  (net 14 "Net-(D13-Pad2)")
  (net 15 "Net-(D14-Pad2)")
  (net 16 "Net-(D15-Pad2)")
  (net 17 "Net-(D16-Pad2)")
  (net 18 "Net-(D17-Pad2)")
  (net 19 "Net-(D18-Pad2)")
  (net 20 "Net-(D19-Pad2)")
  (net 21 "Net-(D20-Pad2)")
  (net 22 "Net-(D21-Pad2)")
  (net 23 "Net-(D22-Pad2)")
  (net 24 "Net-(D23-Pad2)")
  (net 25 "Net-(D24-Pad2)")
  (net 26 "Net-(D25-Pad2)")
  (net 27 "Net-(D26-Pad2)")
  (net 28 "Net-(D27-Pad2)")
  (net 29 "Net-(D28-Pad2)")
  (net 30 "Net-(D29-Pad2)")
  (net 31 "Net-(D30-Pad2)")
  (net 32 "Net-(D31-Pad2)")
  (net 33 "Net-(D32-Pad2)")
  (net 34 "Net-(D33-Pad2)")
  (net 35 "Net-(D34-Pad2)")
  (net 36 "Net-(D35-Pad2)")
  (net 37 "Net-(D36-Pad2)")
  (net 38 "Net-(D37-Pad2)")
  (net 39 "Net-(D38-Pad2)")
  (net 40 "Net-(D39-Pad2)")
  (net 41 "Net-(D40-Pad2)")
  (net 42 "Net-(D41-Pad2)")
  (net 43 "Net-(D42-Pad2)")
  (net 44 "Net-(D43-Pad2)")
  (net 45 "Net-(D44-Pad2)")
  (net 46 "Net-(D45-Pad2)")
  (net 47 "Net-(D46-Pad2)")
  (net 48 "Net-(D47-Pad2)")
  (net 49 "Net-(D48-Pad2)")
  (net 50 "Net-(D49-Pad2)")
  (net 51 "Net-(D50-Pad2)")
  (net 52 "Net-(D51-Pad2)")
  (net 53 "Net-(D52-Pad2)")
  (net 54 "Net-(D53-Pad2)")
  (net 55 "Net-(D54-Pad2)")
  (net 56 "Net-(D55-Pad2)")
  (net 57 "Net-(D56-Pad2)")
  (net 58 "Net-(D57-Pad2)")
  (net 59 "Net-(D58-Pad2)")
  (net 60 "Net-(D59-Pad2)")
  (net 61 "Net-(D60-Pad2)")
  (net 62 "Net-(D61-Pad2)")
  (net 63 "Net-(D62-Pad2)")
  (net 64 "Net-(D63-Pad2)")
  (net 65 "Net-(D64-Pad2)")
  (net 66 VCC)
  (net 67 /D0-D7/CLK)
  (net 68 /D0-D7/LE)
  (net 69 /D0-D7/SIN)
  (net 70 /MISO)
  (net 71 /D24-D31/SOUT)
  (net 72 /D0-D7/Q0)
  (net 73 /D0-D7/Q1)
  (net 74 /D0-D7/Q2)
  (net 75 /D0-D7/Q3)
  (net 76 /D0-D7/Q4)
  (net 77 /D0-D7/Q5)
  (net 78 /D0-D7/Q6)
  (net 79 /D8-D15/SIN)
  (net 80 /D0-D7/Q0L)
  (net 81 /D8-D15/Q0)
  (net 82 /D8-D15/Q1)
  (net 83 /D8-D15/Q2)
  (net 84 /D8-D15/Q3)
  (net 85 /D8-D15/Q4)
  (net 86 /D8-D15/Q5)
  (net 87 /D8-D15/Q6)
  (net 88 /D16-D23/SIN)
  (net 89 /D8-D15/Q0L)
  (net 90 /D16-D23/Q0)
  (net 91 /D16-D23/Q1)
  (net 92 /D16-D23/Q2)
  (net 93 /D16-D23/Q3)
  (net 94 /D16-D23/Q4)
  (net 95 /D16-D23/Q5)
  (net 96 /D16-D23/Q6)
  (net 97 /D24-D31/SIN)
  (net 98 /D16-D23/Q0L)
  (net 99 /D24-D31/Q0)
  (net 100 /D24-D31/Q1)
  (net 101 /D24-D31/Q2)
  (net 102 /D24-D31/Q3)
  (net 103 /D24-D31/Q4)
  (net 104 /D24-D31/Q5)
  (net 105 /D24-D31/Q6)
  (net 106 /D24-D31/Q0L)
  (net 107 /D0-D7/Q1L)
  (net 108 /D0-D7/Q2L)
  (net 109 /D0-D7/Q3L)
  (net 110 /D0-D7/Q4L)
  (net 111 /D0-D7/Q5L)
  (net 112 /D0-D7/Q6L)
  (net 113 /D0-D7/Q7L)
  (net 114 /D8-D15/Q1L)
  (net 115 /D8-D15/Q2L)
  (net 116 /D8-D15/Q3L)
  (net 117 /D8-D15/Q4L)
  (net 118 /D8-D15/Q5L)
  (net 119 /D8-D15/Q6L)
  (net 120 /D8-D15/Q7L)
  (net 121 /D16-D23/Q1L)
  (net 122 /D16-D23/Q2L)
  (net 123 /D16-D23/Q3L)
  (net 124 /D16-D23/Q4L)
  (net 125 /D16-D23/Q5L)
  (net 126 /D16-D23/Q6L)
  (net 127 /D16-D23/Q7L)
  (net 128 /D24-D31/Q1L)
  (net 129 /D24-D31/Q2L)
  (net 130 /D24-D31/Q3L)
  (net 131 /D24-D31/Q4L)
  (net 132 /D24-D31/Q5L)
  (net 133 /D24-D31/Q6L)
  (net 134 /D24-D31/Q7L)
  (net 135 /SIN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D0-D7/CLK)
    (add_net /D0-D7/LE)
    (add_net /D0-D7/Q0)
    (add_net /D0-D7/Q0L)
    (add_net /D0-D7/Q1)
    (add_net /D0-D7/Q1L)
    (add_net /D0-D7/Q2)
    (add_net /D0-D7/Q2L)
    (add_net /D0-D7/Q3)
    (add_net /D0-D7/Q3L)
    (add_net /D0-D7/Q4)
    (add_net /D0-D7/Q4L)
    (add_net /D0-D7/Q5)
    (add_net /D0-D7/Q5L)
    (add_net /D0-D7/Q6)
    (add_net /D0-D7/Q6L)
    (add_net /D0-D7/Q7L)
    (add_net /D0-D7/SIN)
    (add_net /D16-D23/Q0)
    (add_net /D16-D23/Q0L)
    (add_net /D16-D23/Q1)
    (add_net /D16-D23/Q1L)
    (add_net /D16-D23/Q2)
    (add_net /D16-D23/Q2L)
    (add_net /D16-D23/Q3)
    (add_net /D16-D23/Q3L)
    (add_net /D16-D23/Q4)
    (add_net /D16-D23/Q4L)
    (add_net /D16-D23/Q5)
    (add_net /D16-D23/Q5L)
    (add_net /D16-D23/Q6)
    (add_net /D16-D23/Q6L)
    (add_net /D16-D23/Q7L)
    (add_net /D16-D23/SIN)
    (add_net /D24-D31/Q0)
    (add_net /D24-D31/Q0L)
    (add_net /D24-D31/Q1)
    (add_net /D24-D31/Q1L)
    (add_net /D24-D31/Q2)
    (add_net /D24-D31/Q2L)
    (add_net /D24-D31/Q3)
    (add_net /D24-D31/Q3L)
    (add_net /D24-D31/Q4)
    (add_net /D24-D31/Q4L)
    (add_net /D24-D31/Q5)
    (add_net /D24-D31/Q5L)
    (add_net /D24-D31/Q6)
    (add_net /D24-D31/Q6L)
    (add_net /D24-D31/Q7L)
    (add_net /D24-D31/SIN)
    (add_net /D24-D31/SOUT)
    (add_net /D8-D15/Q0)
    (add_net /D8-D15/Q0L)
    (add_net /D8-D15/Q1)
    (add_net /D8-D15/Q1L)
    (add_net /D8-D15/Q2)
    (add_net /D8-D15/Q2L)
    (add_net /D8-D15/Q3)
    (add_net /D8-D15/Q3L)
    (add_net /D8-D15/Q4)
    (add_net /D8-D15/Q4L)
    (add_net /D8-D15/Q5)
    (add_net /D8-D15/Q5L)
    (add_net /D8-D15/Q6)
    (add_net /D8-D15/Q6L)
    (add_net /D8-D15/Q7L)
    (add_net /D8-D15/SIN)
    (add_net /MISO)
    (add_net /SIN)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad2)")
    (add_net "Net-(D24-Pad2)")
    (add_net "Net-(D25-Pad2)")
    (add_net "Net-(D26-Pad2)")
    (add_net "Net-(D27-Pad2)")
    (add_net "Net-(D28-Pad2)")
    (add_net "Net-(D29-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D30-Pad2)")
    (add_net "Net-(D31-Pad2)")
    (add_net "Net-(D32-Pad2)")
    (add_net "Net-(D33-Pad2)")
    (add_net "Net-(D34-Pad2)")
    (add_net "Net-(D35-Pad2)")
    (add_net "Net-(D36-Pad2)")
    (add_net "Net-(D37-Pad2)")
    (add_net "Net-(D38-Pad2)")
    (add_net "Net-(D39-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D40-Pad2)")
    (add_net "Net-(D41-Pad2)")
    (add_net "Net-(D42-Pad2)")
    (add_net "Net-(D43-Pad2)")
    (add_net "Net-(D44-Pad2)")
    (add_net "Net-(D45-Pad2)")
    (add_net "Net-(D46-Pad2)")
    (add_net "Net-(D47-Pad2)")
    (add_net "Net-(D48-Pad2)")
    (add_net "Net-(D49-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D50-Pad2)")
    (add_net "Net-(D51-Pad2)")
    (add_net "Net-(D52-Pad2)")
    (add_net "Net-(D53-Pad2)")
    (add_net "Net-(D54-Pad2)")
    (add_net "Net-(D55-Pad2)")
    (add_net "Net-(D56-Pad2)")
    (add_net "Net-(D57-Pad2)")
    (add_net "Net-(D58-Pad2)")
    (add_net "Net-(D59-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D60-Pad2)")
    (add_net "Net-(D61-Pad2)")
    (add_net "Net-(D62-Pad2)")
    (add_net "Net-(D63-Pad2)")
    (add_net "Net-(D64-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net VCC)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer B.Cu) (tedit 555EF99E)
    (at 190.25 119.75 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C1 (at -0.20066 3.29946 90) (layer B.SilkS))
    (fp_text value CP_Small (at -0.09906 -3.59918 90) (layer B.Fab))
    (pad 2 smd rect (at 3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer B.Cu) (tedit 555EF99E)
    (at 222.25 119.75 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C3 (at -0.20066 3.29946 90) (layer B.SilkS))
    (fp_text value CP_Small (at -0.09906 -3.59918 90) (layer B.Fab))
    (pad 2 smd rect (at 3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer B.Cu) (tedit 555EF99E)
    (at 238.25 119.75 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C4 (at -5 0 180) (layer B.SilkS))
    (fp_text value CP_Small (at -0.09906 -3.59918 90) (layer B.Fab))
    (pad 2 smd rect (at 3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer B.Cu) (tedit 555EF99E)
    (at 206.25 119.75 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C2 (at -0.20066 3.29946 90) (layer B.SilkS))
    (fp_text value CP_Small (at -0.09906 -3.59918 90) (layer B.Fab))
    (pad 2 smd rect (at 3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.12 0 90) (size 2.37 2.43) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 246.79 119.75 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 1.25 -2.71 540) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 /SIN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MISO))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 /D24-D31/SOUT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 57C9F52A)
    (at 167.25 116.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference W4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value MNT (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.5 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 2.165064 60) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 2.165064 120) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 -2.165064 240) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 -2.165064 300) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module Connect:1pin (layer F.Cu) (tedit 57C9DE0D)
    (at 167.25 140.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference W3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value MNT (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.5 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 2.165064 60) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 2.165064 120) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 -2.165064 240) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 -2.165064 300) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module Connect:1pin (layer F.Cu) (tedit 57C9DDFA)
    (at 253.25 140.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference W2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value MNT (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.5 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 2.165064 60) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 2.165064 120) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 -2.165064 240) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 -2.165064 300) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module Connect:1pin (layer F.Cu) (tedit 57C9DDC7)
    (at 253.25 116.75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference W1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value MNT (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.5 0) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 2.165064 60) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 2.165064 120) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.5 0 180) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.25 -2.165064 240) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.25 -2.165064 300) (size 0.3 0.3) (drill 0.3) (layers *.Cu)
      (net 2 GND))
  )
  (module Socket_Strips:Socket_Strip_Angled_2x05 (layer F.Cu) (tedit 0)
    (at 244.25 133.83 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at -2.42 0 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -2.6 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /D0-D7/LE))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /D0-D7/CLK))
    (pad 6 thru_hole oval (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 /D24-D31/SOUT))
    (pad 8 thru_hole oval (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 /SIN))
    (pad 10 thru_hole oval (at 10.16 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_2x05.wrl
      (at (xyz 0.2 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x05 (layer F.Cu) (tedit 0)
    (at 169.79 133.83 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 5.54 -2.92 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 VCC))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /D0-D7/LE))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /D0-D7/CLK))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /D0-D7/SIN))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /MISO))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E6)
    (at 223.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R49 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /D24-D31/Q0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D49-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E7)
    (at 225.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R50 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /D24-D31/Q1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D50-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E9)
    (at 227.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R51 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /D24-D31/Q2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D51-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5EB)
    (at 229.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R52 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /D24-D31/Q3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D52-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5ED)
    (at 231.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R53 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /D24-D31/Q4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D53-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5EE)
    (at 233.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R54 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 /D24-D31/Q5))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D54-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5F0)
    (at 235.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R55 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 /D24-D31/Q6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D55-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5F4)
    (at 237.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R56 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 /D24-D31/SOUT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D56-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C562)
    (at 223.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R57 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 /D24-D31/Q0L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D57-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C563)
    (at 225.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R58 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 128 /D24-D31/Q1L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D58-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C565)
    (at 227.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R59 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 129 /D24-D31/Q2L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D59-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C568)
    (at 229.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R60 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 130 /D24-D31/Q3L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D60-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C56A)
    (at 231.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R61 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 131 /D24-D31/Q4L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D61-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C56B)
    (at 233.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R62 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 132 /D24-D31/Q5L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D62-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C56D)
    (at 235.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R63 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 133 /D24-D31/Q6L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D63-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C56F)
    (at 237.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R64 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 134 /D24-D31/Q7L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D64-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5B8)
    (at 175.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 /D0-D7/Q0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5BA)
    (at 177.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 /D0-D7/Q1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5BB)
    (at 179.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 /D0-D7/Q2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5BC)
    (at 181.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 /D0-D7/Q3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5BE)
    (at 183.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /D0-D7/Q4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5C0)
    (at 185.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 /D0-D7/Q5))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5C2)
    (at 187.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 /D0-D7/Q6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5C4)
    (at 189.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 /D8-D15/SIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C52E)
    (at 175.25 137.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -2 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 /D0-D7/Q0L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C52F)
    (at 177.25 137.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 107 /D0-D7/Q1L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C531)
    (at 179.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 108 /D0-D7/Q2L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C533)
    (at 181.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 109 /D0-D7/Q3L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C535)
    (at 183.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 110 /D0-D7/Q4L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C536)
    (at 185.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 /D0-D7/Q5L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C538)
    (at 187.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 /D0-D7/Q6L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C539)
    (at 189.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 113 /D0-D7/Q7L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D16-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5C6)
    (at 191.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 /D8-D15/Q0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5C7)
    (at 193.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 /D8-D15/Q1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5C9)
    (at 195.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 /D8-D15/Q2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5CB)
    (at 197.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 /D8-D15/Q3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D20-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5CC)
    (at 199.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /D8-D15/Q4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D21-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5CF)
    (at 201.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 /D8-D15/Q5))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5D1)
    (at 203.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 /D8-D15/Q6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5D2)
    (at 205.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 /D16-D23/SIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D24-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C540)
    (at 191.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 /D8-D15/Q0L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D25-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C542)
    (at 193.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 /D8-D15/Q1L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C544)
    (at 195.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 115 /D8-D15/Q2L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D27-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C546)
    (at 197.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 /D8-D15/Q3L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D28-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C548)
    (at 199.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 /D8-D15/Q4L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D29-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C54A)
    (at 201.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 118 /D8-D15/Q5L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D30-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C54D)
    (at 203.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 /D8-D15/Q6L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D31-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C54E)
    (at 205.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 /D8-D15/Q7L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D32-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5D4)
    (at 207.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at -2.5 -0.25 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 /D16-D23/Q0))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D33-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5D5)
    (at 209.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /D16-D23/Q1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D34-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5D7)
    (at 211.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /D16-D23/Q2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D35-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5DA)
    (at 213.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 /D16-D23/Q3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D36-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E0)
    (at 215.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 /D16-D23/Q4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D37-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E1)
    (at 217.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R38 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /D16-D23/Q5))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D38-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E3)
    (at 219.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R39 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /D16-D23/Q6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D39-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C5E4)
    (at 221.25 125.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R40 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /D24-D31/SIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D40-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C550)
    (at 207.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R41 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /D16-D23/Q0L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D41-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C552)
    (at 209.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R42 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 /D16-D23/Q1L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D42-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C554)
    (at 211.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R43 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 /D16-D23/Q2L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D43-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C558)
    (at 213.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R44 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 123 /D16-D23/Q3L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D44-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C55A)
    (at 215.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R45 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 124 /D16-D23/Q4L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D45-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C55C)
    (at 217.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R46 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 125 /D16-D23/Q5L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D46-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C55D)
    (at 219.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R47 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 126 /D16-D23/Q6L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D47-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C5C55F)
    (at 221.25 137.20098 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R48 (at -2.5 0 270) (layer F.SilkS) hide)
    (fp_text value 330R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 127 /D16-D23/Q7L))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D48-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 182.25 134.75 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 7.5 270) (layer B.SilkS))
    (fp_text value 74xx574 (at 0 -7.5 270) (layer B.Fab))
    (pad 1 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 72 /D0-D7/Q0))
    (pad 3 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 /D0-D7/Q1))
    (pad 4 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 74 /D0-D7/Q2))
    (pad 5 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 75 /D0-D7/Q3))
    (pad 6 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 76 /D0-D7/Q4))
    (pad 7 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 77 /D0-D7/Q5))
    (pad 8 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 78 /D0-D7/Q6))
    (pad 9 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 79 /D8-D15/SIN))
    (pad 10 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 /D0-D7/LE))
    (pad 12 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 113 /D0-D7/Q7L))
    (pad 13 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 112 /D0-D7/Q6L))
    (pad 14 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 111 /D0-D7/Q5L))
    (pad 15 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 110 /D0-D7/Q4L))
    (pad 16 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 109 /D0-D7/Q3L))
    (pad 17 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 108 /D0-D7/Q2L))
    (pad 18 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 107 /D0-D7/Q1L))
    (pad 19 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 80 /D0-D7/Q0L))
    (pad 20 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 198.25 134.75 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 7.5 270) (layer B.SilkS))
    (fp_text value 74xx574 (at 0 -7.5 270) (layer B.Fab))
    (pad 1 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 /D8-D15/Q0))
    (pad 3 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 82 /D8-D15/Q1))
    (pad 4 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 /D8-D15/Q2))
    (pad 5 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 /D8-D15/Q3))
    (pad 6 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 85 /D8-D15/Q4))
    (pad 7 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 86 /D8-D15/Q5))
    (pad 8 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 /D8-D15/Q6))
    (pad 9 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 88 /D16-D23/SIN))
    (pad 10 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 /D0-D7/LE))
    (pad 12 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 120 /D8-D15/Q7L))
    (pad 13 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 119 /D8-D15/Q6L))
    (pad 14 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 118 /D8-D15/Q5L))
    (pad 15 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 117 /D8-D15/Q4L))
    (pad 16 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 116 /D8-D15/Q3L))
    (pad 17 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 115 /D8-D15/Q2L))
    (pad 18 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 114 /D8-D15/Q1L))
    (pad 19 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 89 /D8-D15/Q0L))
    (pad 20 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 214.25 134.75 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 7.5 270) (layer B.SilkS))
    (fp_text value 74xx574 (at 0 -7.5 270) (layer B.Fab))
    (pad 1 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 90 /D16-D23/Q0))
    (pad 3 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 91 /D16-D23/Q1))
    (pad 4 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 92 /D16-D23/Q2))
    (pad 5 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 /D16-D23/Q3))
    (pad 6 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 94 /D16-D23/Q4))
    (pad 7 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 95 /D16-D23/Q5))
    (pad 8 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 96 /D16-D23/Q6))
    (pad 9 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 97 /D24-D31/SIN))
    (pad 10 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 /D0-D7/LE))
    (pad 12 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 127 /D16-D23/Q7L))
    (pad 13 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 126 /D16-D23/Q6L))
    (pad 14 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 125 /D16-D23/Q5L))
    (pad 15 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 124 /D16-D23/Q4L))
    (pad 16 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 123 /D16-D23/Q3L))
    (pad 17 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 122 /D16-D23/Q2L))
    (pad 18 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 121 /D16-D23/Q1L))
    (pad 19 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 98 /D16-D23/Q0L))
    (pad 20 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 230.25 134.75 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 0 7.5 270) (layer B.SilkS))
    (fp_text value 74xx574 (at 0 -7.5 270) (layer B.Fab))
    (pad 1 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 99 /D24-D31/Q0))
    (pad 3 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 100 /D24-D31/Q1))
    (pad 4 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 101 /D24-D31/Q2))
    (pad 5 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 102 /D24-D31/Q3))
    (pad 6 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 103 /D24-D31/Q4))
    (pad 7 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 104 /D24-D31/Q5))
    (pad 8 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 105 /D24-D31/Q6))
    (pad 9 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 71 /D24-D31/SOUT))
    (pad 10 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 /D0-D7/LE))
    (pad 12 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 134 /D24-D31/Q7L))
    (pad 13 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 133 /D24-D31/Q6L))
    (pad 14 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 132 /D24-D31/Q5L))
    (pad 15 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 131 /D24-D31/Q4L))
    (pad 16 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 130 /D24-D31/Q3L))
    (pad 17 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 129 /D24-D31/Q2L))
    (pad 18 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 128 /D24-D31/Q1L))
    (pad 19 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 106 /D24-D31/Q0L))
    (pad 20 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4AF)
    (at 175.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4B1)
    (at 177.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4B3)
    (at 179.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4B5)
    (at 181.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4B7)
    (at 183.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D5 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4BA)
    (at 185.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D6 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4BB)
    (at 187.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D7 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4BF)
    (at 189.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D8 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53318)
    (at 175.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D9 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5331A)
    (at 177.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D10 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53336)
    (at 179.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D11 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5333A)
    (at 181.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D12 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5333C)
    (at 183.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D13 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5333E)
    (at 185.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D14 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53341)
    (at 187.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D15 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53344)
    (at 189.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D16 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4C1)
    (at 191.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D17 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D17-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4C4)
    (at 193.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D18 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4C6)
    (at 195.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D19 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D19-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4C8)
    (at 197.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D20 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D20-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4CA)
    (at 199.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D21 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D21-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4CE)
    (at 201.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D22 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4D0)
    (at 203.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D23 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D23-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4D2)
    (at 205.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D24 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D24-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53346)
    (at 191.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D25 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D25-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53348)
    (at 193.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D26 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D26-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5334A)
    (at 195.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D27 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D27-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5334C)
    (at 197.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D28 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D28-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5334E)
    (at 199.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D29 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D29-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53350)
    (at 201.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D30 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D30-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53352)
    (at 203.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D31 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D31-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53354)
    (at 205.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D32 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D32-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4D5)
    (at 207.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D33 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D33-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4D7)
    (at 209.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D34 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D34-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4D9)
    (at 211.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D35 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D35-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4DB)
    (at 213.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D36 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D36-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4DD)
    (at 215.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D37 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D37-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4E2)
    (at 217.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D38 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D38-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4E4)
    (at 219.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D39 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D39-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4E6)
    (at 221.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D40 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D40-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53356)
    (at 207.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D41 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D41-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53358)
    (at 209.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D42 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D42-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5335A)
    (at 211.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D43 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D43-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5335D)
    (at 213.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D44 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D44-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5335F)
    (at 215.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D45 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D45-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53361)
    (at 217.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D46 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D46-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53363)
    (at 219.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D47 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D47-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53365)
    (at 221.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D48 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D48-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4E8)
    (at 223.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D49 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D49-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4EA)
    (at 225.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D50 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D50-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4ED)
    (at 227.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D51 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D51-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4EF)
    (at 229.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D52 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D52-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4F0)
    (at 231.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D53 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D53-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4F2)
    (at 233.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D54 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D54-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4F4)
    (at 235.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D55 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D55-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5C4F7)
    (at 237.25 129.25 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D56 (at -3.5 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D56-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53367)
    (at 223.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D57 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D57-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5336F)
    (at 225.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D58 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D58-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53372)
    (at 227.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D59 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D59-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53376)
    (at 229.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D60 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D60-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C53378)
    (at 231.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D61 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D61-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5337A)
    (at 233.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D62 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D62-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5337C)
    (at 235.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D63 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D63-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C5337F)
    (at 237.25 140.75 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D64 (at -4 0 90) (layer F.SilkS) hide)
    (fp_text value Led_Small (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D64-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791)
    (at 198.25 119.75)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 5.375) (layer B.SilkS))
    (fp_text value 74xx164 (at 0 -5.375) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 79 /D8-D15/SIN))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 79 /D8-D15/SIN))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 /D8-D15/Q0))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 82 /D8-D15/Q1))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 /D8-D15/Q2))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 /D8-D15/Q3))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 /D0-D7/CLK))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 85 /D8-D15/Q4))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 86 /D8-D15/Q5))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 /D8-D15/Q6))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 88 /D16-D23/SIN))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791)
    (at 182.25 119.75)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 5.375) (layer B.SilkS))
    (fp_text value 74xx164 (at 0 -5.375) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 /D0-D7/SIN))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 /D0-D7/SIN))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 72 /D0-D7/Q0))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 /D0-D7/Q1))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 74 /D0-D7/Q2))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 75 /D0-D7/Q3))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 /D0-D7/CLK))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 76 /D0-D7/Q4))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 77 /D0-D7/Q5))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 78 /D0-D7/Q6))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 79 /D8-D15/SIN))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791)
    (at 214.25 119.75)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 5.375) (layer B.SilkS))
    (fp_text value 74xx164 (at 0 -5.375) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 88 /D16-D23/SIN))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 88 /D16-D23/SIN))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 90 /D16-D23/Q0))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 91 /D16-D23/Q1))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 92 /D16-D23/Q2))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 /D16-D23/Q3))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 /D0-D7/CLK))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 94 /D16-D23/Q4))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 95 /D16-D23/Q5))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 96 /D16-D23/Q6))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 97 /D24-D31/SIN))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer B.Cu) (tedit 574D9791)
    (at 230.25 119.75)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 0 5.375) (layer B.SilkS))
    (fp_text value 74xx164 (at 0 -5.375) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 97 /D24-D31/SIN))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 97 /D24-D31/SIN))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 99 /D24-D31/Q0))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 100 /D24-D31/Q1))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 101 /D24-D31/Q2))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 102 /D24-D31/Q3))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 /D0-D7/CLK))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 103 /D24-D31/Q4))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 104 /D24-D31/Q5))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 105 /D24-D31/Q6))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 71 /D24-D31/SOUT))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 VCC))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "32-bit shift-latch" (at 195.25 118.25) (layer F.Mask))
  (gr_text "Disable MISO" (at 228.75 118.75) (layer F.SilkS))
  (gr_text GND (at 172.25 136.75) (layer F.SilkS))
  (gr_text VCC (at 172.25 133.75) (layer F.SilkS))
  (gr_text CLK (at 172.25 131.25) (layer F.SilkS))
  (gr_text CS (at 171.75 128.75) (layer F.SilkS))
  (gr_text MOSI (at 172.5 126.25) (layer F.SilkS))
  (gr_text MISO (at 172.5 123.75) (layer F.SilkS))
  (gr_text "Chain board" (at 228.25 115.75) (layer F.SilkS))
  (gr_text "Return MISO" (at 228.25 121.75) (layer F.SilkS))
  (dimension 16 (width 0.3) (layer Cmts.User)
    (gr_text "16.000 mm" (at 270.6 136.75 90) (layer Cmts.User))
    (feature1 (pts (xy 257.25 128.75) (xy 271.95 128.75)))
    (feature2 (pts (xy 257.25 144.75) (xy 271.95 144.75)))
    (crossbar (pts (xy 269.25 144.75) (xy 269.25 128.75)))
    (arrow1a (pts (xy 269.25 128.75) (xy 269.836421 129.876504)))
    (arrow1b (pts (xy 269.25 128.75) (xy 268.663579 129.876504)))
    (arrow2a (pts (xy 269.25 144.75) (xy 269.836421 143.623496)))
    (arrow2b (pts (xy 269.25 144.75) (xy 268.663579 143.623496)))
  )
  (dimension 16 (width 0.3) (layer Cmts.User)
    (gr_text "16.000 mm" (at 146.9 136.75 90) (layer Cmts.User))
    (feature1 (pts (xy 163.25 128.75) (xy 145.55 128.75)))
    (feature2 (pts (xy 163.25 144.75) (xy 145.55 144.75)))
    (crossbar (pts (xy 148.25 144.75) (xy 148.25 128.75)))
    (arrow1a (pts (xy 148.25 128.75) (xy 148.836421 129.876504)))
    (arrow1b (pts (xy 148.25 128.75) (xy 147.663579 129.876504)))
    (arrow2a (pts (xy 148.25 144.75) (xy 148.836421 143.623496)))
    (arrow2b (pts (xy 148.25 144.75) (xy 147.663579 143.623496)))
  )
  (gr_text 3 (at 229.25 133.75) (layer F.SilkS))
  (gr_text 6 (at 235.25 133.75) (layer F.SilkS))
  (gr_text 5 (at 233.25 133.75) (layer F.SilkS))
  (gr_text 4 (at 231.25 133.75) (layer F.SilkS))
  (gr_text 7 (at 237.25 133.75) (layer F.SilkS))
  (gr_text 0 (at 223.25 133.75) (layer F.SilkS))
  (gr_text 1 (at 225.25 133.75) (layer F.SilkS))
  (gr_text 2 (at 227.25 133.75) (layer F.SilkS))
  (gr_text 3 (at 213.25 133.75) (layer F.SilkS))
  (gr_text 6 (at 219.25 133.75) (layer F.SilkS))
  (gr_text 5 (at 217.25 133.75) (layer F.SilkS))
  (gr_text 4 (at 215.25 133.75) (layer F.SilkS))
  (gr_text 7 (at 221.25 133.75) (layer F.SilkS))
  (gr_text 0 (at 207.25 133.75) (layer F.SilkS))
  (gr_text 1 (at 209.25 133.75) (layer F.SilkS))
  (gr_text 2 (at 211.25 133.75) (layer F.SilkS))
  (gr_text 3 (at 197.25 133.75) (layer F.SilkS))
  (gr_text 6 (at 203.25 133.75) (layer F.SilkS))
  (gr_text 5 (at 201.25 133.75) (layer F.SilkS))
  (gr_text 4 (at 199.25 133.75) (layer F.SilkS))
  (gr_text 7 (at 205.25 133.75) (layer F.SilkS))
  (gr_text 0 (at 191.25 133.75) (layer F.SilkS))
  (gr_text 1 (at 193.25 133.75) (layer F.SilkS))
  (gr_text 2 (at 195.25 133.75) (layer F.SilkS))
  (gr_text 7 (at 189.25 133.75) (layer F.SilkS))
  (gr_text 6 (at 187.25 133.75) (layer F.SilkS))
  (gr_text 5 (at 185.25 133.75) (layer F.SilkS))
  (gr_text 4 (at 183.25 133.75) (layer F.SilkS))
  (gr_text 3 (at 181.25 133.75) (layer F.SilkS))
  (gr_text 2 (at 179.25 133.75) (layer F.SilkS))
  (gr_text 1 (at 177.25 133.75) (layer F.SilkS))
  (gr_text 0 (at 175.25 133.75) (layer F.SilkS))
  (dimension 94 (width 0.3) (layer Dwgs.User)
    (gr_text "94.000 mm" (at 210.25 98.4) (layer Dwgs.User))
    (feature1 (pts (xy 163.25 112.75) (xy 163.25 97.05)))
    (feature2 (pts (xy 257.25 112.75) (xy 257.25 97.05)))
    (crossbar (pts (xy 257.25 99.75) (xy 163.25 99.75)))
    (arrow1a (pts (xy 163.25 99.75) (xy 164.376504 99.163579)))
    (arrow1b (pts (xy 163.25 99.75) (xy 164.376504 100.336421)))
    (arrow2a (pts (xy 257.25 99.75) (xy 256.123496 99.163579)))
    (arrow2b (pts (xy 257.25 99.75) (xy 256.123496 100.336421)))
  )
  (dimension 32 (width 0.3) (layer Dwgs.User)
    (gr_text "32.000 mm" (at 280.6 128.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 257.25 144.75) (xy 281.95 144.75)))
    (feature2 (pts (xy 257.25 112.75) (xy 281.95 112.75)))
    (crossbar (pts (xy 279.25 112.75) (xy 279.25 144.75)))
    (arrow1a (pts (xy 279.25 144.75) (xy 278.663579 143.623496)))
    (arrow1b (pts (xy 279.25 144.75) (xy 279.836421 143.623496)))
    (arrow2a (pts (xy 279.25 112.75) (xy 278.663579 113.876504)))
    (arrow2b (pts (xy 279.25 112.75) (xy 279.836421 113.876504)))
  )
  (gr_line (start 163.25 112.75) (end 163.25 144.75) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 257.25 112.75) (end 163.25 112.75) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 257.25 144.75) (end 257.25 112.75) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 163.25 144.75) (end 257.25 144.75) (layer Edge.Cuts) (width 0.01))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 164.25 143.75) (xy 256.25 143.75) (xy 256.25 113.75) (xy 164.25 113.75)
      )
    )
  )
  (zone (net 66) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 168.75 131.25) (xy 168.75 136.75) (xy 245.25 136.75) (xy 245.25 132.75) (xy 243.75 131.25)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.6) (smoothing fillet))
    (polygon
      (pts
        (xy 249.25 135.75) (xy 245.75 135.75) (xy 245.75 132.25) (xy 245.5 132) (xy 245.5 122.75)
        (xy 245 122.25) (xy 241.25 122.25) (xy 238.75 119.75) (xy 171.25 119.75) (xy 168.25 122.75)
        (xy 168.25 135.75) (xy 165.25 135.75) (xy 165.25 120.75) (xy 164.25 119.75) (xy 164.25 113.75)
        (xy 249.25 113.75) (xy 249.25 135.75)
      )
    )
  )
)
