(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 694)
    (zones 0)
    (modules 57)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu mixed)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (trace_clearance 0.15)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (grid_origin 32.587001 59.765001)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber2/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C7-Pad2)")
  (net 9 +12V)
  (net 10 GND)
  (net 11 +5V)
  (net 12 "Net-(C11-Pad2)")
  (net 13 "Net-(C11-Pad1)")
  (net 14 "Net-(C13-Pad1)")
  (net 15 "Net-(C13-Pad2)")
  (net 16 "Net-(C15-Pad2)")
  (net 17 "Net-(C15-Pad1)")
  (net 18 DATA_IN)
  (net 19 CLK_IN)
  (net 20 DATA_OUT)
  (net 21 CLK_OUT)
  (net 22 FLIP_G_OFF)
  (net 23 "Net-(J5-Pad4)")
  (net 24 VPP)
  (net 25 "Net-(Q1-Pad3)")
  (net 26 FLIP_A_ON)
  (net 27 FLIP_A_OFF)
  (net 28 "Net-(Q3-Pad3)")
  (net 29 FLIP_B_ON)
  (net 30 FLIP_B_OFF)
  (net 31 "Net-(Q5-Pad3)")
  (net 32 FLIP_C_ON)
  (net 33 FLIP_C_OFF)
  (net 34 "Net-(Q7-Pad3)")
  (net 35 FLIP_D_ON)
  (net 36 FLIP_D_OFF)
  (net 37 "Net-(Q10-Pad3)")
  (net 38 FLIP_E_ON)
  (net 39 FLIP_E_OFF)
  (net 40 "Net-(Q11-Pad3)")
  (net 41 FLIP_F_ON)
  (net 42 FLIP_F_OFF)
  (net 43 "Net-(Q13-Pad3)")
  (net 44 FLIP_G_ON)
  (net 45 "Net-(U2-Pad6)")
  (net 46 "Net-(U3-Pad4)")
  (net 47 OPT1_IN)
  (net 48 OPT2_IN)
  (net 49 OPT1_OUT)
  (net 50 OPT2_OUT)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net CLK_IN)
    (add_net CLK_OUT)
    (add_net DATA_IN)
    (add_net DATA_OUT)
    (add_net FLIP_A_OFF)
    (add_net FLIP_A_ON)
    (add_net FLIP_B_OFF)
    (add_net FLIP_B_ON)
    (add_net FLIP_C_OFF)
    (add_net FLIP_C_ON)
    (add_net FLIP_D_OFF)
    (add_net FLIP_D_ON)
    (add_net FLIP_E_OFF)
    (add_net FLIP_E_ON)
    (add_net FLIP_F_OFF)
    (add_net FLIP_F_ON)
    (add_net FLIP_G_OFF)
    (add_net FLIP_G_ON)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q10-Pad3)")
    (add_net "Net-(Q11-Pad3)")
    (add_net "Net-(Q13-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q7-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad4)")
    (add_net OPT1_IN)
    (add_net OPT1_OUT)
    (add_net OPT2_IN)
    (add_net OPT2_OUT)
    (add_net VPP)
  )
  (module dot_flipper:dot_logo (layer B.Cu) (tedit 5FCE44AC)
    (at 69.187001 64.465001)
    (fp_text reference G*** (at -0.4 3.4) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 -3.6) (layer B.SilkS) hide)
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 98.487001 64.965001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q14 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 FLIP_G_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(Q13-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 91.637001 64.815001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q12 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 FLIP_F_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(Q11-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 84.987001 64.765001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q10 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 FLIP_E_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q10-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 77.537001 64.765001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 FLIP_D_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q7-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 51.837001 64.665001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 FLIP_C_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(Q5-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 45.187001 64.665001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 FLIP_B_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-small (layer B.Cu) (tedit 5FCE33A8)
    (at 38.187001 64.165001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value RJU003N03FRA (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at -1.2 0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 FLIP_A_ON))
    (pad 1 smd rect (at -1.2 -0.65 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.4 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 98.287001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 17 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 16 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 90.687001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 14 "Net-(C13-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 15 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 78.987001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 13 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 12 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 71.587001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 7 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 8 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 52.687001 65.265001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 6 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 45.087001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_1206 (layer F.Cu) (tedit 5FCBB9C8)
    (at 37.587001 64.265001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value "10u x2" (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:Pin_Header_Straight_1x05_Pitch1.27mm locked (layer F.Cu) (tedit 5FCA120A)
    (at 62.087001 68.765001 90)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (fp_text reference J5 (at 0 -1.695 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05_Male (at 0 6.775 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 VPP))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 FLIP_G_OFF))
  )
  (module dot_flipper:Pin_Header_Straight_1x02_Pitch2.54mm locked (layer F.Cu) (tedit 5FCA11E3)
    (at 41.477001 68.495001 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 49 OPT1_OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 50 OPT2_OUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:Pin_Header_Straight_1x02_Pitch2.54mm locked (layer F.Cu) (tedit 5FCA11E3)
    (at 41.477001 61.035001 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 47 OPT1_IN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 48 OPT2_IN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:Pin_Header_Straight_1x02_Pitch2.54mm locked (layer F.Cu) (tedit 5FCA11E3)
    (at 71.957001 68.495001 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 20 DATA_OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 CLK_OUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:Pin_Header_Straight_1x02_Pitch2.54mm locked (layer F.Cu) (tedit 5FCA11E3)
    (at 71.957001 61.035001 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 DATA_IN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 19 CLK_IN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:Pin_Header_Straight_1x02_Pitch2.54mm locked (layer F.Cu) (tedit 5FCA11E3)
    (at 82.117001 68.495001 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:Pin_Header_Straight_1x02_Pitch2.54mm locked (layer F.Cu) (tedit 5FCA11E3)
    (at 82.117001 61.035001 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 94.187001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 22 FLIP_G_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 95.887001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 44 FLIP_G_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 92.887001 64.765001 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q13-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 87.387001 64.865001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 FLIP_F_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 89.187001 64.865001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 41 FLIP_F_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 85.907001 64.765001 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Q11-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 80.787001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 39 FLIP_E_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 82.487001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 38 FLIP_E_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 81.187001 64.765001 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q10-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 73.187001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 36 FLIP_D_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 74.887001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 35 FLIP_D_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 73.787001 64.765001 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q7-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 55.987001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 FLIP_C_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 54.187001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 32 FLIP_C_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 53.237001 62.265001)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Q5-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 49.387001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 30 FLIP_B_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 47.587001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 29 FLIP_B_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 50.337001 64.765001 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 42.587001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 27 FLIP_A_OFF))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer B.Cu) (tedit 5FCA124A)
    (at 40.787001 64.765001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 26 FLIP_A_ON))
    (pad 2 smd rect (at 1.05 0 270) (size 1.1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:R_0805 (layer F.Cu) (tedit 5FCA124A)
    (at 42.837001 64.765001 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 1.05 0 90) (size 1.1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_0805 (layer F.Cu) (tedit 5FC796C7)
    (at 62.867001 62.315001 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 11 +5V))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:C_0805 (layer F.Cu) (tedit 5FC796C7)
    (at 60.507001 65.205001 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 9 +12V))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5FCA1255)
    (at 65.177001 65.315001 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U3 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value NCP718BSN500T1G (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 90) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 +12V))
    (pad 2 smd roundrect (at -1.35 0 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (pad 3 smd roundrect (at -1.35 0.95 90) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 4 smd roundrect (at 1.35 0.95 90) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(U3-Pad4)"))
    (pad 5 smd roundrect (at 1.35 -0.95 90) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 95.187001 64.765001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q13 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 FLIP_G_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(Q13-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C15-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C15-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 88.087001 64.785001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q11 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 FLIP_F_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(Q11-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C13-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C13-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 83.387001 64.965001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q9 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 FLIP_E_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q10-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 75.987001 64.965001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q7 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 FLIP_D_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(Q7-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C7-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C7-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 55.587001 65.265001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q5 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 FLIP_C_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(Q5-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 48.087001 64.765001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q3 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 FLIP_B_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(Q3-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5FCA125F)
    (at 40.587001 64.765001 270)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference Q1 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value DMG6602SVT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.95 270) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 FLIP_A_OFF))
    (pad 2 smd roundrect (at -1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +12V))
    (pad 3 smd roundrect (at -1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(Q1-Pad3)"))
    (pad 4 smd roundrect (at 1.35 0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)"))
    (pad 6 smd roundrect (at 1.35 -0.95 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)"))
    (pad 5 smd roundrect (at 1.35 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:MountingHole_2.2mm_M2_Pad_thin locked (layer F.Cu) (tedit 5FC78E90)
    (at 101.387001 61.965001)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -0.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.2 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.3 3.3) (drill 2.1) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module dot_flipper:MountingHole_2.2mm_M2_Pad_thin locked (layer F.Cu) (tedit 5FC78E90)
    (at 34.787001 67.565001)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -0.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.2 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.3 3.3) (drill 2.1) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module dot_flipper:QFN-28-1EP_4x4mm_Pitch0.4mm_wide (layer B.Cu) (tedit 5FCA123F)
    (at 62.587001 64.265001 45)
    (descr "28-Lead Plastic Quad Flat, No Lead Package (MK) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U2 (at -0.8 3.6 45) (layer B.SilkS) hide)
    (fp_text value PIC16F15355-I-MV (at 0 -3.35 45) (layer B.Fab))
    (pad 29 thru_hole circle (at 0 0 45) (size 0.8 0.8) (drill 0.3) (layers *.Cu *.Mask)
      (net 10 GND) (solder_paste_margin_ratio -0.2))
    (pad 1 smd rect (at -2.45 1.2 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask)
      (net 32 FLIP_C_ON))
    (pad 2 smd roundrect (at -2.3 0.8 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 35 FLIP_D_ON))
    (pad 3 smd roundrect (at -2.3 0.4 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 38 FLIP_E_ON))
    (pad 4 smd roundrect (at -2.3 0 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 FLIP_F_ON))
    (pad 5 smd roundrect (at -2.3 -0.4 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 10 GND))
    (pad 6 smd roundrect (at -2.3 -0.8 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 45 "Net-(U2-Pad6)"))
    (pad 7 smd roundrect (at -2.4 -1.2 45) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 FLIP_G_ON))
    (pad 8 smd roundrect (at -1.2 -2.4 315) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 18 DATA_IN))
    (pad 9 smd roundrect (at -0.8 -2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 CLK_IN))
    (pad 10 smd roundrect (at -0.4 -2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 47 OPT1_IN))
    (pad 11 smd roundrect (at 0 -2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 48 OPT2_IN))
    (pad 12 smd roundrect (at 0.4 -2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 20 DATA_OUT))
    (pad 13 smd roundrect (at 0.8 -2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 21 CLK_OUT))
    (pad 14 smd roundrect (at 1.2 -2.4 315) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 49 OPT1_OUT))
    (pad 15 smd roundrect (at 2.4 -1.2 45) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 50 OPT2_OUT))
    (pad 16 smd roundrect (at 2.3 -0.8 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 10 GND))
    (pad 17 smd roundrect (at 2.3 -0.4 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 11 +5V))
    (pad 18 smd roundrect (at 2.3 0 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 27 FLIP_A_OFF))
    (pad 19 smd roundrect (at 2.3 0.4 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 30 FLIP_B_OFF))
    (pad 20 smd roundrect (at 2.3 0.8 45) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 33 FLIP_C_OFF))
    (pad 21 smd roundrect (at 2.4 1.2 45) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 36 FLIP_D_OFF))
    (pad 22 smd roundrect (at 1.2 2.4 315) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 39 FLIP_E_OFF))
    (pad 23 smd roundrect (at 0.8 2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 42 FLIP_F_OFF))
    (pad 24 smd roundrect (at 0.4 2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 22 FLIP_G_OFF))
    (pad 25 smd roundrect (at 0 2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 23 "Net-(J5-Pad4)"))
    (pad 26 smd roundrect (at -0.4 2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 24 VPP))
    (pad 27 smd roundrect (at -0.8 2.3 315) (size 1.4 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 26 FLIP_A_ON))
    (pad 28 smd roundrect (at -1.2 2.4 315) (size 1.2 0.2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 29 FLIP_B_ON))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28-1EP_4x4mm_P0.4mm_EP2.4x2.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dot_flipper:7_flip_dots locked (layer F.Cu) (tedit 5FC7966A)
    (at 36.087001 61.265001)
    (fp_text reference U1 (at 0 0.5) (layer F.Fab) hide)
    (fp_text value 7_flip_dots (at 0 -2.54) (layer F.Fab) hide)
    (fp_text user " " (at 3.2 7.5) (layer F.Fab) hide)
    (pad 2-UG thru_hole circle (at 64.16 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2-UF thru_hole circle (at 54 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2-UE thru_hole circle (at 43.84 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2-UD thru_hole circle (at 33.68 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2-UC thru_hole circle (at 23.52 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2-UB thru_hole circle (at 13.36 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1-UG thru_hole circle (at 60.96 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C15-Pad1)"))
    (pad 1-UF thru_hole circle (at 50.8 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C13-Pad1)"))
    (pad 1-UE thru_hole circle (at 40.64 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C11-Pad1)"))
    (pad 1-UD thru_hole circle (at 30.48 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 1-UC thru_hole circle (at 20.32 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 1-UB thru_hole circle (at 10.16 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2-UA thru_hole circle (at 3.2 7) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1-UA thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (gr_text .wordpress.com (at 99.287001 68.765001) (layer B.Mask))
  (gr_text PierreMuth (at 97.087001 67.965001) (layer B.Mask))
  (gr_text "DOT\nFLIPPER v1.1" (at 56.687001 68.265001) (layer B.SilkS))
  (gr_text ICSP (at 65.887001 67.565001) (layer B.SilkS))
  (gr_text 12V (at 86.687001 68.865001) (layer B.SilkS))
  (gr_text GND (at 80.087001 60.665001) (layer B.SilkS))
  (gr_text CLK (at 76.487001 68.565001) (layer B.SilkS))
  (gr_text DATA (at 69.487001 60.665001) (layer B.SilkS))
  (gr_text OPT1 (at 39.287001 60.665001) (layer B.SilkS))
  (gr_text OPT2 (at 46.287001 68.765001) (layer B.SilkS))
  (gr_text OUTPUT (at 102.487001 66.065001 90) (layer B.SilkS))
  (gr_text INPUT (at 33.787001 63.465001 270) (layer B.SilkS))
  (gr_line (start 103.587001 69.765001) (end 32.587001 69.765001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.587001 59.765001) (end 103.587001 69.765001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 32.587001 59.765001) (end 103.587001 59.765001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 32.587001 69.765001) (end 32.587001 59.765001) (layer Edge.Cuts) (width 0.05))
  (zone (net 9) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 32.987001 60.165001) (xy 32.987001 69.365001) (xy 103.187001 69.365001) (xy 103.187001 60.165001)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 32.987001 60.165001) (xy 32.987001 69.365001) (xy 103.187001 69.365001) (xy 103.187001 60.165001)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 32.987001 60.165001) (xy 32.987001 69.365001) (xy 103.187001 69.365001) (xy 103.187001 60.165001)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 32.987001 60.165001) (xy 32.987001 69.365001) (xy 103.187001 69.365001) (xy 103.187001 60.165001)
      )
    )
  )
)
