<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-13.5" y1="10" x2="-13.5" y2="-10" width="0" layer="20"/>
<wire x1="-13.5" y1="-10" x2="-10" y2="-13.5" width="0" layer="20" curve="90"/>
<wire x1="-10" y1="-13.5" x2="10" y2="-13.5" width="0" layer="20"/>
<wire x1="10" y1="-13.5" x2="13.5" y2="-10" width="0" layer="20" curve="90"/>
<wire x1="13.5" y1="-10" x2="13.5" y2="10" width="0" layer="20"/>
<wire x1="13.5" y1="10" x2="10" y2="13.5" width="0" layer="20" curve="90"/>
<wire x1="10" y1="13.5" x2="-10" y2="13.5" width="0" layer="20"/>
<wire x1="-10" y1="13.5" x2="-13.5" y2="10" width="0" layer="20" curve="90"/>
<text>Mercury v1.0</text>
</plain>
<libraries>
<library name="mc18-microprocessors">
<description>&lt;b&gt;Microprocessors&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;MCU, MPU, CPU and related devices
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="QFP-10X10-64L">
<description>&lt;b&gt;QFP-10X10-64L&lt;/b&gt;
&lt;br&gt;

&lt;br&gt;Based on : STMicroelectronics STM32F303RD
- &lt;a href="http://www.st.com/content/st_com/en/products/microcontrollers/stm32-32-bit-arm-cortex-mcus/stm32-mainstream-mcus/stm32f3-series/stm32f303/stm32f303rd.htmll"&gt;Product Page&lt;/a&gt;
- &lt;a href="http://www.st.com/resource/en/datasheet/stm32f303rd.pdf"&gt;Datasheet&lt;/a&gt;

&lt;br&gt;Based on : STMicroelectronics STM32F411RE
- &lt;a href="http://www.st.com/content/st_com/en/products/microcontrollers/stm32-32-bit-arm-cortex-mcus/stm32-mainstream-mcus/stm32f3-series/stm32f303/stm32f303re.htmll"&gt;Product Page&lt;/a&gt;
- &lt;a href="http://www.st.com/resource/en/datasheet/stm32f303re.pdf"&gt;Datasheet&lt;/a&gt;

&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mc18-storage">
<description>&lt;b&gt;Data Storage / Memory&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Data storage devices, memory, sdcard, etc
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="WSON-6X5-8L">
<description>&lt;b&gt;WSON-6X5-8L&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Based on : Winbond W25Q128
- &lt;a href="http://www.winbond.com/hq/product/code-storage-flash-memory/serial-nor-flash/?__locale=en&amp;partNo=W25Q128JV"&gt;Product Page&lt;/a&gt;
- &lt;a href="http://www.winbond.com/resource-files/w25q128jv%20spi%20revd%2005022017.pdf"&gt;Datasheet&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Exposed pad removed as unnecessary to provide more room for traces
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mc18-connectors">
<description>&lt;b&gt;Connectors&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Headers, Jacks, and Pads for connecting wires to boards
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="USB-MICROB-HOR-SMD-MOLEX">
<description>&lt;b&gt;USB Micro-B&lt;/b&gt;, Horizontal, SMD
&lt;br&gt;
&lt;br&gt;Based on : Molex 473460001
- &lt;a href="http://www.molex.com/pdm_docs/sd/473460001_sd.pdf"&gt;Datasheet&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="1X02-SMD-0804">
</package>
<package name="1X02-THD-2.54">
<description>&lt;b&gt;1x02 Hole&lt;/b&gt; 40/70 mil i/o dia
&lt;br&gt;
&lt;br&gt;Standard 0.1 inch spacing</description>
</package>
<package name="1X05-SMD-0804">
</package>
<package name="1X03-SMD-0804">
</package>
<package name="1X01-THD-2.54">
<description>&lt;b&gt;1x01 Hole&lt;/b&gt; 40/70 mil i/o dia</description>
</package>
</packages>
</library>
<library name="mc18-clockgen">
<description>&lt;b&gt;Clock Generators&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Devices used to generate or manage clock or timing signals
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="DFN-2.0X1.6-4L-EXT">
<description>&lt;b&gt;DFN-4 (4-SMD)&lt;/b&gt; : 2.0mm x 1.6mm
&lt;br&gt;
&lt;br&gt;Pads extended for hand soldering
&lt;br&gt;
&lt;br&gt;Based on : Abracon ASA
- &lt;a href="http://www.abracon.com/Support/PackageDrawing/Oscillators/ASA.PDF"&gt;Drawing&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mc18-sensors">
<description>&lt;b&gt;Sensors&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Motion, Magnetic, Environmental, etc
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="QFN-4X4-24L(16)">
<description>&lt;b&gt;QFN-4X4-24L&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Based on : Ivensense MPU-6050
- &lt;a href="https://www.invensense.com/products/motion-tracking/6-axis/mpu-6050/"&gt;Product Page&lt;/a&gt;
- &lt;a href="https://www.invensense.com/wp-content/uploads/2015/02/MPU-6000-Datasheet1.pdf"&gt;Datasheet&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Pads on sides 1 and 3 are 0.5mm shorter than those on sides 2 and 4 as indicated by datasheet (#11.2).
&lt;br&gt;While the part itself has an exposed pad, the smd pad has been removed per #11.4.2 of the datasheet.
&lt;br&gt;The smd pads for pins 2-5 and 14-17 have been removed to accomodate a ground shield under the device per
&lt;br&gt;datasheet sections #7.1 and #11.4.1,3
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mc18-aesthetics">
<description>&lt;b&gt;Visual Elements&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Frames, Arrows, Notes, other visual elements for documentation or silkscreen placement
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="HOLE-M2">
</package>
<package name="LOGO_NERDGARAGE_150">
</package>
<package name="ARROW">
</package>
</packages>
</library>
<library name="mc18-passives">
<description>&lt;b&gt;Passives&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Resistors, Capacitors, Inductors
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="C1206">
<description>&lt;b&gt;1206&lt;/b&gt; SMD Device
&lt;br&gt;
&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)
&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="C0603">
<description>&lt;b&gt;0603&lt;/b&gt; SMD Device
&lt;br&gt;

&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="R0603">
<description>&lt;b&gt;0603&lt;/b&gt; SMD Device
&lt;br&gt;

&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
<library name="mercury">
<packages>
<package name="LMZM23600V3">
</package>
<package name="UCC2500-FOOTPRINT">
</package>
</packages>
</library>
<library name="mc18-discrete">
<description>&lt;b&gt;Discrete Components&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Stand alone silicon components. Diodes, Leds, Transistors, etc
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="SOD123">
<description>&lt;b&gt;SOD-123&lt;/b&gt; (PMDU) Package (this is the base 123 package, no trailing letter)
&lt;br&gt;
&lt;br&gt;Based on : Rhom
 - &lt;a href="http://rohmfs.rohm.com/en/products/databook/package/spec/discrete/diodepkg.pdf"&gt;Diode Packages&lt;/a&gt; (pkg &amp; pin size)
&lt;br&gt;Based on : LightOn
 - &lt;a href="http://www.liteon-semi.com/upfiles/application/Suggested%20Pad%20Layout%20-%20dec%202011.pdf"&gt;Suggested Pad Layouts&lt;/a&gt; (pads)
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="DIO-0603">
<description>&lt;b&gt;0603&lt;/b&gt; Diode
&lt;br&gt;
&lt;br&gt;Device outline based on standard dimensions
&lt;br&gt;Device contacts based on 25% of device length
&lt;br&gt;PCB pad centered at end of device and sized to match device contact
&lt;br&gt;
&lt;br&gt;Based on : &lt;a href="http://www.kemet.com/Lists/TechnicalArticles/Attachments/29/f2100e.pdf"&gt;Kemet dimension document&lt;/a&gt; (device, contact sizes)
&lt;br&gt;Based on : &lt;a href="http://www.resistorguide.com/resistor-sizes-and-packages/"&gt;Resistor Guide&lt;/a&gt; (pad sizes)

&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
<package name="SOD323">
<description>&lt;b&gt;SOD323/F&lt;/b&gt; (SC-90) Package
&lt;br&gt;
&lt;br&gt;Based on : Rhom
 - &lt;a href="http://rohmfs.rohm.com/en/products/databook/package/spec/discrete/diodepkg.pdf"&gt;Diode Packages&lt;/a&gt; (pkg &amp; pin size)
&lt;br&gt;Based on : LightOn
 - &lt;a href="http://www.liteon-semi.com/upfiles/application/Suggested%20Pad%20Layout%20-%20dec%202011.pdf"&gt;Suggested Pad Layouts&lt;/a&gt; (pads)
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017
&lt;br&gt;
&lt;br&gt;Notes: Package and contact dimensions are based on the F version,
&lt;br&gt;which differs from the normal version only in that the contact extends under the body.
&lt;br&gt;This drawing and pads should handle both the SC-76 and SC-90 versions of this part.</description>
</package>
</packages>
</library>
<library name="mc18-switches">
<description>&lt;b&gt;Switches&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Mechanical switching devices
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
<packages>
<package name="B3U-1000P">
<description>&lt;b&gt;B3U-1000P&lt;/b&gt; Pushbutton Switch, Top
&lt;br&gt;
&lt;br&gt;Based on : Omron B3U-1000P
- &lt;a href="http://www.omron.com/ecb/products/pdf/en-b3u.pdf"&gt;Datasheet&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Author : Leon Salisbury
&lt;br&gt;Licence : Copyright (C) 2017</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="mc18-microprocessors" package="QFP-10X10-64L" value="STM32F405R">
<attribute name="MPN" value="STM32F405R"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="mc18-storage" package="WSON-6X5-8L" value="W25Q128-WSON-6X5">
<attribute name="MFR" value="Winbond"/>
<attribute name="MPN" value="W25Q128JVPIQ"/>
<attribute name="DIGIKEY" value="W25Q128JVPIQ CT-ND"/>
<attribute name="NAME"/>
</element>
<element name="X1" library="mc18-connectors" package="USB-MICROB-HOR-SMD-MOLEX" value="CON-USB-MICROB-HOR-SMD-MOLEX">
<attribute name="EAGLEUP" value="047346-0001"/>
<attribute name="MPN" value="047346-0001"/>
<attribute name="DIGIKEY" value="WM17141CT-ND"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="mc18-clockgen" package="DFN-2.0X1.6-4L-EXT" value="8 MHz">
<attribute name="EAGLEUP" value="DFN-2.0X1.6-4L"/>
<attribute name="MPN" value="ASA-8.000MHZ-L-T"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="mc18-sensors" package="QFN-4X4-24L(16)" value="MPU-6000">
<attribute name="EAGLEUP" value="QFN-4X4-24L"/>
<attribute name="MPN" value="MPU-6000"/>
<attribute name="DIGIKEY" value="1428-1005-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="mc18-aesthetics" package="HOLE-M2" value=""/>
<element name="U$2" library="mc18-aesthetics" package="HOLE-M2" value=""/>
<element name="U$3" library="mc18-aesthetics" package="HOLE-M2" value=""/>
<element name="U$4" library="mc18-aesthetics" package="HOLE-M2" value=""/>
<element name="C1" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C11" library="mc18-passives" package="C0603" value="2.2uF">
<attribute name="MPN" value="GRM188R61H225KE11D"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C12" library="mc18-passives" package="C0603" value="2.2uF">
<attribute name="MPN" value="GRM188R61H225KE11D"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C13" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R5" library="mc18-passives" package="R0603" value="10k">
<attribute name="MPN" value="ESR03EZPJ103"/>
<attribute name="NAME"/>
</element>
<element name="C21" library="mc18-passives" package="C0603" value="470nF">
<attribute name="MPN" value="CC0603BRNPO9BNR47"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C15" library="mc18-passives" package="C0603" value="2.2nF">
<attribute name="MPN" value="C0603C222K5RACTU"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C14" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C16" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C4" library="mc18-passives" package="C0603" value="1uF">
<attribute name="MPN" value="CL10A105KB8NNNC"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C3" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="U5" library="mercury" package="LMZM23600V3" value="LMZM23600V3">
<attribute name="MPN" value="LMZM23600V3"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C18" library="mc18-passives" package="C1206" value="10uF">
<attribute name="MPN" value="CL31A106KBHNNNE"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C19" library="mc18-passives" package="C1206" value="33uF">
<attribute name="MPN" value="C3216X5R1C336M160AB"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C20" library="mc18-connectors" package="1X02-THD-2.54" value="opt">
<attribute name="NAME"/>
</element>
<element name="C22" library="mc18-passives" package="C0603" value="470nF">
<attribute name="MPN" value="CC0603BRNPO9BNR47"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R6" library="mc18-passives" package="R0603" value="1">
<attribute name="MPN" value="ESR03EZPJ1R0"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="mc18-discrete" package="SOD123" value="">
<attribute name="MPN" value="SMF26A-E3-18"/>
<attribute name="NAME"/>
</element>
<element name="D2" library="mc18-discrete" package="SOD323" value="">
<attribute name="MPN" value="PMEG4010BEA,115"/>
<attribute name="NAME"/>
</element>
<element name="D3" library="mc18-discrete" package="SOD323" value="">
<attribute name="MPN" value="PMEG4010BEA,115"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="mc18-passives" package="C0603" value="470nF">
<attribute name="MPN" value="CC0603BRNPO9BNR47"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C6" library="mc18-passives" package="C0603" value="470nF">
<attribute name="MPN" value="CC0603BRNPO9BNR47"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C7" library="mc18-passives" package="C0603" value="470nF">
<attribute name="MPN" value="CC0603BRNPO9BNR47"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C8" library="mc18-passives" package="C0603" value="470nF">
<attribute name="MPN" value="CC0603BRNPO9BNR47"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C9" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C10" library="mc18-passives" package="C0603" value="1uF">
<attribute name="MPN" value="CL10A105KB8NNNC"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R1" library="mc18-passives" package="R0603" value="10k">
<attribute name="MPN" value="ESR03EZPJ103"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="mc18-passives" package="R0603" value="1k">
<attribute name="MPN" value="ESR03EZPJ102"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="mc18-passives" package="R0603" value="220">
<attribute name="MPN" value="ESR03EZPJ221"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="mc18-passives" package="C0603" value="100nF">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="SPEC" value=""/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="D4" library="mc18-discrete" package="DIO-0603" value="RED">
<attribute name="MFR" value="Vishay"/>
<attribute name="EAGLEUP" value="MF-LED-0603"/>
<attribute name="MPN" value="VLMS1300-GS08"/>
<attribute name="DIGIKEY" value="VLMS1300-GS08CT-ND"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="mc18-connectors" package="1X02-SMD-0804" value="uart">
<attribute name="NAME"/>
</element>
<element name="J3" library="mc18-connectors" package="1X05-SMD-0804" value="motors">
<attribute name="NAME"/>
</element>
<element name="J1" library="mc18-connectors" package="1X02-THD-2.54" value="power">
<attribute name="NAME"/>
</element>
<element name="SW1" library="mc18-switches" package="B3U-1000P" value="B3U-1000P">
<attribute name="MFR" value="Omron"/>
<attribute name="MPN" value="B3U-1000P"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="mc18-passives" package="R0603" value="10k">
<attribute name="MPN" value="ESR03EZPJ103"/>
<attribute name="NAME"/>
</element>
<element name="J4" library="mc18-connectors" package="1X03-SMD-0804" value="debug">
<attribute name="NAME"/>
</element>
<element name="M1" library="mercury" package="UCC2500-FOOTPRINT" value="UCC2500"/>
<element name="U$5" library="mc18-aesthetics" package="LOGO_NERDGARAGE_150" value=""/>
<element name="U$6" library="mc18-aesthetics" package="ARROW" value=""/>
<element name="ANT" library="mc18-connectors" package="1X01-THD-2.54" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="USB_5V">
<contactref element="X1" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="STM_USB_DM">
<contactref element="X1" pad="2"/>
<contactref element="U1" pad="44"/>
</signal>
<signal name="STM_USB_DP">
<contactref element="X1" pad="3"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="STM_SPI3_CS">
<contactref element="U1" pad="50"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="STM_SPI3_SCK">
<contactref element="U1" pad="51"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="STM_SPI3_MISO">
<contactref element="U1" pad="52"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="STM_SPI3_MOSI">
<contactref element="U1" pad="53"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="STM_ADC_IN10">
<contactref element="U1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="63"/>
<contactref element="Y1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="X1" pad="P6"/>
<contactref element="X1" pad="P5"/>
<contactref element="X1" pad="P1"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="P4"/>
<contactref element="X1" pad="P3"/>
<contactref element="X1" pad="P2"/>
<contactref element="C21" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="U4" pad="18"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="11"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="U5" pad="11"/>
<contactref element="U5" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C5" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="M1" pad="11"/>
<contactref element="M1" pad="10"/>
<contactref element="M1" pad="1"/>
<contactref element="M1" pad="9"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="STM_OSC_IN">
<contactref element="U1" pad="5"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="LED1">
<contactref element="U1" pad="10"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="STM_UART1_TX">
<contactref element="U1" pad="58"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="STM_UART1_RX">
<contactref element="U1" pad="59"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="STM_TIM2/5_CH1">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="STM_TIM2/5_CH2">
<contactref element="U1" pad="15"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="STM_TIM2/5_CH3">
<contactref element="U1" pad="16"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="STM_TIM2/5_CH4">
<contactref element="U1" pad="17"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="STM_SPI1_CS">
<contactref element="U1" pad="20"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="STM_SPI1_SCK">
<contactref element="U1" pad="21"/>
<contactref element="U4" pad="23"/>
</signal>
<signal name="STM_SPI1_MISO">
<contactref element="U1" pad="22"/>
<contactref element="U4" pad="9"/>
</signal>
<signal name="STM_SPI1_MOSI">
<contactref element="U1" pad="23"/>
<contactref element="U4" pad="24"/>
</signal>
<signal name="MPU6000_INT">
<contactref element="U1" pad="24"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="STM_SWCLK">
<contactref element="U1" pad="49"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="STM_SWDIO">
<contactref element="U1" pad="46"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="STM_SPI2_CS">
<contactref element="U1" pad="33"/>
<contactref element="M1" pad="8"/>
</signal>
<signal name="STM_SPI2_SCK">
<contactref element="U1" pad="34"/>
<contactref element="M1" pad="4"/>
</signal>
<signal name="STM_SPI2_MISO">
<contactref element="U1" pad="35"/>
<contactref element="M1" pad="5"/>
</signal>
<signal name="STM_SPI2_MOSI">
<contactref element="U1" pad="36"/>
<contactref element="M1" pad="3"/>
</signal>
<signal name="CC2500_CE">
<contactref element="U1" pad="37"/>
<contactref element="M1" pad="6"/>
</signal>
<signal name="CC2500_IRQ">
<contactref element="U1" pad="38"/>
<contactref element="M1" pad="7"/>
</signal>
<signal name="STM_RESET">
<contactref element="U1" pad="7"/>
<contactref element="C13" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="31"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U1" pad="47"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="STM_BOOT0">
<contactref element="U1" pad="60"/>
<contactref element="SW1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="48"/>
<contactref element="Y1" pad="1"/>
<contactref element="Y1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="R5" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="U4" pad="13"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="7"/>
<contactref element="C22" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="SW1" pad="2"/>
<contactref element="M1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U4" pad="10"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="20"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="4"/>
<contactref element="R6" pad="2"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="VSAFE">
<contactref element="R6" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="C17" pad="2"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="VBAT">
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D4" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="ANT">
<contactref element="M1" pad="12"/>
<contactref element="ANT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
