(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 129)
    (zones 0)
    (modules 44)
    (nets 16)
  )
  (page USLetter)
  (title_block
    (title "Fisher 500 Power Supply Capacitor Board")
    (date 2020-03-02)
    (company "SDS Labs")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 1.905)
    (user_trace_width 2.54)
    (user_trace_width 3.175)
    (user_trace_width 3.81)
    (trace_clearance 0.2)
    (zone_clearance 1.27)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.35 6.35)
    (pad_drill 4.445)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C5-Pad1)")
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C8-Pad1)")
  (net 8 "Net-(C9-Pad1)")
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C12-Pad1)")
  (net 12 "Net-(C13-Pad1)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(D3-Pad3)")
  (net 15 "Net-(D3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D3-Pad3)")
  )
  (module TestPoint:TestPoint_Pad_D3.0mm (layer F.Cu) (tedit 5E6E6998)
    (at 161.29 131.064)
    (descr "SMD pad as test Point, diameter 3.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.398) (layer F.SilkS))
    (fp_text value TestPoint_Pad_D3.0mm (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 4.445) (layers *.Cu *.Mask))
  )
  (module TestPoint:TestPoint_Pad_D3.0mm (layer F.Cu) (tedit 5E6E699E)
    (at 161.29 131.064)
    (descr "SMD pad as test Point, diameter 3.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.398) (layer F.SilkS))
    (fp_text value TestPoint_Pad_D3.0mm (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 4.445) (layers *.Cu *.Mask))
  )
  (module TestPoint:TestPoint_Pad_D3.0mm (layer F.Cu) (tedit 5E6E69A7)
    (at 72.136 131.064)
    (descr "SMD pad as test Point, diameter 3.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.398) (layer F.SilkS))
    (fp_text value TestPoint_Pad_D3.0mm (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 4.445) (layers *.Cu *.Mask))
  )
  (module TestPoint:TestPoint_Pad_D3.0mm (layer F.Cu) (tedit 5E6E69AD)
    (at 72.136 131.064)
    (descr "SMD pad as test Point, diameter 3.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.398) (layer F.SilkS))
    (fp_text value TestPoint_Pad_D3.0mm (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 4.445) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6962)
    (at 157.48 74.168 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.508 -4.572) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.81 -0.762) (layer B.SilkS))
    (fp_text user %R (at 2.032 -4.572) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6954)
    (at 157.48 93.472 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C2 (at 0.127 -3.937) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 4.064 -0.508) (layer B.SilkS))
    (fp_text user %R (at 1.778 -4.064) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E693B)
    (at 157.48 112.776 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C3 (at -0.889 -4.572) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.556 0) (layer B.SilkS))
    (fp_text user %R (at 1.016 -4.826 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6A20)
    (at 136.652 112.776 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C4 (at -0.508 -4.699) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.556 -0.254) (layer B.SilkS))
    (fp_text user %R (at 1.524 -4.064) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6A61)
    (at 136.652 93.472 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C5 (at -0.254 -5.334) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.81 -0.254) (layer B.SilkS))
    (fp_text user %R (at 2.286 -4.318) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6A6F)
    (at 136.652 74.168 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C6 (at 0.635 -3.937) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.75 -0.508) (layer B.SilkS))
    (fp_text user %R (at 2.286 -3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6B80)
    (at 110.744 74.168 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C7 (at 0.635 -5.334) (layer F.SilkS))
    (fp_text value "47uf 400V" (at 3.683 -0.127) (layer B.SilkS))
    (fp_text user %R (at 2.032 -5.461) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6B72)
    (at 110.744 93.472 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C8 (at 0.762 -4.445) (layer F.SilkS))
    (fp_text value "47uf 400V" (at 3.683 -0.254) (layer B.SilkS))
    (fp_text user %R (at 2.159 -4.572) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6B65)
    (at 110.744 112.776 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C9 (at 0.762 -5.08) (layer F.SilkS))
    (fp_text value "47uf 400V" (at 3.81 -0.254) (layer B.SilkS))
    (fp_text user %R (at 2.413 -5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6B39)
    (at 100.584 48.768 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C10 (at 0.762 -5.207) (layer F.SilkS))
    (fp_text value "2200uf 35V" (at 3.81 -0.381) (layer B.SilkS))
    (fp_text user %R (at 2.286 -5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6B1D)
    (at 119.888 48.768 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C11 (at 1.016 -4.318) (layer F.SilkS))
    (fp_text value "2200uf 35V" (at 3.683 -0.508) (layer B.SilkS))
    (fp_text user %R (at 2.54 -4.445) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6C0F)
    (at 82.804 107.188 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C12 (at 0.254 -4.699) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.683 -0.127) (layer B.SilkS))
    (fp_text user %R (at 2.159 -4.826) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5E6E6C2C)
    (at 82.804 87.376 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C13 (at 0.889 -4.572) (layer F.SilkS))
    (fp_text value "100uf 250V" (at 3.683 -0.254) (layer B.SilkS))
    (fp_text user %R (at 2.667 -4.699) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E6981)
    (at 170.688 70.612 270)
    (descr "Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D1 (at 6.858 0 270) (layer F.SilkS))
    (fp_text value 1N5408 (at 7.62 0 270) (layer B.SilkS))
    (fp_text user K (at 0 -2.6 270) (layer F.SilkS))
    (fp_text user K (at 0 -2.6 270) (layer F.Fab))
    (fp_text user %R (at 8.3325 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E698E)
    (at 170.688 90.932 270)
    (descr "Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 -3.72 270) (layer F.SilkS))
    (fp_text value 1N5408 (at 8.128 -0.254 270) (layer B.SilkS))
    (fp_text user %R (at 8.3325 0 270) (layer F.Fab))
    (fp_text user K (at 0 -2.6 270) (layer F.Fab))
    (fp_text user K (at 0 -2.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:Diode_Bridge_Vishay_KBU (layer F.Cu) (tedit 5E6E6C72)
    (at 78.232 60.96 270)
    (descr "Vishay KBU rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88656/kbu4.pdf")
    (tags "Vishay KBU rectifier diode bridge")
    (fp_text reference D3 (at 4.826 3.429 270) (layer F.SilkS))
    (fp_text value KBU8M (at 7.747 3.429 270) (layer B.SilkS))
    (fp_text user %R (at 7.7 3.3 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 15.24 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 "Net-(D3-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/Diode_Bridge_Vishay_KBU.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal (layer F.Cu) (tedit 5E6E6C41)
    (at 85.852 44.196 270)
    (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
    (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
    (fp_text reference R1 (at 8.89 0 270) (layer F.SilkS))
    (fp_text value "15 5w" (at 12.065 0 270) (layer B.SilkS))
    (fp_text user %R (at 11.43 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 22.86 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E6CAF)
    (at 69.596 102.616 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R2 (at 5.461 0 270) (layer F.SilkS))
    (fp_text value "470 3W" (at 7.366 0.127 270) (layer B.SilkS))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E6CA5)
    (at 69.596 82.804 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R3 (at 5.207 0 270) (layer F.SilkS))
    (fp_text value "470 3W" (at 7.62 0.127 270) (layer B.SilkS))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E6BA1)
    (at 97.028 85.852 90)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R4 (at 10.033 -0.127 90) (layer F.SilkS))
    (fp_text value "2.7K 1W" (at 7.874 0.127 90) (layer B.SilkS))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E6BAC)
    (at 97.028 105.156 90)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R5 (at 10.033 -0.127 90) (layer F.SilkS))
    (fp_text value "22K 1W" (at 8.509 -0.127 90) (layer B.SilkS))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5E6E6BC1)
    (at 97.028 109.22 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R6 (at 5.207 0 270) (layer F.SilkS))
    (fp_text value "82K 1W" (at 7.112 0.127 270) (layer B.SilkS))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5E6E6AC6)
    (at 123.952 77.724 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (fp_text reference R7 (at 4.318 0 270) (layer F.SilkS))
    (fp_text value "330K 0.5W" (at 6.223 -0.127 270) (layer B.SilkS))
    (fp_text user %R (at 6.35 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5E6E6ADA)
    (at 123.952 94.996 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (fp_text reference R8 (at 4.064 0 270) (layer F.SilkS))
    (fp_text value "330K 0.5W" (at 6.604 0 270) (layer B.SilkS))
    (fp_text user %R (at 6.35 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L19.0mm_W6.0mm_P15.00mm_MKS4 (layer F.Cu) (tedit 5E6E6A3F)
    (at 170.688 125.984 90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 19mm width 6mm Capacitor")
    (fp_text reference C14 (at 7.5 -4.25 90) (layer F.SilkS))
    (fp_text value "0.01uF 630V" (at 7.874 0 90) (layer B.SilkS))
    (fp_text user %R (at 7.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L19.0mm_W6.0mm_P15.00mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E69EF)
    (at 176.784 90.932)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value "B1 RedYel (B+)" (at 1.524 9.144 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E69F8)
    (at 176.784 80.264)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J2 (at -0.254 3.429) (layer F.SilkS))
    (fp_text value "B2 Red (B+)" (at 1.651 -7.747 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6C92)
    (at 69.596 72.136)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J3 (at -0.127 3.429) (layer F.SilkS))
    (fp_text value "Filament 1" (at 2.54 4.826 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 14 "Net-(D3-Pad3)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6C83)
    (at 69.596 65.024)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS))
    (fp_text value "Filament 2" (at 2.413 -6.731 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 15 "Net-(D3-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6B92)
    (at 97.028 66.04)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J5 (at 3.937 -1.27) (layer F.SilkS))
    (fp_text value "A (350v)" (at 6.477 0.762) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6ABA)
    (at 123.952 71.628)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J6 (at -3.81 -2.286) (layer F.SilkS))
    (fp_text value "B (375V)" (at -0.381 -4.064) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6AB0)
    (at 147.32 70.104)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J7 (at 3.556 -1.524) (layer F.SilkS))
    (fp_text value "C (430V)" (at 0 6.096 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6BDF)
    (at 102.108 87.884)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J8 (at 3.429 -0.254) (layer F.SilkS))
    (fp_text value "D (295V)" (at -1.524 -6.35 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6BDC)
    (at 102.616 107.188)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J9 (at 3.556 -0.254) (layer F.SilkS))
    (fp_text value "E (215V)" (at -2.032 -6.223 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6C21)
    (at 88.392 79.248)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS))
    (fp_text value "F (160V)" (at 0 -3.683) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 12 "Net-(C13-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6B0F)
    (at 110.236 61.468)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J11 (at 0 -3.81) (layer F.SilkS))
    (fp_text value "Filament Out" (at 0 3.81) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1.5mm (layer F.Cu) (tedit 5E6E6A11)
    (at 122.936 128.524)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J12 (at 0 -3.81) (layer F.SilkS))
    (fp_text value GND (at 0 3.81) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.0005 4.0005) (drill 1.50114) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module TestPoint:TestPoint_Pad_D3.0mm (layer F.Cu) (tedit 5E6E6C5D)
    (at 72.39 48.26)
    (descr "SMD pad as test Point, diameter 3.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.398) (layer F.SilkS))
    (fp_text value TestPoint_Pad_D3.0mm (at 0 2.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 4.445) (layers *.Cu *.Mask))
  )
  (module sdsLogos:sdsLabs-large-fSilk (layer F.Cu) (tedit 5A94A1E6)
    (at 106.045 130.81)
    (fp_text reference G*** (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08) (layer F.SilkS) hide)
  )
  (module sdsLogos:sdsLabs-medium-bSilk (layer F.Cu) (tedit 5A94A272)
    (at 123.19 117.602)
    (fp_text reference G*** (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 -2.54) (layer B.SilkS) hide)
  )
  (gr_text "Fisher 500c Capboard" (at 141.224 131.572) (layer F.SilkS))
  (gr_circle (center 161.29 131.064) (end 163.83 131.064) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 72.136 131.064) (end 74.676 131.064) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 72.39 48.26) (end 74.93 48.26) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 72.39 48.26) (end 74.93 48.26) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 161.29 130.81) (end 163.83 130.81) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 72.39 130.81) (end 74.93 130.81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.04 41.91) (end 66.04 137.16) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 41.91) (end 66.04 41.91) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 67.31) (end 129.54 41.91) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 67.31) (end 129.54 67.31) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 137.16) (end 180.34 67.31) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.04 137.16) (end 180.34 137.16) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 1.27))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.635) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 66.04 137.16) (xy 180.34 137.16) (xy 180.34 67.056) (xy 129.54 67.056) (xy 129.54 42.164)
        (xy 66.04 42.164)
      )
    )
  )
)
