(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 11)
    (zones 0)
    (modules 3)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3)
    (at 167.86 96.78158)
    (attr smd)
    (fp_text reference Q2 (at 0.034 -2.67458) (layer F.SilkS) hide)
    (fp_text value SI3400A (at 0.034 3.04042) (layer F.SilkS) hide)
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3)
    (at 167.86 89.154)
    (attr smd)
    (fp_text reference Q1 (at 0.034 2.667) (layer F.SilkS) hide)
    (fp_text value AO3400 (at 0.025 -2.794) (layer F.SilkS) hide)
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)") (solder_mask_margin 0.07))
  )
  (module project_mosfet_test:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 600C770A)
    (at 159.512 86.614)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at -1.845 -2.27 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Male (at -1.845 14.97 180) (layer F.Fab))
    (fp_text user %R (at -0.23 6.35 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Sam Pearce" (at 159.004 90.17 270) (layer B.SilkS))
  (gr_text "MOSFET test v2" (at 169.037 94.488 270) (layer B.SilkS))
  (gr_line (start 157.988 100.584) (end 171.45 100.584) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.45 85.344) (end 171.45 100.584) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.988 85.344) (end 157.988 100.584) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.988 85.344) (end 171.45 85.344) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 92.837) (xy 163.83 92.837) (xy 163.83 85.344) (xy 171.45 85.344)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad5)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 100.584) (xy 163.83 100.584) (xy 163.83 93.091) (xy 171.45 93.091)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 92.837) (xy 163.83 92.837) (xy 163.83 89.281) (xy 171.45 89.281)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 89.027) (xy 163.83 89.027) (xy 163.83 85.344) (xy 171.45 85.344)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 96.647) (xy 163.83 96.647) (xy 163.83 93.091) (xy 171.45 93.091)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad6)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 100.584) (xy 163.83 100.584) (xy 163.83 96.901) (xy 171.45 96.901)
      )
    )
  )
)
