(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 125)
    (zones 0)
    (modules 3)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4572)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.4572)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VBAT)
  (net 2 /32)
  (net 3 /30)
  (net 4 /33)
  (net 5 /31)
  (net 6 /29)
  (net 7 /DAT1)
  (net 8 /DAT0)
  (net 9 /GND-SD)
  (net 10 /CLK)
  (net 11 /3V3-SD)
  (net 12 /CMD)
  (net 13 /DAT3)
  (net 14 /DAT2)
  (net 15 /VUSB)
  (net 16 /D-)
  (net 17 /D+)
  (net 18 /25)
  (net 19 /27)
  (net 20 /28)
  (net 21 /26)
  (net 22 /24)
  (net 23 /ON_OFF)
  (net 24 /PROGRAM)
  (net 25 /GND-1)
  (net 26 /3V3-1)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /24)
    (add_net /25)
    (add_net /26)
    (add_net /27)
    (add_net /28)
    (add_net /29)
    (add_net /30)
    (add_net /31)
    (add_net /32)
    (add_net /33)
    (add_net /3V3-1)
    (add_net /3V3-SD)
    (add_net /CLK)
    (add_net /CMD)
    (add_net /D+)
    (add_net /D-)
    (add_net /DAT0)
    (add_net /DAT1)
    (add_net /DAT2)
    (add_net /DAT3)
    (add_net /GND-1)
    (add_net /GND-SD)
    (add_net /ON_OFF)
    (add_net /PROGRAM)
    (add_net /VBAT)
    (add_net /VUSB)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Teensy:Teensy40_SMT (layer F.Cu) (tedit 5D52D69C)
    (at 160.02 97.79 270)
    (fp_text reference U1 (at 0 -10.16 90) (layer F.SilkS))
    (fp_text value GND-1 (at 0 10.16 90) (layer F.Fab))
    (pad 13 thru_hole circle (at 13.97 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at -16.51 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at -13.97 -5.08 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 /VUSB))
    (pad 32 thru_hole circle (at -13.97 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at -11.43 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at -8.89 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at -6.35 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -3.81 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -1.27 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 1.27 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 3.81 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 6.35 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 8.89 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 11.43 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 13.97 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 16.51 -7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 16.51 -5.08 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 /ON_OFF))
    (pad 18 thru_hole circle (at 16.51 -2.54 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 /PROGRAM))
    (pad 17 thru_hole circle (at 16.51 0 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 /GND-1))
    (pad 16 thru_hole circle (at 16.51 2.54 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 /3V3-1))
    (pad 15 thru_hole circle (at 16.51 5.08 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 14 thru_hole circle (at 16.51 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 11.43 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 8.89 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 6.35 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 3.81 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1.27 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.27 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.81 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -6.35 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -8.89 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -11.43 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 54 thru_hole circle (at -15.875 1.27 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D+))
    (pad 53 thru_hole circle (at -15.875 -1.27 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D-))
    (pad 52 thru_hole circle (at -9.3716 3.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 14 /DAT2))
    (pad 51 thru_hole circle (at -9.3716 2.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 13 /DAT3))
    (pad 50 thru_hole circle (at -9.3716 1.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 /CMD))
    (pad 49 thru_hole circle (at -9.3716 0.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 /3V3-SD))
    (pad 48 thru_hole circle (at -9.3716 -0.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 /CLK))
    (pad 47 thru_hole circle (at -9.3716 -1.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 /GND-SD))
    (pad 46 thru_hole circle (at -9.3716 -2.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 /DAT0))
    (pad 45 thru_hole circle (at -9.3716 -3.5 270) (size 0.804 0.804) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 /DAT1))
    (pad 44 thru_hole circle (at 8.89 5.08 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 4 /33))
    (pad 43 thru_hole circle (at 11.43 5.08 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 2 /32))
    (pad 42 thru_hole circle (at 8.89 2.54 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 5 /31))
    (pad 41 thru_hole circle (at 11.43 2.54 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 3 /30))
    (pad 40 thru_hole circle (at 8.89 0 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 6 /29))
    (pad 39 thru_hole circle (at 11.43 0 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 20 /28))
    (pad 38 thru_hole circle (at 8.89 -2.54 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 19 /27))
    (pad 37 thru_hole circle (at 11.43 -2.54 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 21 /26))
    (pad 36 thru_hole circle (at 8.89 -5.08 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 18 /25))
    (pad 35 thru_hole circle (at 11.43 -5.08 270) (size 1.304 1.304) (drill 1) (layers *.Cu *.Mask)
      (net 22 /24))
    (pad 2 thru_hole circle (at -13.97 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -16.51 7.62 270) (size 1.404 1.404) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 170.18 114.3 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 35.35) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /VUSB))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D-))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D+))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /27))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /25))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /26))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /28))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /24))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /3V3-1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /GND-1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PROGRAM))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /ON_OFF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 149.86 81.28)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 0 35.35) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VBAT))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /30))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /32))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /33))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /31))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /29))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /DAT2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /DAT3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CMD))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /3V3-SD))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /CLK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND-SD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DAT0))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DAT1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2019-09-10 (at 159.9438 111.6584) (layer B.SilkS))
  (gr_text "teensy 4\nbreakout\n" (at 158.7246 85.1154) (layer B.SilkS))
  (gr_line (start 151.638 115.57) (end 148.59 115.57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.638 114.3) (end 151.638 115.57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.91 114.3) (end 151.638 114.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.91 115.57) (end 168.91 114.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.45 115.57) (end 168.91 115.57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.37 109.22) (end 166.37 106.68) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 109.22) (end 166.37 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 106.68) (end 153.67 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 104.775) (end 153.67 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.37 104.775) (end 153.67 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.37 88.392) (end 166.37 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 88.392) (end 166.37 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166.37 106.68) (end 153.67 106.68) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.845 80.01) (end 148.59 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.845 81.915) (end 156.845 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.195 81.915) (end 156.845 81.915) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.195 80.01) (end 163.195 81.915) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.45 80.01) (end 163.195 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.59 115.57) (end 148.59 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.45 80.01) (end 171.45 115.57) (layer Edge.Cuts) (width 0.05))
)
