(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 418)
    (zones 0)
    (modules 39)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.762)
    (user_trace_width 2.794)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /Shoulder/GPS/V_BATT)
  (net 2 /Shoulder/Q_3V3)
  (net 3 "Net-(D601-Pad1)")
  (net 4 /Shoulder/GPS/GPS_ANT1)
  (net 5 /Shoulder/SCL)
  (net 6 /Shoulder/SDA)
  (net 7 +5V)
  (net 8 /Shoulder/GPS/Regulator/BYP)
  (net 9 /Shoulder/GPS/USB/CC1)
  (net 10 /Shoulder/GPS/USB/PD-)
  (net 11 /Shoulder/GPS/USB/PD+)
  (net 12 /Shoulder/GPS/USB/CC2)
  (net 13 "Net-(J701-PadS1)")
  (net 14 /Shoulder/GPS/R_D+)
  (net 15 /Shoulder/GPS/R_D-)
  (net 16 /Shoulder/GPS/D-)
  (net 17 /Shoulder/GPS/D+)
  (net 18 /Shoulder/Q_MAG~RST)
  (net 19 /Shoulder/Q_PPS)
  (net 20 /Shoulder/Q_TX_SDA)
  (net 21 /Shoulder/Q_RX_SDA)
  (net 22 /Shoulder/Q_TX_SCL)
  (net 23 /Shoulder/Q_RX_SCL)
  (net 24 /Shoulder/Q_TX_GPS)
  (net 25 /Shoulder/Q_RX_GPS)
  (net 26 /Shoulder/Q_INT)
  (net 27 "Net-(R620-Pad1)")
  (net 28 "Net-(R621-Pad1)")
  (net 29 /Shoulder/Q_GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net +5V)
    (add_net /Shoulder/GPS/D+)
    (add_net /Shoulder/GPS/D-)
    (add_net /Shoulder/GPS/R_D+)
    (add_net /Shoulder/GPS/R_D-)
    (add_net /Shoulder/GPS/Regulator/BYP)
    (add_net /Shoulder/GPS/USB/CC1)
    (add_net /Shoulder/GPS/USB/CC2)
    (add_net /Shoulder/GPS/USB/PD+)
    (add_net /Shoulder/GPS/USB/PD-)
    (add_net /Shoulder/GPS/V_BATT)
    (add_net /Shoulder/Q_3V3)
    (add_net /Shoulder/Q_GND)
    (add_net /Shoulder/Q_INT)
    (add_net /Shoulder/Q_MAG~RST)
    (add_net /Shoulder/Q_PPS)
    (add_net /Shoulder/Q_RX_GPS)
    (add_net /Shoulder/Q_RX_SCL)
    (add_net /Shoulder/Q_RX_SDA)
    (add_net /Shoulder/Q_TX_GPS)
    (add_net /Shoulder/Q_TX_SCL)
    (add_net /Shoulder/Q_TX_SDA)
    (add_net /Shoulder/SCL)
    (add_net /Shoulder/SDA)
    (add_net "Net-(D601-Pad1)")
    (add_net "Net-(J701-PadS1)")
    (add_net "Net-(R620-Pad1)")
    (add_net "Net-(R621-Pad1)")
  )
  (net_class RF ""
    (clearance 0.254)
    (trace_width 2.794)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /Shoulder/GPS/GPS_ANT1)
  )
  (module KwanSystems:GCTUSBTypeC_PTH (layer F.Cu) (tedit 5F3D494F)
    (at 120.904 86.36)
    (descr "Part GCT USB4105. Digikey 2073-USB4105-GF-ACT-ND")
    (tags USB)
    (attr smd)
    (fp_text reference J701 (at 9.144 2.794) (layer F.SilkS) hide)
    (fp_text value USB_C_Receptacle_USB2.0 (at -4.826 4.572) (layer F.Fab))
    (fp_text user "PCB edge" (at -6.604 0.762) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at -2.89 -6.28) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -6.28) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad A1 smd rect (at -3.2 -7.6425) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad A12 smd rect (at 3.2 -7.6425) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad B12 smd rect (at -3.2 -7.0675) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad A4 smd rect (at -2.4 -7.6425) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad B9 smd rect (at -2.4 -7.0675) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad B8 smd rect (at -1.75 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 9 /Shoulder/GPS/USB/CC1))
    (pad B7 smd rect (at -0.75 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoulder/GPS/USB/PD-))
    (pad A6 smd rect (at -0.25 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 11 /Shoulder/GPS/USB/PD+))
    (pad A7 smd rect (at 0.25 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoulder/GPS/USB/PD-))
    (pad B6 smd rect (at 0.75 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 11 /Shoulder/GPS/USB/PD+))
    (pad A8 smd rect (at 1.25 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -7.355) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 12 /Shoulder/GPS/USB/CC2))
    (pad B4 smd rect (at 2.4 -7.0675) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad A9 smd rect (at 2.4 -7.6425) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad B1 smd rect (at 3.2 -7.0675) (size 0.6 0.575) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad S1 thru_hole oval (at -4.32 -6.78) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J701-PadS1)"))
    (pad S1 thru_hole oval (at -4.32 -2.6) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J701-PadS1)"))
    (pad S1 thru_hole oval (at 4.32 -2.6) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J701-PadS1)"))
    (pad S1 thru_hole oval (at 4.32 -6.78) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J701-PadS1)"))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/USB4105-GF-A--3DModel-STEP-46669.STEP
      (offset (xyz 0 3.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module KwanSystems:NEO-M9N_M8T_M8U (layer F.Cu) (tedit 5F3D5C96)
    (at 129.54 70.358 270)
    (descr "<h3>u-blox NEO-M9N GPS Module</h3>\n\n<h4>Mechanical Specifications</h4>\n<ul>\n<li>Overall: 12.2mm x 16.0mm</li>\n<li>Pad Pitch: 1.1mm</li>\n<li>Pad Width: .8mm </li>\n<li>Pad Length: .9mm</li>\n<li>Number of Pins: 24</li>\n<li></li>\n<li></li>\n<li></li>\n<li></li>\n<li></li>\n<li></li>\n</ul>")
    (fp_text reference U601 (at -6.1 -8.5 90) (layer F.SilkS) hide)
    (fp_text value NEO_M8U (at -6.1 9 90) (layer F.SilkS) hide)
    (fp_text user >Value (at -6.1 9 90) (layer F.Fab))
    (fp_text user >Name (at -6.1 -8.5 90) (layer F.SilkS) hide)
    (fp_text user Z (at -1.1 0 90) (layer Dwgs.User))
    (fp_text user Y (at 3.5 0 90) (layer Dwgs.User))
    (fp_text user X (at 0 3.7 90) (layer Dwgs.User))
    (pad 1 smd rect (at 6 7 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 6 5.9 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 6 4.8 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 19 /Shoulder/Q_PPS) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 6 3.7 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 6 2.6 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 15 /Shoulder/GPS/R_D-) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 6 1.5 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 14 /Shoulder/GPS/R_D+) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at 6 0.4 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.1016))
    (pad 8 smd rect (at 6 -2.6 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 smd rect (at 6 -3.7 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 6 -4.8 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 6 -5.9 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 4 /Shoulder/GPS/GPS_ANT1) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 6 -7 270) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
    (pad 13 smd rect (at -6 -7 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
    (pad 14 smd rect (at -6 -5.9 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 15 smd rect (at -6 -4.8 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 smd rect (at -6 -3.7 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 17 smd rect (at -6 -2.6 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 18 smd rect (at -6 0.4 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 19 smd rect (at -6 1.5 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (solder_mask_margin 0.1016))
    (pad 20 smd rect (at -6 2.6 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 27 "Net-(R620-Pad1)") (solder_mask_margin 0.1016))
    (pad 21 smd rect (at -6 3.7 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 28 "Net-(R621-Pad1)") (solder_mask_margin 0.1016))
    (pad 22 smd rect (at -6 4.8 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 1 /Shoulder/GPS/V_BATT) (solder_mask_margin 0.1016))
    (pad 23 smd rect (at -6 5.9 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.1016))
    (pad 24 smd rect (at -6 7 90) (size 1.8 0.8) (layers F.Cu F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/NEO-M8Q-0--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Package_SO:TSSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5F459D4B)
    (at 104.14 71.374 90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U202 (at 0 -2.55 90) (layer F.SilkS) hide)
    (fp_text value P82B96 (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.15 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 7 smd rect (at 2.15 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoulder/SCL))
    (pad 6 smd rect (at 2.15 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 /Shoulder/Q_RX_SCL))
    (pad 5 smd rect (at 2.15 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 /Shoulder/Q_TX_SCL))
    (pad 4 smd rect (at -2.15 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 3 smd rect (at -2.15 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /Shoulder/Q_TX_SDA))
    (pad 2 smd rect (at -2.15 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /Shoulder/Q_RX_SDA))
    (pad 1 smd rect (at -2.15 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoulder/SDA))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 105.156 71.374 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J207 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Open (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 5 /Shoulder/SCL))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 22 /Shoulder/Q_TX_SCL))
  )
  (module KwanSystems:SolderJumper-2_Bridged (layer F.Cu) (tedit 5F4584FB)
    (at 103.124 71.374 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference J201 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Open (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 6 /Shoulder/SDA))
    (pad 2 smd rect (at 0.65 0 90) (size 1 1.5) (layers F.Cu F.Mask)
      (net 21 /Shoulder/Q_RX_SDA))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 101.092 70.612 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R207 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /Shoulder/SCL))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 101.092 71.882)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R201 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /Shoulder/SDA))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.03 67.31)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 2.2uF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:StKwansSoldermask (layer B.Cu) (tedit 5F40003C)
    (at 103.886 81.788 180)
    (fp_text reference G902 (at -3.683 2.7432) (layer B.Mask) hide)
    (fp_text value KwanSystems (at 4.2926 -3.7084) (layer B.Mask) hide)
    (fp_text user github.com/kwan3217/kicad (at -9.652 10.668 unlocked) (layer B.SilkS))
    (fp_text user stkwans.blogspot.com (at -14.986 12.7 unlocked) (layer B.SilkS))
    (fp_text user "a division of Kwan Systems" (at 4.064 3.556 unlocked) (layer B.SilkS) hide)
    (fp_text user "St Kwan's Home for" (at 3.81 8.636 unlocked) (layer B.SilkS))
    (fp_text user "the Terminally ADD" (at 4.318 6.096 unlocked) (layer B.SilkS))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.38 74.93)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R702 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1k (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /Shoulder/GPS/USB/CC2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.38 76.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R701 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1k (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /Shoulder/GPS/USB/CC1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.222 62.484 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R621 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 27 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /Shoulder/Q_RX_GPS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R621-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.508 62.484)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R620 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 27 (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /Shoulder/Q_TX_GPS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(R620-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.27 78.994 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R606 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 27 (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /Shoulder/GPS/R_D+))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /Shoulder/GPS/D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.746 78.994 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R605 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 27 (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /Shoulder/GPS/R_D-))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /Shoulder/GPS/D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:Axis (layer F.Cu) (tedit 590A7BBF)
    (at 115.062 62.992 180)
    (descr "Built for the MPU-9250 using guidelines found in http://cds.linear.com/docs/en/packaging/Carsem%20MLP%20users%20guide.pdf")
    (fp_text reference G504 (at -1.3 1.5) (layer F.Fab) hide)
    (fp_text value Axis (at -1.8 2.75) (layer F.SilkS) hide)
    (fp_text user Z (at 3.5 -2) (layer B.SilkS))
    (fp_text user Y (at -1.016 -3) (layer B.SilkS))
    (fp_text user X (at 3.2 0.1) (layer B.SilkS))
    (fp_text user Z (at 3.5 -2) (layer F.SilkS))
    (fp_text user X (at 3.2 0.1) (layer F.SilkS))
    (fp_text user Y (at -1.016 -3) (layer F.SilkS))
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 120.904 82.042 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference G903 (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW (at 0.75 0) (layer B.Fab) hide)
  )
  (module KwanSystems:Symbol_KiCAD-Logo_CopperAndSilkScreenTop_small (layer B.Cu) (tedit 0)
    (at 130.048 84.582 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference G901 (at 0 0) (layer B.SilkS) hide)
    (fp_text value DesignedWithKicad (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 105.41 64.262 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 106.426 64.262 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.22 73.66)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C408 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.22 69.596 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.712 64.262 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C308 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.728 64.262 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C305 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_1.27mm:PinSocket_1x12_P1.27mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 5F3DC010)
    (at 107.95 77.47 270)
    (descr "surface-mounted straight socket strip, 1x12, 1.27mm pitch, single row, style 1 (pin 1 left) (https://gct.co/pdfjs/web/viewer.html?file=/Files/Drawings/BD075.pdf&t=1511594726925), script generated")
    (tags "Surface mounted socket strip SMD 1x12 1.27mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J202 (at 5.655 -2.27 270) (layer F.SilkS) hide)
    (fp_text value Conn_02x06_Male (at 5.655 14.97 270) (layer F.Fab))
    (fp_text user %R (at 5.31 6.35 180) (layer F.Fab))
    (pad 12 smd rect (at 1.35 6.985 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 /Shoulder/Q_MAG~RST))
    (pad 10 smd rect (at 1.35 4.445 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 /Shoulder/Q_RX_SDA))
    (pad 8 smd rect (at 1.35 1.905 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 /Shoulder/Q_RX_SCL))
    (pad 6 smd rect (at 1.35 -0.635 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 /Shoulder/Q_RX_GPS))
    (pad 4 smd rect (at 1.35 -3.175 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 2 smd rect (at 1.35 -5.715 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 11 smd rect (at -1.35 5.715 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 9 smd rect (at -1.35 3.175 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 /Shoulder/Q_TX_SDA))
    (pad 7 smd rect (at -1.35 0.635 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 /Shoulder/Q_TX_SCL))
    (pad 5 smd rect (at -1.35 -1.905 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 24 /Shoulder/Q_TX_GPS))
    (pad 3 smd rect (at -1.35 -4.445 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /Shoulder/Q_PPS))
    (pad 1 smd rect (at -1.35 -6.985 270) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 /Shoulder/Q_INT))
  )
  (module KwanSystems:BME280 (layer F.Cu) (tedit 5F3D9117)
    (at 109.22 71.628 180)
    (fp_text reference U401 (at -0.05 2.5) (layer F.SilkS) hide)
    (fp_text value BME280 (at 0 -2.5) (layer F.Fab))
    (pad 6 smd rect (at -1.025 0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 7 smd rect (at -1.025 -0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 5 smd rect (at -1.025 0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 4 smd rect (at 1.025 0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoulder/SCL))
    (pad 1 smd rect (at 1.025 -0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 3 smd rect (at 1.025 0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoulder/SDA))
    (pad 8 smd rect (at -1.025 -0.975 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 2 smd rect (at 1.025 -0.325 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (model /home/jeppesen/workspace/kicad/KwanSystems.pretty/BME280--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.634 63.5)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100k (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.84 64.008 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 33 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoulder/GPS/V_BATT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 106.172 66.548 180)
    (fp_text reference U501 (at 3.048 0.405 180) (layer F.Fab))
    (fp_text value LSM6DSO (at 4.826 -0.762) (layer F.Fab) hide)
    (fp_text user >Name (at -2 -1.5) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoulder/SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoulder/SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:LGA-14L (layer F.Cu) (tedit 5F3D6253)
    (at 109.474 66.548 180)
    (fp_text reference U301 (at 3.048 0.405 180) (layer F.Fab))
    (fp_text value LSM6DSO (at 4.826 -0.762) (layer F.Fab) hide)
    (fp_text user >Name (at -2 -1.5) (layer F.Fab) hide)
    (fp_text user Z (at -0.45 0.25) (layer Dwgs.User))
    (fp_text user X (at 0.35 0.25) (layer Dwgs.User))
    (fp_text user Y (at -0.4 -0.5) (layer Dwgs.User))
    (pad 1 smd rect (at -1.1625 -0.75 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1625 -0.25 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1625 0.25 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -1.1625 0.75 180) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Shoulder/Q_INT) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.5 0.9125 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0 0.9125 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at 0.5 0.9125 270) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 1.1625 0.75) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 1.1625 0.25) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 1.1625 -0.25) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 1.1625 -0.75) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 0.5 -0.9125 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 0 -0.9125 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoulder/SCL) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -0.5 -0.9125 90) (size 0.475 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoulder/SDA) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:W3011 (layer F.Cu) (tedit 5F3D4E93)
    (at 135.96 80.772 90)
    (fp_text reference Y601 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value W3011 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "PCB edge" (at 0.2 1.1 90) (layer Dwgs.User))
    (fp_text user "No pour within this boundary, on either side" (at 0 -2.9 90) (layer Dwgs.User))
    (fp_text user Antenna (at 0 -1.594 90) (layer F.SilkS))
    (fp_text user >Value (at 0 -1 90) (layer F.Fab))
    (fp_text user "Reversible\nAntenna" (at 0 -0.0662 90) (layer F.Fab))
    (pad 3 smd rect (at -1.6 0 90) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 1.6 0.475 90) (size 0.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at 1.6 -0.475 90) (size 0.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /Shoulder/GPS/GPS_ANT1) (solder_mask_margin 0.1016))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 3.2 3.2 3.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:AK09970 (layer F.Cu) (tedit 5F3D3F3B)
    (at 102.108 65.532 180)
    (fp_text reference U201 (at 0 0.3) (layer Dwgs.User))
    (fp_text value AK09970 (at 0.2 -0.3) (layer Dwgs.User))
    (fp_text user Z (at -0.6 0.7) (layer Dwgs.User))
    (fp_text user Y (at -0.7 -0.9) (layer Dwgs.User))
    (fp_text user X (at 0.8 0.7) (layer Dwgs.User))
    (pad 16 smd rect (at -1.5375 0.75 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 18 /Shoulder/Q_MAG~RST))
    (pad 15 smd rect (at -1.5375 0.25 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 14 smd rect (at -1.5375 -0.25 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -1.5375 -0.75 90) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 12 smd rect (at -0.75 -1.5375) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 11 smd rect (at -0.25 -1.5375) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 0.25 -1.5375) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 0.75 -1.5375) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 1.5375 -0.75 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.5375 -0.25 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.5375 0.25 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.5375 0.75 270) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 6 /Shoulder/SDA))
    (pad 4 smd rect (at 0.75 1.5375 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.25 1.5375 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 5 /Shoulder/SCL))
    (pad 2 smd rect (at -0.25 1.5375 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 1 smd rect (at -0.75 1.5375 180) (size 0.3 0.575) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 113.03 70.866 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U801 (at 0 -2.9 90) (layer F.SilkS) hide)
    (fp_text value "MIC5319 3.3V" (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /Shoulder/Q_3V3))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /Shoulder/GPS/Regulator/BYP))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 128.016 82.55)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U701 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value USBLC6-2SC6 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 /Shoulder/GPS/D+))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 /Shoulder/GPS/D-))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /Shoulder/GPS/USB/PD-))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 /Shoulder/GPS/USB/PD+))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 119.6085 65.024)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D601 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0.5A/40V/420mV (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /Shoulder/Q_3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D601-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.03 68.326 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.17) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /Shoulder/GPS/Regulator/BYP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.03 73.406 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.84 65.024 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /Shoulder/Q_GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /Shoulder/GPS/V_BATT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KwanSystems:Coin_Cell_ML414H (layer F.Cu) (tedit 5EC6E8B4)
    (at 118.364 68.834)
    (descr "<h3>SEIKO ML414H-IV01E Reflowable Lithium Battery</h3>\n\n<p>\nML414H is a rechargeable, coin type battery with features\nsuch as Pb-free reflowable (Peak temperature: 260 C) and\nhigh temperature heat resistance.\n</p>\n\n<ul>\n<li>3V</li>\n<li>1mAH</li>\n<li>4.8mm Diamter</li>\n</ul>")
    (fp_text reference B601 (at -1.905004 -1.270003) (layer F.SilkS) hide)
    (fp_text value ML414H (at -1.016 3.302) (layer F.Fab) hide)
    (pad 1 smd rect (at 2.022 -2.032) (size 1 1) (layers F.Cu F.Mask)
      (net 1 /Shoulder/GPS/V_BATT) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0.6 1.85) (size 4.2 1.7) (layers F.Cu F.Mask)
      (net 29 /Shoulder/Q_GND) (solder_mask_margin 0.1016))
  )
  (gr_text "a division of\nKwan Systems" (at 107.442 78.74) (layer B.SilkS))
  (gr_text INT (at 114.935 77.47 90) (layer F.SilkS))
  (gr_text PPS (at 112.395 77.47 90) (layer F.SilkS))
  (gr_text TGPS (at 109.855 77.47 90) (layer F.SilkS))
  (gr_text TSCL (at 107.315 77.47 90) (layer F.SilkS))
  (gr_text TSDA (at 104.775 77.47 90) (layer F.SilkS))
  (gr_text ID (at 102.235 77.47 90) (layer F.SilkS))
  (gr_text GND (at 113.665 77.47 90) (layer F.SilkS))
  (gr_text 3V3 (at 111.125 77.47 90) (layer F.SilkS))
  (gr_text RGPS (at 108.585 77.47 90) (layer F.SilkS))
  (gr_text RSCL (at 106.045 77.47 90) (layer F.SilkS))
  (gr_text RSDA (at 103.505 77.47 90) (layer F.SilkS))
  (gr_text M~RST (at 100.965 77.47 90) (layer F.SilkS))
  (gr_text "Wearable Pocketometer\nShoulder Board\nv1.0\n2020 Sep 01" (at 135.636 64.516) (layer B.SilkS))
  (gr_line (start 99.06 63.5) (end 99.06 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.06 66.04) (end 99.06 83.82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 86.36) (end 134.62 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.6 83.82) (end 99.06 83.82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.6 63.5) (end 101.6 60.96) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 134.62 63.5) (end 137.16 63.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 134.62 83.82) (end 134.62 86.36) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 60.96) (end 101.6 60.96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 83.82) (end 137.16 63.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 29) (net_name /Shoulder/Q_GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 60.96) (xy 137.16 78.74) (xy 132.842 78.74) (xy 132.842 82.804) (xy 135.128 82.804)
        (xy 135.128 82.042) (xy 136.906 82.042) (xy 136.906 82.804) (xy 137.16 82.804) (xy 137.16 86.36)
        (xy 99.06 86.36) (xy 99.06 60.96)
      )
    )
  )
  (zone (net 29) (net_name /Shoulder/Q_GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.16 60.96) (xy 137.16 78.74) (xy 132.842 78.74) (xy 132.842 82.804) (xy 137.16 82.804)
        (xy 137.16 86.36) (xy 99.06 86.36) (xy 99.06 60.96)
      )
    )
  )
)
