<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.76" y2="0" width="0" layer="20"/>
<wire x1="17.76" y1="0" x2="17.76" y2="48.565" width="0" layer="20"/>
<wire x1="17.76" y1="48.565" x2="0" y2="48.565" width="0" layer="20"/>
<wire x1="0" y1="48.565" x2="0" y2="0" width="0" layer="20"/>
<text>ESProg01</text>
<text>v1.0c</text>
<text>2</text>
<text>0</text>
<text>3V3</text>
<text>GND</text>
<text>gitlab.vsb.cz/oshw/esprog01</text>
<text>More info at:</text>
<text>2016</text>
</plain>
<libraries>
<library name="ph-pas">
<description>&lt;h2&gt;PetrH's Passive Components Library&lt;/h2&gt;
&lt;h4&gt;© 2012 Petr Havlíček&lt;/h4&gt;
&lt;p&gt;
High quality hand made libraries by Petr Havlíček. Land patterns and silkscreens are based on IPC-7351 through Mentor Graphics IPC-7351 LP Viewer.&lt;/p&gt;</description>
<packages>
<package name="CAPC0805">
<description>&lt;h3&gt;Capacitor SMD 0805&lt;/h3&gt;

&lt;pre&gt;
&lt;b&gt;Type:&lt;/b&gt;	Ceramic Chip Capacitor
&lt;b&gt;Mounting:&lt;/b&gt;	SMT
&lt;b&gt;Standart:&lt;/b&gt;	EIA 0805
&lt;b&gt;IPC Name:&lt;/b&gt;	CAPC2013X95N
&lt;b&gt;Pins:&lt;/b&gt;	2
&lt;/pre&gt;</description>
</package>
<package name="F-PTC-1210">
</package>
<package name="RESC0805">
<description>&lt;h3&gt;Resistor SMD 0805&lt;/h3&gt;

&lt;pre&gt;
&lt;b&gt;Type:&lt;/b&gt;	Thin Film Chip Resistor
&lt;b&gt;Mounting:&lt;/b&gt;	SMT
&lt;b&gt;Standart:&lt;/b&gt;	EIA 0805
&lt;b&gt;IPC Name:&lt;/b&gt;	RESC2013X65N
&lt;b&gt;Pins:&lt;/b&gt;	2
&lt;/pre&gt;</description>
</package>
</packages>
</library>
<library name="ph-con">
<description>&lt;h2&gt;PetrH's Connectors Library&lt;/h2&gt;
&lt;h4&gt;© 2012 Petr Havlíček&lt;/h4&gt;
&lt;p&gt;
High quality hand made libraries by Petr Havlíček. Land patterns and silkscreens are based on IPC-7351 through Mentor Graphics IPC-7351 LP Viewer.&lt;/p&gt;</description>
<packages>
<package name="USB-A-M-SMT">
</package>
<package name="J1X04">
</package>
<package name="J1X02">
</package>
</packages>
</library>
<library name="ph-oth">
<description>&lt;h2&gt;PetrH's Other Library&lt;/h2&gt;
&lt;h4&gt;© 2012 Petr Havlíček&lt;/h4&gt;
&lt;p&gt;
High quality hand made libraries by Petr Havlíček. Land patterns and silkscreens are based on IPC-7351 through Mentor Graphics IPC-7351 LP Viewer.&lt;/p&gt;</description>
<packages>
<package name="MOD-ESP8266-01">
</package>
<package name="LOGO-PH-SILK">
<description>&lt;h1&gt;PetrH - Logo&lt;/h1&gt;</description>
</package>
</packages>
</library>
<library name="ph-dis">
<description>&lt;h2&gt;PetrH's Dicretes Library&lt;/h2&gt;
&lt;h4&gt;© 2012 Petr Havlíček&lt;/h4&gt;
&lt;p&gt;
High quality hand made libraries by Petr Havlíček. Land patterns and silkscreens are based on IPC-7351 through Mentor Graphics IPC-7351 LP Viewer.&lt;/p&gt;</description>
<packages>
<package name="SOT230P700X180-4N">
<description>&lt;h3&gt;SOT-223 Transistor&lt;/h3&gt;&lt;pre&gt;
&lt;b&gt;Type:&lt;/b&gt;	Transistor
&lt;b&gt;Mounting:&lt;/b&gt;	SMD
&lt;b&gt;IPC name:&lt;/b&gt;	SOT230P700x180-4N
&lt;b&gt;Standart:&lt;/b&gt;	JEDEC TO-261AA 
&lt;b&gt;Pins:&lt;/b&gt;	4</description>
</package>
<package name="LED-0805">
<description>&lt;h3&gt;SMD 0805 LED&lt;/h3&gt;&lt;pre&gt;
&lt;b&gt;Type:&lt;/b&gt;	LED
&lt;b&gt;Mounting:&lt;/b&gt;	SMT
&lt;b&gt;Size:&lt;/b&gt;	0805
&lt;b&gt;Pins:&lt;/b&gt;	2</description>
</package>
</packages>
</library>
<library name="ph-ic">
<description>&lt;h2&gt;PetrH's Integrated Circuits Library&lt;/h2&gt;
&lt;h4&gt;© 2012 Petr Havlíček&lt;/h4&gt;
&lt;p&gt;
High quality hand made libraries by Petr Havlíček. Land patterns and silkscreens are based on IPC-7351 through Mentor Graphics IPC-7351 LP Viewer.&lt;/p&gt;</description>
<packages>
<package name="SOP65P780X200-20N">
<description>&lt;h3&gt;SMD SSOP-20 IC&lt;/h3&gt;&lt;pre&gt;
&lt;b&gt;Name:&lt;/b&gt;	Shrink Small Outline Integrated Circuit
&lt;b&gt;IPC Name:&lt;/b&gt;	SOP65P780X200-20N
&lt;b&gt;Standart:&lt;/b&gt;	JEDEC MO-150AE
&lt;b&gt;Type:&lt;/b&gt;	Integrate Circuit
&lt;b&gt;Mounting:&lt;/b&gt;	SMT
&lt;b&gt;Pins:&lt;/b&gt;	20</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="ph-pas" package="CAPC0805" value="100nF/50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ph-pas" package="CAPC0805" value="10uF/6.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="ph-pas" package="CAPC0805" value="100nF/50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ph-pas" package="CAPC0805" value="10nF/100V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ph-pas" package="CAPC0805" value="47pF/50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="ph-pas" package="CAPC0805" value="47pF/50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="ph-pas" package="CAPC0805" value="100nF/50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="ph-pas" package="CAPC0805" value="4.7uF/6.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON1" library="ph-con" package="USB-A-M-SMT" value="DS1098-BN0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="ph-oth" package="MOD-ESP8266-01" value="ZL262-8DG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="ph-pas" package="F-PTC-1210" value="SM035-16">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="ph-dis" package="SOT230P700X180-4N" value="LD1117S33TR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="ph-dis" package="LED-0805" value="EL17-215SYGC/53">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ph-pas" package="RESC0805" value="680R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="ph-pas" package="RESC0805" value="27R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ph-pas" package="RESC0805" value="27R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="ph-pas" package="RESC0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="ph-con" package="J1X04" value="ZL262-4SG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="ph-pas" package="RESC0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="ph-ic" package="SOP65P780X200-20N" value="FT231XS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="ph-pas" package="RESC0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="ph-pas" package="CAPC0805" value="100nF/50V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="ph-oth" package="LOGO-PH-SILK" value="LOGO-SILK"/>
<element name="J1" library="ph-con" package="J1X02" value="ZL201-02G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3V3">
<contactref element="J3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="J2" pad="8"/>
<contactref element="R6" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="CON1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="4"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="6"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="F1" pad="1"/>
<contactref element="CON1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="D-">
<contactref element="CON1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D+">
<contactref element="CON1" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GPIO2">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GPIO0">
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="J2" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="J2" pad="7"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$11">
<contactref element="C8" pad="1"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$9">
</signal>
<signal name="4">
</signal>
<signal name="N$6">
<contactref element="J2" pad="4"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="J2" pad="6"/>
<contactref element="R4" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="12"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="11"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VOUT">
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="IC1" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
