(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 0.1916)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "#808080D4") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (color "Polyimide") (thickness 0.1016) (material "Polyimide") (epsilon_r 3.2) (loss_tangent 0.004))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "#808080FF"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00210fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "output/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J2-Pin_7-Pad7)")
  (net 2 "/VCC_TARGET")
  (net 3 "/TMS")
  (net 4 "/GND")
  (net 5 "/TCK")
  (net 6 "/TDO")
  (net 7 "unconnected-(J1-Pin_7-Pad7)")
  (net 8 "/TDI")
  (net 9 "unconnected-(J1-Pin_9-Pad9)")
  (net 10 "/~{SRST}")
  (net 11 "unconnected-(J2-Pin_8-Pad8)")
  (footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD" (layer "F.Cu")
    (at 152.4 93.98 -90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (property "Sheetfile" "swd-blaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J1" (at 0 1.905 -180) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Counter_Clockwise" (at 0 4.235 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -2.54 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/VCC_TARGET") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 1.95 -2.54 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/TMS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.95 -1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 1.95 -1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/TCK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.95 0 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.95 0 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/TDO") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -1.95 1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(J1-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 1.95 1.27 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/TDI") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at -1.95 2.54 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(J1-Pin_9-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 1.95 2.54 270) (size 2.4 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/~{SRST}") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "custom:PinSocket_2x05_P100mil_Board_Tab" (layer "F.Cu")
    (at 157.48 102.87 -90)
    (descr "Through hole angled socket strip, 2x05, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x05 2.54mm double row")
    (property "Sheetfile" "swd-blaster.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 8.255 5.08) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Counter_Clockwise" (at -5.65 12.93 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -8.315 5.08) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/TCK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/TDO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/VCC_TARGET") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/TMS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/~{SRST}") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(J2-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(J2-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/TDI") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/GND") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x05_P2.54mm_Horizontal.wrl"
      (offset (xyz -2.54 -10.16 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "custom:gs_logo_200mil" (layer "B.Cu")
    (at 148.59 92.71 -135)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "GS1" (at 0 3.175 45) (layer "B.SilkS") hide)
    (fp_text value "GS_logo" (at 0 0.5 45) (layer "B.Fab"))
    (pad "1" smd custom (at 0 0 225) (size 5.08 5.08) (layers "B.Cu")
      (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
  )
  (gr_arc (start 150.495 106.045) (mid 150.944013 106.230987) (end 151.13 106.68)
    (layer "Edge.Cuts"))
  (gr_line (start 158.75 92.71) (end 158.75 104.775)
    (layer "Edge.Cuts"))
  (gr_line (start 150.495 106.045) (end 147.32 106.045)
    (layer "Edge.Cuts"))
  (gr_arc (start 153.67 106.68) (mid 153.855987 106.230987) (end 154.305 106.045)
    (layer "Edge.Cuts"))
  (gr_arc (start 156.21 90.17) (mid 158.006051 90.913949) (end 158.75 92.71)
    (layer "Edge.Cuts"))
  (gr_line (start 146.05 104.775) (end 146.05 92.71)
    (layer "Edge.Cuts"))
  (gr_line (start 151.13 111.125) (end 151.13 106.68)
    (layer "Edge.Cuts"))
  (gr_arc (start 146.05 92.71) (mid 146.793949 90.913949) (end 148.59 90.17)
    (layer "Edge.Cuts"))
  (gr_line (start 157.48 106.045) (end 154.305 106.045)
    (layer "Edge.Cuts"))
  (gr_arc (start 147.32 106.045) (mid 146.421974 105.673026) (end 146.05 104.775)
    (layer "Edge.Cuts"))
  (gr_line (start 153.67 106.68) (end 153.67 111.125)
    (layer "Edge.Cuts"))
  (gr_arc (start 158.75 104.775) (mid 158.378026 105.673026) (end 157.48 106.045)
    (layer "Edge.Cuts"))
  (gr_arc (start 153.67 111.125) (mid 152.4 112.395) (end 151.13 111.125)
    (layer "Edge.Cuts"))
  (gr_line (start 148.59 90.17) (end 156.21 90.17)
    (layer "Edge.Cuts"))
  (gr_text "VCC" (at 154.94 98.425) (layer "B.SilkS"))
  (gr_text "Altera\nBlaster\nAdapter" (at 154.94 93.98) (layer "B.SilkS"))
  (gr_text "TMS" (at 152.4 104.775) (layer "B.SilkS"))
  (gr_text "TDO" (at 154.94 104.775) (layer "B.SilkS"))
  (gr_text "GND" (at 147.32 98.425) (layer "B.SilkS"))
  (gr_text "TCK" (at 157.48 104.775) (layer "B.SilkS"))
  (gr_text "TDI" (at 147.32 104.775) (layer "B.SilkS"))
  (gr_text "RST" (at 152.4 98.425) (layer "B.SilkS"))
  (gr_text "GND" (at 157.48 98.425) (layer "B.SilkS"))
  (zone (net 4) (net_name "/GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.3048) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 90.17)
        (xy 158.75 90.17)
        (xy 158.75 106.045)
        (xy 146.05 106.045)
      )
    )
  )
)
