(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 64)
    (no_connects 0)
    (area 46.914999 77.394999 199.465001 128.345001)
    (thickness 1.6)
    (drawings 6)
    (tracks 160)
    (zones 0)
    (modules 52)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(CN1-Pad1)")
  (net 2 "Net-(CN1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(CN1-Pad4)")
  (net 5 "Net-(CN1-Pad5)")
  (net 6 "Net-(CN1-Pad7)")
  (net 7 "Net-(CN1-Pad8)")
  (net 8 "Net-(CN2-Pad1)")
  (net 9 "Net-(CN2-Pad2)")
  (net 10 "Net-(CN2-Pad4)")
  (net 11 "Net-(CN2-Pad5)")
  (net 12 "Net-(CN2-Pad7)")
  (net 13 "Net-(CN2-Pad8)")
  (net 14 "Net-(CN3-Pad1)")
  (net 15 "Net-(CN3-Pad2)")
  (net 16 "Net-(CN3-Pad4)")
  (net 17 "Net-(CN3-Pad5)")
  (net 18 "Net-(CN3-Pad7)")
  (net 19 "Net-(CN3-Pad8)")
  (net 20 "Net-(CN4-Pad1)")
  (net 21 "Net-(CN4-Pad2)")
  (net 22 "Net-(CN4-Pad3)")
  (net 23 "Net-(CN4-Pad4)")
  (net 24 "Net-(CN4-Pad5)")
  (net 25 "Net-(CN4-Pad6)")
  (net 26 "Net-(D1-Pad2)")
  (net 27 "Net-(D2-Pad2)")
  (net 28 "Net-(D3-Pad2)")
  (net 29 "Net-(D4-Pad2)")
  (net 30 "Net-(D5-Pad2)")
  (net 31 "Net-(D6-Pad2)")
  (net 32 "Net-(D7-Pad2)")
  (net 33 "Net-(D8-Pad2)")
  (net 34 "Net-(D9-Pad2)")
  (net 35 "Net-(D10-Pad2)")
  (net 36 "Net-(D11-Pad2)")
  (net 37 "Net-(D12-Pad2)")
  (net 38 "Net-(D13-Pad2)")
  (net 39 "Net-(D14-Pad2)")
  (net 40 "Net-(D15-Pad2)")
  (net 41 "Net-(D16-Pad2)")
  (net 42 "Net-(D17-Pad2)")
  (net 43 "Net-(D18-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(CN1-Pad1)")
    (add_net "Net-(CN1-Pad2)")
    (add_net "Net-(CN1-Pad4)")
    (add_net "Net-(CN1-Pad5)")
    (add_net "Net-(CN1-Pad7)")
    (add_net "Net-(CN1-Pad8)")
    (add_net "Net-(CN2-Pad1)")
    (add_net "Net-(CN2-Pad2)")
    (add_net "Net-(CN2-Pad4)")
    (add_net "Net-(CN2-Pad5)")
    (add_net "Net-(CN2-Pad7)")
    (add_net "Net-(CN2-Pad8)")
    (add_net "Net-(CN3-Pad1)")
    (add_net "Net-(CN3-Pad2)")
    (add_net "Net-(CN3-Pad4)")
    (add_net "Net-(CN3-Pad5)")
    (add_net "Net-(CN3-Pad7)")
    (add_net "Net-(CN3-Pad8)")
    (add_net "Net-(CN4-Pad1)")
    (add_net "Net-(CN4-Pad2)")
    (add_net "Net-(CN4-Pad3)")
    (add_net "Net-(CN4-Pad4)")
    (add_net "Net-(CN4-Pad5)")
    (add_net "Net-(CN4-Pad6)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_09x5.08mm_Vertical (layer F.Cu) (tedit 5797DB0C)
    (at 52.07 123.19)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 09; pin pitch: 5.08mm; Vertical || order number: 1755804 12A || order number: 1924376 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x09_G_5.08mm")
    (fp_text reference CN1 (at 20.32 -6) (layer F.SilkS))
    (fp_text value CONN_01X09 (at 20.32 5.3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(CN1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(CN1-Pad2)"))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 15.24 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(CN1-Pad4)"))
    (pad 5 thru_hole oval (at 20.32 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(CN1-Pad5)"))
    (pad 6 thru_hole oval (at 25.4 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 30.48 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(CN1-Pad7)"))
    (pad 8 thru_hole oval (at 35.56 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 "Net-(CN1-Pad8)"))
    (pad 9 thru_hole oval (at 40.64 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_09x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_09x5.08mm_Vertical (layer F.Cu) (tedit 5797DB0C)
    (at 102.87 123.19)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 09; pin pitch: 5.08mm; Vertical || order number: 1755804 12A || order number: 1924376 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x09_G_5.08mm")
    (fp_text reference CN2 (at 20.32 -6) (layer F.SilkS))
    (fp_text value CONN_01X09 (at 20.32 5.3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(CN2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 "Net-(CN2-Pad2)"))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 15.24 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 "Net-(CN2-Pad4)"))
    (pad 5 thru_hole oval (at 20.32 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 "Net-(CN2-Pad5)"))
    (pad 6 thru_hole oval (at 25.4 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 30.48 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 12 "Net-(CN2-Pad7)"))
    (pad 8 thru_hole oval (at 35.56 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 13 "Net-(CN2-Pad8)"))
    (pad 9 thru_hole oval (at 40.64 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_09x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_09x5.08mm_Vertical (layer F.Cu) (tedit 5797DB0C)
    (at 153.67 123.19)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 09; pin pitch: 5.08mm; Vertical || order number: 1755804 12A || order number: 1924376 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x09_G_5.08mm")
    (fp_text reference CN3 (at 20.32 -6) (layer F.SilkS))
    (fp_text value CONN_01X09 (at 20.32 5.3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 "Net-(CN3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 "Net-(CN3-Pad2)"))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 15.24 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 "Net-(CN3-Pad4)"))
    (pad 5 thru_hole oval (at 20.32 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 "Net-(CN3-Pad5)"))
    (pad 6 thru_hole oval (at 25.4 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 30.48 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 "Net-(CN3-Pad7)"))
    (pad 8 thru_hole oval (at 35.56 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 "Net-(CN3-Pad8)"))
    (pad 9 thru_hole oval (at 40.64 0) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_09x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_08x5.08mm_Vertical (layer F.Cu) (tedit 5797DB0C)
    (at 95.25 82.55 180)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 08; pin pitch: 5.08mm; Vertical || order number: 1755794 12A || order number: 1924363 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x08_G_5.08mm")
    (fp_text reference CN4 (at 17.78 -6 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 17.78 5.3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 20 "Net-(CN4-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 "Net-(CN4-Pad2)"))
    (pad 3 thru_hole oval (at 10.16 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 "Net-(CN4-Pad3)"))
    (pad 4 thru_hole oval (at 15.24 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 23 "Net-(CN4-Pad4)"))
    (pad 5 thru_hole oval (at 20.32 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 24 "Net-(CN4-Pad5)"))
    (pad 6 thru_hole oval (at 25.4 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 25 "Net-(CN4-Pad6)"))
    (pad 7 thru_hole oval (at 30.48 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole oval (at 35.56 0 180) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_08x5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F1DF)
    (at 53.34 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D1 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CN4-Pad1)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F1E4)
    (at 60.96 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D2 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(CN4-Pad2)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F1E6)
    (at 68.58 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D3 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CN4-Pad1)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F240)
    (at 76.2 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D4 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(CN4-Pad2)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F242)
    (at 83.82 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D5 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CN4-Pad1)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F244)
    (at 90.17 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D6 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(CN4-Pad2)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F24A)
    (at 104.14 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D7 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(CN4-Pad3)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F24D)
    (at 111.76 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D8 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(CN4-Pad4)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F236)
    (at 119.38 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D9 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(CN4-Pad3)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F234)
    (at 127 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D10 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(CN4-Pad4)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F231)
    (at 134.62 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D11 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(CN4-Pad3)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F257)
    (at 142.24 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D12 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(CN4-Pad4)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F266)
    (at 154.94 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D13 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(CN4-Pad5)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F270)
    (at 162.56 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D14 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(CN4-Pad6)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F276)
    (at 170.18 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D15 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(CN4-Pad5)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F296)
    (at 177.8 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D16 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(CN4-Pad6)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F28C)
    (at 185.42 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D17 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D17-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(CN4-Pad5)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:DO-214AB_Handsoldering (layer F.Cu) (tedit 57F8F27D)
    (at 193.04 102.87 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D18 (at -7.62 1.27 270) (layer F.SilkS))
    (fp_text value D (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(CN4-Pad6)"))
    (model Diodes_SMD.3dshapes/DO-214AB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 57.15 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(CN1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 60.96 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(CN1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 67.31 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CN1-Pad4)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 72.39 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CN1-Pad5)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 82.55 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN1-Pad7)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 87.63 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CN1-Pad8)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 102.87 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CN2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 107.95 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CN2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 118.11 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CN2-Pad4)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 123.19 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CN2-Pad5)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 133.35 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CN2-Pad7)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 138.43 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CN2-Pad8)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 153.67 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CN3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 158.75 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CN3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D14-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 168.91 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(CN3-Pad4)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 173.99 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CN3-Pad5)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D16-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 184.15 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(CN3-Pad7)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 189.23 113.03 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(CN3-Pad8)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BF0A)
    (at 97.79 114.3)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BF14)
    (at 52.07 114.3)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BF03)
    (at 148.59 114.3)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BEFA)
    (at 194.31 114.3)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BEC0)
    (at 52.07 83.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BECF)
    (at 102.87 83.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57F9BEE6)
    (at 194.31 83.82)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (fp_text reference REF** (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 4) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module graphics:pinout-legend2 (layer F.Cu) (tedit 0)
    (at 151.13 88.9)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module graphics:JCCC-LOGO1 (layer F.Cu) (tedit 0)
    (at 148.59 85.09)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module graphics:farsworth-sketch (layer B.Cu) (tedit 0)
    (at 115.57 99.06)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module graphics:boing-ball (layer B.Cu) (tedit 0)
    (at 63.5 102.87)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module graphics:standback-medium1 (layer B.Cu) (tedit 0)
    (at 170.18 95.25)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "10/2016 - RSH" (at 173.99 83.82) (layer F.SilkS))
  (gr_text "Switcher Tally Isolation Interface" (at 152.4 80.01) (layer F.SilkS))
  (gr_line (start 46.99 77.47) (end 46.99 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.39 77.47) (end 46.99 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.39 128.27) (end 199.39 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 46.99 128.27) (end 199.39 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.39 128.27) (xy 46.99 128.27) (xy 46.99 77.47) (xy 199.39 77.47)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.39 128.27) (xy 46.99 128.27) (xy 46.99 77.47) (xy 199.39 77.47)
      )
    )
  )
)
