(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 50)
    (no_connects 4)
    (area 210.109999 85.878788 239.470001 124.535001)
    (thickness 1.6)
    (drawings 14)
    (tracks 235)
    (zones 0)
    (modules 25)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.007874)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.015748)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.007874)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6002 1.6002)
    (pad_drill 1.6002)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 175.26 93.98)
    (grid_origin 175.26 93.98)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory out/origGerber/))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 /CH1)
  (net 4 /AO1)
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 "Net-(C6-Pad2)")
  (net 10 /AO2)
  (net 11 "Net-(C7-Pad2)")
  (net 12 /CH2)
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(J1-Pad5)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J1-Pad3)")
  (net 17 "Net-(J1-Pad2)")
  (net 18 "Net-(J2-Pad5)")
  (net 19 "Net-(J2-Pad4)")
  (net 20 +5V)
  (net 21 -5V)
  (net 22 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net -5V)
    (add_net /AO1)
    (add_net /AO2)
    (add_net /CH1)
    (add_net /CH2)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
  )
  (module friesw:Switchcraft_TRS_Jack_SMD (layer B.Cu) (tedit 56B948BC)
    (at 210.185 94.615)
    (descr 35RASMT4BHNTRX)
    (fp_text reference J2 (at 6.35 -3.81) (layer B.SilkS))
    (fp_text value JACK_TRS_5PINS (at 7.62 -7.62) (layer B.Fab))
    (pad 4 smd rect (at 15.7988 0.7366) (size 2.5908 2.6924) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 3 smd rect (at 4.2926 4.0005) (size 2.0066 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at 1.6002 4.0005) (size 2.0066 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J2-Pad5)"))
    (pad 2 smd rect (at 11.7094 -4.0005) (size 2.6924 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C6-Pad1)"))
    (pad "" thru_hole circle (at 10.5156 0) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask B.SilkS))
    (pad "" thru_hole circle (at 3.5052 0) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2.3876 -4.0005) (size 2.0066 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module friesw:Switchcraft_TRS_Jack_SMD (layer B.Cu) (tedit 56B948BC)
    (at 210.185 111.633)
    (descr 35RASMT4BHNTRX)
    (fp_text reference J1 (at 6.35 -3.81) (layer B.SilkS))
    (fp_text value JACK_TRS_5PINS (at 7.62 -7.62) (layer B.Fab))
    (pad 4 smd rect (at 15.7988 0.7366) (size 2.5908 2.6924) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 4.2926 4.0005) (size 2.0066 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at 1.6002 4.0005) (size 2.0066 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 11.7094 -4.0005) (size 2.6924 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad2)"))
    (pad "" thru_hole circle (at 10.5156 0) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask B.SilkS))
    (pad "" thru_hole circle (at 3.5052 0) (size 1.6002 1.6002) (drill 1.6002) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2.3876 -4.0005) (size 2.0066 2.1082) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:c_elec_6.3x7.7 (layer F.Cu) (tedit 56750BF5)
    (at 216.535 99.06)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (attr smd)
    (fp_text reference C1 (at 0 0) (layer F.SilkS))
    (fp_text value 220uF (at 0 4.318) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at -2.75082 0) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x7.7 (layer F.Cu) (tedit 56750BD9)
    (at 216.535 106.68 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (attr smd)
    (fp_text reference C2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 220uF (at 0 4.318 180) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 21 -5V))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:C_Rect_L7.2_W4.5_P5 (layer F.Cu) (tedit 56750C10)
    (at 236.855 92.075 270)
    (descr "Film Capacitor Length 7mm x Width 4.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 47pF (at 2.5 3.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /CH1))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /AO1))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W4.5_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:C_Rect_L7.2_W7.2_P5 (layer B.Cu) (tedit 56750C9C)
    (at 222.25 99.695 270)
    (descr WIMA_MKS2B042201F00)
    (tags Capacitor)
    (fp_text reference C4 (at 2.413 0.254 270) (layer B.SilkS))
    (fp_text value 2.2uF (at 2.286 -5.08 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:C_Rect_L7.2_W7.2_P5 (layer B.Cu) (tedit 56750C9F)
    (at 231.14 100.33 270)
    (descr WIMA_MKS2B042201F00)
    (tags Capacitor)
    (fp_text reference C5 (at 2.286 0 270) (layer B.SilkS))
    (fp_text value 2.2uF (at 2.286 -5.08 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 4 /AO1))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:C_Rect_L7.2_W7.2_P5 (layer F.Cu) (tedit 56750BEE)
    (at 226.695 100.33 270)
    (descr WIMA_MKS2B042201F00)
    (tags Capacitor)
    (fp_text reference C6 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 2.286 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C6-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:C_Rect_L7.2_W7.2_P5 (layer F.Cu) (tedit 56750BF0)
    (at 235.585 100.33 270)
    (descr WIMA_MKS2B042201F00)
    (tags Capacitor)
    (fp_text reference C7 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 2.286 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /AO2))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C7-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:C_Rect_L7.2_W4.5_P5 (layer B.Cu) (tedit 56750CA4)
    (at 233.045 92.075 270)
    (descr "Film Capacitor Length 7mm x Width 4.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 2.413 -0.127 270) (layer B.SilkS))
    (fp_text value 47pF (at 2.5 -3.5 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 12 /CH2))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 10 /AO2))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W4.5_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:LED-0805-HandSoldering (layer F.Cu) (tedit 56750C3E)
    (at 217.17 112.395)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at -0.254 -1.651) (layer F.SilkS))
    (fp_text value LED (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.19958 0 180) (size 1.5 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.19958 0 180) (size 1.5 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 21 -5V))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:SOIC-8-N-HandSoldering (layer F.Cu) (tedit 56750C0C)
    (at 226.06 95.25 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference P1 (at 0 0 90) (layer F.SilkS))
    (fp_text value DIL8 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 7 smd rect (at -0.635 -3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 10 /AO2))
    (pad 6 smd rect (at 0.635 -3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 12 /CH2))
    (pad 5 smd rect (at 1.905 -3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 21 -5V))
    (pad 3 smd rect (at 0.635 3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.635 3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /CH1))
    (pad 1 smd rect (at -1.905 3.4785 90) (size 0.508 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /AO1))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56750CDB)
    (at 213.995 104.775 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.429 2.159 180) (layer B.SilkS))
    (fp_text value 100k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56750CD6)
    (at 213.995 102.235)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.429 2.921) (layer B.SilkS))
    (fp_text value 100k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 -5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 56750BCF)
    (at 217.17 114.935 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 56750C2B)
    (at 215.9 93.345 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0.635 -1.905 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /CH1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56750CB8)
    (at 238.125 94.615 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -0.127 1.651 270) (layer B.SilkS))
    (fp_text value 390k (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /CH1))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /AO1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 56750BFF)
    (at 218.44 93.345 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0.635 1.905 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /CH2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 56750C14)
    (at 231.775 94.615 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 390k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /CH2))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /AO2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:LED-0805-HandSoldering (layer B.Cu) (tedit 56B951ED)
    (at 237.49 112.395 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at -0.127 -1.524 90) (layer B.SilkS))
    (fp_text value LED (at 0 -1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.19958 0 270) (size 1.5 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.19958 0 270) (size 1.5 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 21 -5V))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56750CC2)
    (at 229.235 109.22 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 1.016 -1.778 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module friesw:9V_Battery_Snaps (layer F.Cu) (tedit 56B950B4)
    (at 231.14 122.555 180)
    (descr "Keystone 593 & 594")
    (fp_text reference BT1 (at 23.495 4.445 180) (layer F.SilkS))
    (fp_text value 9V (at 0 6.35 180) (layer F.Fab))
    (fp_text user "\\/ Edge of PCB \\/" (at 6.35 -3.81 180) (layer F.SilkS))
    (fp_text user - (at 12.7 2.54 180) (layer F.SilkS))
    (fp_text user + (at 0 2.54 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 17.3355 2.9972 180) (size 3 3) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 21 -5V))
    (pad 2 thru_hole circle (at 8.0645 2.9972 180) (size 3 3) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 21 -5V))
    (pad 2 thru_hole circle (at 12.7 0 180) (size 3 3) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 21 -5V))
    (pad 1 thru_hole circle (at 4.6355 2.9972 180) (size 3 3) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at -4.6355 2.9972 180) (size 3 3) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BT1-Pad1)"))
  )
  (module friesw:Dual_Switched_Pot (layer F.Cu) (tedit 56777FBB)
    (at 239.395 112.395 270)
    (descr APLS_RK0971221Z05)
    (fp_text reference RV1 (at 0 16.764 270) (layer F.SilkS))
    (fp_text value DUAL_SWITCHED_POT (at -0.762 -6.858 270) (layer F.Fab))
    (fp_text user P1H (at -2.54 2.54 360) (layer F.SilkS))
    (fp_text user P1W (at 0 2.54 360) (layer F.SilkS))
    (fp_text user P1L (at 2.54 2.54 360) (layer F.SilkS))
    (fp_text user P2H (at -2.54 10.16 360) (layer F.SilkS))
    (fp_text user P2L (at 2.54 10.16 360) (layer F.SilkS))
    (fp_text user P2W (at 0 10.16 360) (layer F.SilkS))
    (fp_text user SW (at 4.064 13.716 360) (layer F.SilkS))
    (fp_text user SW (at -4.064 13.716 360) (layer F.SilkS))
    (pad 6 thru_hole circle (at 2.5 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at -2.5 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad2)"))
    (pad 7 thru_hole circle (at -2.5 13.75 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 +5V))
    (pad 5 thru_hole circle (at 0 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad2)"))
    (pad 8 thru_hole circle (at 2.5 13.75 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at -2.5 5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C7-Pad2)"))
  )
  (module friesw:INDUCTOR_V_WO_CIRCLE (layer F.Cu) (tedit 56B95147)
    (at 217.805 88.265 20)
    (descr "Inductor (vertical)")
    (tags INDUCTOR)
    (fp_text reference L1 (at 0 0 20) (layer F.SilkS))
    (fp_text value 22mH (at 0.09906 -1.99898 20) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 20) (size 1.905 1.905) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 20) (size 1.905 1.905) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J2-Pad5)"))
  )
  (module friesw:INDUCTOR_V_WO_CIRCLE (layer F.Cu) (tedit 56B95147)
    (at 231.775 88.265 160)
    (descr "Inductor (vertical)")
    (tags INDUCTOR)
    (fp_text reference L2 (at 0 0 160) (layer F.SilkS))
    (fp_text value 22mH (at 0.09906 -1.99898 160) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 160) (size 1.905 1.905) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 160) (size 1.905 1.905) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J2-Pad4)"))
  )
  (gr_text "CC BY-NC-SA Jonas Gruska of LOM Instruments" (at 224.663 117.094) (layer B.SilkS))
  (gr_line (start 239.395 89.535) (end 239.395 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.125 88.265) (end 235.585 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.125 88.265) (end 239.395 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.125 124.46) (end 211.455 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.125 124.46) (end 239.395 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.185 123.19) (end 210.185 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.185 123.19) (end 211.455 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 211.455 88.265) (end 213.995 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.185 89.535) (end 211.455 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "PCB layout William Fries\ngithub.com/FriesW/" (at 237.744 103.124 270) (layer B.SilkS))
  (gr_line (start 229.235 85.953789) (end 235.585 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 220.345 85.953789) (end 213.995 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 220.345 85.953789) (end 229.235 85.953789) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 241.935 124.46) (xy 206.375 124.46) (xy 206.375 79.375) (xy 246.38 78.74) (xy 243.84 123.19)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 246.38 126.365) (xy 202.565 127) (xy 201.295 81.915) (xy 242.57 82.55) (xy 245.11 120.015)
      )
    )
  )
)
