(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 68)
    (no_connects 0)
    (area 96.52 46.355 156.399999 81.836)
    (thickness 1.6)
    (drawings 21)
    (tracks 435)
    (zones 0)
    (modules 40)
    (nets 20)
  )
  (page A4)
  (title_block
    (title upRTL)
    (date 2018-03-01)
    (rev 1)
    (company "1rel interactive")
  )
  (layers
    (0 F.SIG1 signal)
    (31 B.SIG2 signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.35044)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.812917)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.35)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUT/gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RF_IN)
  (net 3 "Net-(C102-Pad1)")
  (net 4 "Net-(C104-Pad1)")
  (net 5 /RF_IF)
  (net 6 "Net-(C107-Pad1)")
  (net 7 "Net-(C109-Pad2)")
  (net 8 "Net-(C110-Pad1)")
  (net 9 "Net-(C111-Pad2)")
  (net 10 /RF_OUT)
  (net 11 /LO)
  (net 12 +3.3V)
  (net 13 +5V)
  (net 14 "Net-(GS102-Pad2)")
  (net 15 /RF_MIX)
  (net 16 "Net-(U103-Pad4)")
  (net 17 "Net-(XO101-Pad1)")
  (net 18 "Net-(C113-Pad1)")
  (net 19 "Net-(R101-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U103-Pad4)")
    (add_net "Net-(XO101-Pad1)")
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.35)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net +5V)
    (add_net "Net-(GS102-Pad2)")
  )
  (net_class RF ""
    (clearance 0.1524)
    (trace_width 0.812917)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LO)
    (add_net /RF_IF)
    (add_net /RF_IN)
    (add_net /RF_MIX)
    (add_net /RF_OUT)
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(C107-Pad1)")
    (add_net "Net-(C109-Pad2)")
    (add_net "Net-(C110-Pad1)")
    (add_net "Net-(C111-Pad2)")
    (add_net "Net-(C113-Pad1)")
    (add_net "Net-(R101-Pad1)")
  )
  (module mylib:HO-25B (layer F.SIG1) (tedit 5A974608)
    (at 142.494 68.072 90)
    (fp_text reference XO101 (at 0 7.366 270) (layer F.SilkS))
    (fp_text value HO-25B (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 8 thru_hole circle (at -3.81 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 +3.3V))
    (pad 1 thru_hole circle (at -3.81 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(XO101-Pad1)"))
    (pad 5 thru_hole circle (at 3.81 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(R101-Pad1)"))
    (pad 4 thru_hole circle (at 3.81 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mylib:ADE-1 (layer F.SIG1) (tedit 5A97462A)
    (at 121.539 68.707 270)
    (fp_text reference U101 (at 4.572 -0.127 360) (layer F.SilkS))
    (fp_text value ADE-1 (at 0 -0.5 270) (layer F.Fab) hide)
    (pad 6 smd rect (at -2.54 -2.54 270) (size 1.65 2.54) (layers F.SIG1 F.Paste F.Mask)
      (net 11 /LO))
    (pad 5 smd rect (at 0 -2.54 270) (size 1.65 2.54) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.54 -2.54 270) (size 1.65 2.54) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.54 2.54 270) (size 1.65 2.54) (layers F.SIG1 F.Paste F.Mask)
      (net 15 /RF_MIX))
    (pad 2 smd rect (at 0 2.54 270) (size 1.65 2.54) (layers F.SIG1 F.Paste F.Mask)
      (net 5 /RF_IF))
    (pad 1 smd rect (at -2.54 2.54 270) (size 1.65 2.54) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A958443)
    (at 111.76 76.454 270)
    (descr "Inductor SMD, 0805")
    (fp_text reference L104 (at 2.794 0 360) (layer F.SilkS))
    (fp_text value 39n (at 2.794 1.524 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0 270) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 7 "Net-(C109-Pad2)"))
    (pad 2 smd rect (at 0.889 0 270) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.SIG1) (tedit 5A91D688)
    (at 139.7 77.47)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P103 (at 0 -2.032) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 +3.3V))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.SIG1) (tedit 5A91D68B)
    (at 142.24 77.47 180)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P104 (at 0 2.032 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745DF)
    (at 108.204 67.564 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C101 (at -3.048 -0.635 180) (layer F.SilkS))
    (fp_text value 100p (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 2 /RF_IN))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745E5)
    (at 109.22 62.992)
    (descr "SMT capacitor, 0603")
    (fp_text reference C102 (at -0.254 -2.286) (layer F.SilkS))
    (fp_text value 10p (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 2 /RF_IN))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745E1)
    (at 110.744 67.564 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C103 (at -3.048 -0.254 180) (layer F.SilkS))
    (fp_text value 150p (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745E6)
    (at 112.268 62.992)
    (descr "SMT capacitor, 0603")
    (fp_text reference C104 (at 0.127 -2.286) (layer F.SilkS))
    (fp_text value 33p (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 4 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745E2)
    (at 113.284 67.564 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C105 (at -3.048 0.254 180) (layer F.SilkS))
    (fp_text value 100p (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 4 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A970A82)
    (at 115.697 65.786 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C106 (at 2.286 -1.143 270) (layer F.SilkS))
    (fp_text value 10n (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 5 /RF_IF))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 4 "Net-(C104-Pad1)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745D7)
    (at 115.57 74.168 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C107 (at -0.127 1.778 180) (layer F.SilkS))
    (fp_text value 100p (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 15 /RF_MIX))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9584EB)
    (at 116.078 76.454 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C108 (at 1.8796 -1.2192 270) (layer F.SilkS))
    (fp_text value 12p (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745D9)
    (at 113.03 74.168)
    (descr "SMT capacitor, 0603")
    (fp_text reference C109 (at -0.254 -1.778) (layer F.SilkS))
    (fp_text value 15p (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 7 "Net-(C109-Pad2)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A970A5C)
    (at 131.826 63.246 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C110 (at -3.1115 0.254 450) (layer F.SilkS))
    (fp_text value 20p (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 8 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745DA)
    (at 110.49 74.168)
    (descr "SMT capacitor, 0603")
    (fp_text reference C111 (at -0.508 -1.778) (layer F.SilkS))
    (fp_text value 15p (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 7 "Net-(C109-Pad2)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 9 "Net-(C111-Pad2)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9745DC)
    (at 107.95 74.168)
    (descr "SMT capacitor, 0603")
    (fp_text reference C112 (at -0.889 -1.778) (layer F.SilkS))
    (fp_text value 33p (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 9 "Net-(C111-Pad2)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 10 /RF_OUT))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0603 (layer F.SIG1) (tedit 5A9709C7)
    (at 134.874 62.611 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R101 (at -2.3495 -1.27 360) (layer F.SilkS))
    (fp_text value 160R (at 0 0.6096 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 19 "Net-(R101-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0603 (layer F.SIG1) (tedit 5A9709B4)
    (at 134.112 64.77)
    (descr "SMT resistor, 0603")
    (fp_text reference R102 (at -0.1905 2.6035) (layer F.SilkS))
    (fp_text value 36R (at 0 0.6096) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 19 "Net-(R101-Pad1)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 8 "Net-(C110-Pad1)"))
    (model walter/smd_resistors/r_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0603 (layer F.SIG1) (tedit 5A9709CB)
    (at 133.35 62.611 270)
    (descr "SMT resistor, 0603")
    (fp_text reference R103 (at -2.667 -0.6985 450) (layer F.SilkS))
    (fp_text value 160R (at 0 0.6096 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 8 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.SIG1) (tedit 5A91D686)
    (at 129.54 77.47)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P105 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.SIG1) (tedit 5A974621)
    (at 129.54 73.152 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C114 (at -0.127 -1.524 270) (layer F.SilkS))
    (fp_text value 10u (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.SIG1 F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.SIG1) (tedit 5A970E11)
    (at 133.858 70.7136)
    (descr "SMT capacitor, 0805")
    (fp_text reference C115 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 10u (at 0 0.9906) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0) (size 1.30048 1.4986) (layers F.SIG1 F.Paste F.Mask)
      (net 12 +3.3V))
    (pad 2 smd rect (at -0.9525 0) (size 1.30048 1.4986) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.SIG1) (tedit 5A91D684)
    (at 132.08 77.47)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P106 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:solder_bridge (layer F.SIG1) (tedit 5A933900)
    (at 134.874 72.39)
    (fp_text reference GS102 (at 2.413 -0.127) (layer F.SilkS) hide)
    (fp_text value GS2 (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.45 0) (size 0.7 0.8001) (layers F.SIG1 F.Paste F.Mask)
      (net 12 +3.3V))
    (pad 2 smd rect (at -0.45 0) (size 0.7 0.8001) (layers F.SIG1 F.Paste F.Mask)
      (net 14 "Net-(GS102-Pad2)"))
  )
  (module w_smd_trans:sot23-5 (layer F.SIG1) (tedit 5A970E0C)
    (at 132.334 73.406 270)
    (descr SOT23-5)
    (fp_text reference U103 (at 2.032 -0.508 360) (layer F.SilkS))
    (fp_text value AP2112 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 13 +5V))
    (pad 3 smd rect (at 0.9525 1.05664 270) (size 0.59944 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 0 1.05664 270) (size 0.59944 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.9525 -1.05664 270) (size 0.59944 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 16 "Net-(U103-Pad4)"))
    (pad 5 smd rect (at -0.9525 -1.05664 270) (size 0.59944 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 14 "Net-(GS102-Pad2)"))
    (model walter/smd_trans/sot23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A958441)
    (at 114.3 76.454 270)
    (descr "Inductor SMD, 0805")
    (fp_text reference L103 (at 2.794 0 360) (layer F.SilkS))
    (fp_text value 39n (at 2.794 2.032 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0 270) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 0.889 0 270) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A958434)
    (at 109.22 76.454 270)
    (descr "Inductor SMD, 0805")
    (fp_text reference L105 (at 2.794 0 360) (layer F.SilkS))
    (fp_text value 39n (at 0 1.80086 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0 270) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 9 "Net-(C111-Pad2)"))
    (pad 2 smd rect (at 0.889 0 270) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A974615)
    (at 109.22 65.024)
    (descr "Inductor SMD, 0805")
    (fp_text reference L101 (at -2.159 -0.508 90) (layer F.SilkS))
    (fp_text value 390n (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 2 /RF_IN))
    (pad 2 smd rect (at 0.889 0) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A9584D7)
    (at 112.268 65.024)
    (descr "Inductor SMD, 0805")
    (fp_text reference L102 (at 2.7432 -2.9464 90) (layer F.SilkS))
    (fp_text value 330n (at 0.254 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 0.889 0) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 4 "Net-(C104-Pad1)"))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:mounting_hole0 (layer F.SIG1) (tedit 5A958496)
    (at 152.4 76.835)
    (descr "Hole 4mm")
    (fp_text reference H102 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value mounting_hole (at 0 3.429) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.0005) (layers *.Cu *.Mask)
      (net 1 GND))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:mounting_hole0 (layer F.SIG1) (tedit 5A95848D)
    (at 122.809 76.835)
    (descr "Hole 4mm")
    (fp_text reference H104 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value mounting_hole (at 0 3.429) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.0005) (layers *.Cu *.Mask)
      (net 1 GND))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9709B1)
    (at 130.429 65.532 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C113 (at -0.5715 -1.9685 180) (layer F.SilkS))
    (fp_text value 10p (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 18 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 8 "Net-(C110-Pad1)"))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:mounting_hole0 (layer F.SIG1) (tedit 5A96D254)
    (at 152.4 61.595)
    (descr "Hole 4mm")
    (fp_text reference H103 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value mounting_hole (at 0 3.429) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.0005) (layers *.Cu *.Mask)
      (net 1 GND))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A970996)
    (at 129.9845 62.2935 90)
    (descr "Inductor SMD, 0805")
    (fp_text reference L106 (at 2.0955 -1.5875 180) (layer F.SilkS))
    (fp_text value 120n (at 0 1.80086 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0 90) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 8 "Net-(C110-Pad1)"))
    (pad 2 smd rect (at 0.889 0 90) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0805 (layer F.SIG1) (tedit 5A970E1E)
    (at 127.254 65.532 180)
    (descr "Inductor SMD, 0805")
    (fp_text reference L107 (at -1.27 -3.048 180) (layer F.SilkS))
    (fp_text value 150n (at 0 1.80086 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 0 180) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 18 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at 0.889 0 180) (size 1.016 1.778) (layers F.SIG1 F.Paste F.Mask)
      (net 11 /LO))
    (model walter/smd_inductors/inductor_smd_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:mounting_hole0 (layer F.SIG1) (tedit 5A96F871)
    (at 122.809 61.595)
    (descr "Hole 4mm")
    (fp_text reference H101 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value mounting_hole (at 0 3.429) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.0005) (layers *.Cu *.Mask)
      (net 1 GND))
    (model walter/details/hole.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:sma-side-connector (layer F.SIG1) (tedit 5A974634)
    (at 100.33 74.93 270)
    (fp_text reference P102 (at 4.318 -2.54 540) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 2.5 -2.5 270) (size 2 5) (layers F.SIG1 F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.5 -2.5 270) (size 2 5) (layers F.SIG1 F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -2.5 270) (size 1.5 5) (layers F.SIG1 F.Mask)
      (net 10 /RF_OUT))
    (pad 2 smd rect (at 2.5 -2.5 270) (size 2 5) (layers B.SIG2 B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.5 -2.5 270) (size 2 5) (layers B.SIG2 B.Mask)
      (net 1 GND))
  )
  (module mylib:sma-side-connector (layer F.SIG1) (tedit 5A970770)
    (at 100.33 63.5 270)
    (fp_text reference P101 (at -4.2672 -2.6416 540) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 -6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 2.5 -2.5 270) (size 2 5) (layers F.SIG1 F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.5 -2.5 270) (size 2 5) (layers F.SIG1 F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -2.5 270) (size 1.5 5) (layers F.SIG1 F.Mask)
      (net 2 /RF_IN))
    (pad 2 smd rect (at 2.5 -2.5 270) (size 2 5) (layers B.SIG2 B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.5 -2.5 270) (size 2 5) (layers B.SIG2 B.Mask)
      (net 1 GND))
  )
  (module w_smd_cap:c_0603 (layer F.SIG1) (tedit 5A9753EC)
    (at 135.128 74.295 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C116 (at -2.0574 1.1684 90) (layer F.SilkS))
    (fp_text value 10n (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 12 +3.3V))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.SIG1 F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 155.575 58.42) (end 100.33 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 80.01) (end 155.575 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "RF OUT" (at 101.7016 70.6628) (layer F.SilkS))
  (gr_text "ANT IN" (at 100.7872 67.818) (layer F.SilkS))
  (gr_text "upRTL rev1\nrel/2018-03" (at 147.447 60.3885) (layer B.SilkS))
  (gr_line (start 100.33 80.01) (end 100.33 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.575 58.42) (end 155.575 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 134.112 78.486 90) (layer F.SilkS))
  (gr_text 3V3 (at 137.668 78.486 90) (layer F.SilkS))
  (gr_text GND (at 144.272 78.613 90) (layer F.SilkS))
  (gr_text 5V (at 127.508 76.835 90) (layer B.SilkS))
  (gr_text 5V (at 127.508 78.232 90) (layer F.SilkS))
  (gr_text 3V3 (at 137.668 76.708 90) (layer B.SilkS))
  (gr_text GND (at 134.112 76.327 90) (layer B.SilkS))
  (gr_text GND (at 144.272 76.581 90) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 149.86 73.66) (xy 96.52 73.66) (xy 96.52 46.355) (xy 149.86 46.355)
      )
    )
  )
  (zone (net 12) (net_name +3.3V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 149.86 73.66) (xy 96.52 73.66) (xy 96.52 46.355) (xy 149.86 46.355)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 145.034 48.895) (xy 139.7 48.895) (xy 139.7 46.355) (xy 145.034 46.355)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 145.034 48.895) (xy 141.478 48.895) (xy 141.478 46.355) (xy 145.034 46.355)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.SIG1) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 155.575 80.01) (xy 100.33 80.01) (xy 100.33 58.42) (xy 155.575 58.42)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.SIG2) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 155.575 80.01) (xy 100.33 80.01) (xy 100.33 58.42) (xy 155.575 58.42)
      )
    )
  )
)
