(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 12)
    (no_connects 0)
    (area 137.592999 94.412999 163.651001 113.867001)
    (thickness 1.6)
    (drawings 10)
    (tracks 39)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 sig1)
  (net 3 sig2)
  (net 4 sig3)
  (net 5 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.15)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net sig1)
    (add_net sig2)
    (add_net sig3)
  )
  (module RJ45:EJ45_RJHSE-5080 (layer F.Cu) (tedit 58771648)
    (at 153.924 97.536 270)
    (fp_text reference J1 (at 6.51002 3.79476 270) (layer F.SilkS))
    (fp_text value RJ45 (at 6.62178 -8.3312 270) (layer F.Fab))
    (fp_text user RJ45 (at 6.35 1.905 270) (layer F.SilkS))
    (pad 8 thru_hole circle (at 2.794 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 7 thru_hole circle (at 3.81 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 6 thru_hole circle (at 4.826 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 4 thru_hole circle (at 6.858 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 8.89 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole circle (at 5.842 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 sig3))
    (pad 3 thru_hole circle (at 7.874 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 sig2))
    (pad 1 thru_hole circle (at 9.906 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 sig1))
    (pad "" thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 587A4B1C)
    (at 144.78 96.52 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference A (at -0.127 -2.6035 360) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 sig1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 587A4B22)
    (at 144.78 104.14 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference B (at 0 -2.7305 360) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 sig2))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 587A4B27)
    (at 144.78 111.76 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference C (at 0.127 -2.6035 360) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 sig3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "v0.2\n3xDIO/PWM\n/ANALOG" (at 150.622 103.886 270) (layer B.SilkS))
  (gr_text FRC2168 (at 160.782 103.886 270) (layer B.SilkS))
  (gr_text 3xDIO/PWM/AN (at 137.668 99.314 350) (layer F.SilkS))
  (gr_text Sig (at 145.288 108.077 270) (layer F.SilkS))
  (gr_text 5V (at 142.24 107.95 270) (layer F.SilkS))
  (gr_text Gnd (at 139.7 108.077 270) (layer F.SilkS))
  (gr_line (start 137.668 113.792) (end 137.668 94.488) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 113.792) (end 137.668 113.792) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 94.488) (end 163.576 113.792) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 94.488) (end 163.576 94.488) (angle 90) (layer Edge.Cuts) (width 0.15))
)
