<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="26.035" y1="67.437" x2="10.795" y2="67.437" width="0" layer="20"/>
<wire x1="10.795" y1="67.437" x2="10.16" y2="66.802" width="0" layer="20" curve="90"/>
<wire x1="10.16" y1="66.802" x2="10.16" y2="50.038" width="0" layer="20"/>
<wire x1="10.16" y1="50.038" x2="10.795" y2="49.403" width="0" layer="20" curve="90"/>
<wire x1="10.795" y1="49.403" x2="26.035" y2="49.403" width="0" layer="20"/>
<wire x1="26.035" y1="49.403" x2="26.67" y2="50.038" width="0" layer="20" curve="90"/>
<wire x1="26.67" y1="50.038" x2="26.67" y2="66.802" width="0" layer="20"/>
<wire x1="26.67" y1="66.802" x2="26.035" y2="67.437" width="0" layer="20" curve="90"/>
<text>HPMA115S0-XXX
breakout</text>
<text>NC</text>
<text>RX</text>
<text>TX</text>
<text>VCC</text>
<text>3.3V</text>
<text>GND</text>
<text>@0x76656e</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-molex-picoblade">
<description>&lt;b&gt;MOLEX PicoBlade Series Connectors&lt;/b&gt; - v1.01 (09/07/2010)&lt;p&gt;
1.25MM (0.05") Wire-To-Board Connectors&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2010, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="53398-0810">
<description>&lt;b&gt;HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="P1" library="con-molex-picoblade" package="53398-0810" value="53398-0810"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="6"/>
<contactref element="P1" pad="8"/>
</signal>
<signal name="RX">
<contactref element="P1" pad="7"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="P1" pad="6"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="P1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="P1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="NC">
<contactref element="P1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
