(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 5)
    (no_connects 3)
    (area 144.704999 93.904999 152.475001 114.375001)
    (thickness 1.6)
    (drawings 15)
    (tracks 10)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page USLetter)
  (title_block
    (title "Neopixel WS2812B Breakout Board")
    (date "1 Sep 2016")
    (rev v1.0)
    (company "CERN Open Hardware License v1.2")
    (comment 1 jenner@wickerbox.net)
    (comment 2 http://wickerbox.net)
    (comment 3 "Wickerbox Electronics")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x3d0fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /DO)
  (net 3 /DI)
  (net 4 GND)
  (net 5 "Net-(LED1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /DI)
    (add_net /DO)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(LED1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.3302)
    (trace_width 0.508)
    (via_dia 0.762)
    (via_drill 0.4064)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x02 (layer F.Cu) (tedit 57C8B9F5)
    (at 149.86 111.76 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 1.25 360) (layer F.Fab))
    (fp_text value INPUT (at 0 -3.1 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.334 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /DI))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x02 (layer F.Cu) (tedit 57C8B9F8)
    (at 149.86 96.52 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 1.25 360) (layer F.Fab))
    (fp_text value OUTPUT (at 0 -3.1 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.334 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /DO))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 147.447 107.696 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R1 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 470 (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at -2.794 -0.127 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /DI))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(LED1-Pad2)"))
  )
  (module Wickerlib:LED-RGB-5050-SMD (layer F.Cu) (tedit 57C8BD40)
    (at 148.7424 102.9462 180)
    (fp_text reference LED1 (at 0.025 0 180) (layer F.Fab))
    (fp_text value WS2812B (at 0.025 0.05 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.1 -3.302 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.4384 1.651 180) (size 1.4986 0.889) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2.4384 -1.651 180) (size 1.4986 0.889) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(LED1-Pad2)"))
    (pad 3 smd rect (at -2.4384 -1.651 180) (size 1.4986 0.889) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (pad 4 smd rect (at -2.4384 1.651 180) (size 1.4986 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 /DO))
  )
  (gr_text 2/7/17 (at 148.59 116.332) (layer F.Fab))
  (gr_text "RGB5050 Neopixel\nBreakout v1.1" (at 149.098 91.186) (layer F.Fab))
  (gr_text "WS2812B\nNeopixel\nBreakout" (at 148.5265 104.0765 90) (layer B.SilkS))
  (gr_text DO (at 150.368 98.9965) (layer F.SilkS))
  (gr_text GND (at 147.066 98.933) (layer F.SilkS))
  (gr_text DI (at 146.939 109.4105) (layer F.SilkS))
  (gr_text VCC (at 150.368 109.347) (layer F.SilkS))
  (gr_line (start 144.78 93.98) (end 152.4 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 114.3) (end 144.78 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 114.3) (end 144.78 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 93.98) (end 152.4 114.3) (layer Edge.Cuts) (width 0.15))
)
