(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 87)
    (no_connects 0)
    (area 20.244999 46.914999 88.975001 100.405001)
    (thickness 1.6)
    (drawings 79)
    (tracks 403)
    (zones 0)
    (modules 31)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.300387)
    (user_trace_width 0.781437)
    (user_trace_width 1.36703)
    (user_trace_width 2.03286)
    (user_trace_width 2.76552)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.44 1.12)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 Din1)
  (net 4 Din2)
  (net 5 /SS)
  (net 6 "Net-(M1-Pad3)")
  (net 7 /INT/SQW)
  (net 8 "Net-(M1-Pad6)")
  (net 9 /VBATT)
  (net 10 /MOSI)
  (net 11 /SCLK)
  (net 12 /MISO)
  (net 13 "Net-(SHIELD1-PadAD5)")
  (net 14 "Net-(SHIELD1-PadAD4)")
  (net 15 "Net-(SHIELD1-PadV_IN)")
  (net 16 "Net-(SHIELD1-Pad3V3)")
  (net 17 "Net-(SHIELD1-PadRST)")
  (net 18 "Net-(SHIELD1-Pad0)")
  (net 19 "Net-(SHIELD1-Pad1)")
  (net 20 GSM_RX)
  (net 21 GSM_TX)
  (net 22 GSM_reset)
  (net 23 "Net-(SHIELD1-PadGND3)")
  (net 24 "Net-(SHIELD1-PadAREF)")
  (net 25 "Net-(SHIELD1-PadSDA)")
  (net 26 "Net-(SHIELD1-PadSCL)")
  (net 27 "Net-(SHIELD1-PadIO_R)")
  (net 28 "Net-(SHIELD1-PadNC)")
  (net 29 "Net-(SHIELD1-PadSP1)")
  (net 30 "Net-(SHIELD1-PadSP2)")
  (net 31 "Net-(SHIELD1-PadSP3)")
  (net 32 "Net-(SHIELD1-PadSP4)")
  (net 33 "Net-(SHIELD1-PadSP5)")
  (net 34 "Net-(SHIELD1-PadSP6)")
  (net 35 "Net-(J2-Pad1)")
  (net 36 "Net-(JP1-Pad2)")
  (net 37 Ain1)
  (net 38 "Net-(JP2-Pad2)")
  (net 39 Ain2)
  (net 40 /OPA_input_1/in)
  (net 41 /OPA_input_2/in)
  (net 42 "Net-(D1_on1-Pad2)")
  (net 43 "Net-(D2_on1-Pad2)")
  (net 44 "Net-(J1-Pad1)")
  (net 45 "Net-(R1_2-Pad2)")
  (net 46 "Net-(R2_2-Pad2)")
  (net 47 Alarm_out)
  (net 48 "Net-(D1-Pad1)")
  (net 49 "Net-(JP3-Pad2)")
  (net 50 Alarm_enable)
  (net 51 "Net-(SHIELD1-PadAD3)")
  (net 52 "Net-(SHIELD1-PadAD2)")
  (net 53 "Net-(D1_off1-Pad2)")
  (net 54 "Net-(D2_off1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /INT/SQW)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /OPA_input_1/in)
    (add_net /OPA_input_2/in)
    (add_net /SCLK)
    (add_net /SS)
    (add_net /VBATT)
    (add_net Ain1)
    (add_net Ain2)
    (add_net Alarm_enable)
    (add_net Alarm_out)
    (add_net Din1)
    (add_net Din2)
    (add_net GND)
    (add_net GSM_RX)
    (add_net GSM_TX)
    (add_net GSM_reset)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1_off1-Pad2)")
    (add_net "Net-(D1_on1-Pad2)")
    (add_net "Net-(D2_off1-Pad2)")
    (add_net "Net-(D2_on1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(R1_2-Pad2)")
    (add_net "Net-(R2_2-Pad2)")
    (add_net "Net-(SHIELD1-Pad0)")
    (add_net "Net-(SHIELD1-Pad1)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-PadAD2)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadGND3)")
    (add_net "Net-(SHIELD1-PadIO_R)")
    (add_net "Net-(SHIELD1-PadNC)")
    (add_net "Net-(SHIELD1-PadRST)")
    (add_net "Net-(SHIELD1-PadSCL)")
    (add_net "Net-(SHIELD1-PadSDA)")
    (add_net "Net-(SHIELD1-PadSP1)")
    (add_net "Net-(SHIELD1-PadSP2)")
    (add_net "Net-(SHIELD1-PadSP3)")
    (add_net "Net-(SHIELD1-PadSP4)")
    (add_net "Net-(SHIELD1-PadSP5)")
    (add_net "Net-(SHIELD1-PadSP6)")
    (add_net "Net-(SHIELD1-PadV_IN)")
  )
  (net_class 1A ""
    (clearance 0.1524)
    (trace_width 0.300387)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net VCC)
  )
  (net_class 2A ""
    (clearance 0.1524)
    (trace_width 0.781437)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class 3A ""
    (clearance 0.1524)
    (trace_width 1.36703)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class 4A ""
    (clearance 0.1524)
    (trace_width 2.03286)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class 5A ""
    (clearance 0.1524)
    (trace_width 2.76552)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 59083423)
    (at 83.82 83.82)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J_ALARM/SQW1 (at 0 -5) (layer F.SilkS) hide)
    (fp_text value CONN_COAXIAL (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 49 "Net-(JP3-Pad2)"))
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 58C301F2)
    (at 25.4 77.47)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J2 (at 0 -5) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (model /Users/luis/Desktop/CellularSafetyBoard/sma_angled.wrl
      (at (xyz -0.435 0 0.2854330709))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz -90 0 90))
    )
  )
  (module kicad_footprints_lsrggr:ARDUINO_UNO_SHIELD locked (layer F.Cu) (tedit 0)
    (at 20.32 100.33)
    (fp_text reference SHIELD1 (at 5.715 -57.15) (layer F.SilkS))
    (fp_text value ARDUINO_SHIELD (at 10.16 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 Ain1))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 Ain2))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(SHIELD1-PadAD2)"))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SHIELD1-PadV_IN)"))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SHIELD1-PadRST)"))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(SHIELD1-Pad0)"))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SHIELD1-Pad1)"))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 GSM_RX))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 GSM_TX))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 Din1))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 Din2))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 Alarm_enable))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GSM_reset))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 Alarm_out))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /INT/SQW))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SS))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MOSI))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /MISO))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCLK))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(SHIELD1-PadGND3)"))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad "" np_thru_hole circle (at 66.04 -7.62 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 66.04 -35.56 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 15.24 -50.8 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 13.97 -2.54 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad SDA thru_hole oval (at 21.336 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-PadSDA)"))
    (pad SCL thru_hole oval (at 18.796 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-PadSCL)"))
    (pad IO_R thru_hole oval (at 30.48 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(SHIELD1-PadIO_R)"))
    (pad NC thru_hole oval (at 27.94 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(SHIELD1-PadNC)"))
    (pad SP1 thru_hole circle (at 63.5 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(SHIELD1-PadSP1)"))
    (pad SP2 thru_hole circle (at 66.04 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(SHIELD1-PadSP2)"))
    (pad SP3 thru_hole circle (at 63.5 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SHIELD1-PadSP3)"))
    (pad SP4 thru_hole circle (at 66.04 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(SHIELD1-PadSP4)"))
    (pad SP5 thru_hole circle (at 63.5 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(SHIELD1-PadSP5)"))
    (pad SP6 thru_hole circle (at 66.04 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(SHIELD1-PadSP6)"))
  )
  (module kicad_footprints_lsrggr:S8201-46R (layer F.Cu) (tedit 58F4E1F8)
    (at 25.4 58.65 270)
    (fp_text reference BT1 (at 0 3.81 270) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -7.85 0 270) (size 3.7 3.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBATT))
    (pad 1 smd rect (at 7.85 0 270) (size 3.7 3.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBATT))
    (pad 2 smd rect (at 0 0 270) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 44.831 68.03 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 58.97 93.98)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 3.26 0.127) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-FreqCtrl:DS3234 (layer F.Cu) (tedit 59085F96)
    (at 46.355 58.42)
    (attr smd)
    (fp_text reference M1 (at -7.493 -0.635 90) (layer F.SilkS))
    (fp_text value DS3234 (at 8.128 0.254 90) (layer F.SilkS))
    (pad 1 smd rect (at -5.715 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 5 /SS))
    (pad 2 smd rect (at -4.445 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.175 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-Pad3)"))
    (pad 4 smd rect (at -1.905 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 5 smd rect (at -0.635 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 7 /INT/SQW))
    (pad 6 smd rect (at 0.635 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-Pad6)"))
    (pad 7 smd rect (at 1.905 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.175 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.445 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 5.715 4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 5.715 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.445 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 3.175 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 1.905 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 0.635 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.635 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBATT))
    (pad 17 smd rect (at -1.905 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 10 /MOSI))
    (pad 18 smd rect (at -3.175 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCLK))
    (pad 19 smd rect (at -4.445 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (pad 20 smd rect (at -5.715 -4.68376 180) (size 0.52832 1.97866) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCLK))
    (model Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module brunoeagle:JS202011SCQN (layer F.Cu) (tedit 573E25CB)
    (at 44.66 90.21 270)
    (fp_text reference SW1 (at -5.154 0.107 360) (layer F.SilkS))
    (fp_text value SW_DPDT_JS202011SCQN_one (at 0.043 0.091 270) (layer F.Fab))
    (pad 4 smd rect (at -2.5 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D1_off1-Pad2)"))
    (pad 5 smd rect (at 0 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R1_2-Pad2)"))
    (pad 6 smd rect (at 2.5 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D1_on1-Pad2)"))
    (pad 3 smd rect (at 2.5 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 40 /OPA_input_1/in))
    (pad 1 smd rect (at -2.5 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 46.778 68.58 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.736 1.016 180) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /INT/SQW))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 35.56 87.63)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Din1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(JP1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 Ain1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 35.56 74.93)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 Din2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(JP2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 Ain2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module brunoeagle:JS202011SCQN (layer F.Cu) (tedit 573E25CB)
    (at 44.66 77.43 270)
    (fp_text reference SW2 (at -5.154 0.107 360) (layer F.SilkS))
    (fp_text value SW_DPDT_JS202011SCQN_one (at 0.04 0.21 270) (layer F.Fab))
    (pad 4 smd rect (at -2.5 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D2_off1-Pad2)"))
    (pad 5 smd rect (at 0 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R2_2-Pad2)"))
    (pad 6 smd rect (at 2.5 -2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D2_on1-Pad2)"))
    (pad 3 smd rect (at 2.5 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 41 /OPA_input_2/in))
    (pad 1 smd rect (at -2.5 2.75 270) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53.34 92.54 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1_on1 (at -0.424 2.032 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D1_on1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53.34 80.01 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2_on1 (at -0.762 1.778 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D2_on1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 58C301F2)
    (at 25.4 90.17)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J1 (at 0 -5) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 59.42 91.44)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.27 -2.54) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 76.2 83.82 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 Alarm_out))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 69.85 81.28)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP3 (at 0 7.747) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 Alarm_out))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(JP3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /INT/SQW))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 45.27 66.04)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 2.355 -0.254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /INT/SQW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 31.115 92.271 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1_1 (at -2.863 0.635 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 49.98 90.17 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1_2 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R1_2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 74.48 54.356 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -1.974 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 Alarm_enable))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 31.0896 79.56 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2_1 (at -2.979 0.3556 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 50.604 77.47 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2_2 (at 0 -1.35 180) (layer F.SilkS))
    (fp_text value 150 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R2_2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 76.2 87.942 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0.069 1.524 270) (layer F.SilkS))
    (fp_text value 150 (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_DIP_x1_W8.61mm_Slide_LowProfile (layer F.Cu) (tedit 590880F3)
    (at 76.2 60.96 90)
    (descr "1x-dip-switch, Slide, row spacing 8.61 mm (338 mils), SMD, LowProfile")
    (tags "DIP Switch Slide 8.61mm 338mil SMD LowProfile")
    (attr smd)
    (fp_text reference SW4 (at 0 -3.17 90) (layer F.SilkS))
    (fp_text value SW_DIP_x01 (at 0 3.17 90) (layer F.Fab))
    (pad 1 smd rect (at -4.305 0 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 4.305 0 90) (size 2.44 1.12) (layers F.Cu F.Paste F.Mask)
      (net 50 Alarm_enable))
    (model Buttons_Switches.3dshapes/SW_DIP_x1_W8.61mm_Slide_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53.34 87.8 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1_off1 (at -0.678 -2.032 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D1_off1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 53.34 75.1 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2_off1 (at -0.17 -1.778 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D2_off1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 64.262 67.522 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_footprints_lsrggr:Logos (layer F.Cu) (tedit 0)
    (at 74.295 73.025)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 59085F6E)
    (at 67.216 62.865 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value OPA2340D (at 0 3.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(JP1-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(JP1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /OPA_input_1/in))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /OPA_input_2/in))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(JP2-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(JP2-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "GSM shield" (at 72.136 52.451) (layer F.SilkS))
  (gr_text off (at 80.391 65.278) (layer F.SilkS))
  (gr_text on (at 80.137 58.293) (layer F.SilkS))
  (gr_text "al enable?" (at 75.946 68.072) (layer F.SilkS))
  (gr_text al? (at 76.2 80.264) (layer F.SilkS))
  (gr_text out (at 64.77 76.454) (layer F.SilkS))
  (gr_text DS3234 (at 64.897 86.614) (layer F.SilkS))
  (gr_text source (at 69.342 78.613) (layer F.SilkS))
  (gr_text D8 (at 66.548 81.28) (layer F.SilkS))
  (gr_text "alarm out" (at 83.82 89.281) (layer F.SilkS))
  (gr_text "alarm 1" (at 43.053 96.139) (layer F.SilkS))
  (gr_text "alarm 2" (at 43.18 83.058) (layer F.SilkS))
  (gr_text "input 2" (at 25.781 82.931) (layer F.SilkS))
  (gr_text "input 1" (at 25.781 95.885) (layer F.SilkS))
  (gr_text on (at 48.133 94.615) (layer F.SilkS))
  (gr_text on (at 48.387 81.915) (layer F.SilkS))
  (gr_text off (at 48.387 85.852) (layer F.SilkS))
  (gr_text off (at 48.641 73.152) (layer F.SilkS))
  (gr_text D4 (at 32.766 86.868 90) (layer F.SilkS))
  (gr_text A0 (at 32.766 93.726 90) (layer F.SilkS))
  (gr_text A1 (at 32.766 81.153 90) (layer F.SilkS))
  (gr_text D5 (at 32.766 74.168 90) (layer F.SilkS))
  (gr_text "Cellular Safety v1.0\nL. Riegger 2017" (at 73.914 93.853) (layer F.SilkS))
  (gr_line (start 20.32 46.99) (end 85.09 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.32 100.33) (end 20.32 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 100.33) (end 20.32 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 97.79) (end 86.36 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 95.25) (end 86.36 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 62.23) (end 88.9 95.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 59.69) (end 88.9 62.23) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.36 48.26) (end 86.36 59.69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.09 46.99) (end 86.36 48.26) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.574 46.482) (xy 88.646 46.482) (xy 88.646 100.076) (xy 20.701 99.949)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.447 47.117) (xy 91.694 47.117) (xy 92.202 100.203) (xy 20.574 100.076)
      )
    )
  )
)
