(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 378)
    (zones 0)
    (modules 77)
    (nets 59)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(C9-Pad1)")
  (net 4 "Net-(C10-Pad1)")
  (net 5 "Net-(C11-Pad1)")
  (net 6 "Net-(C12-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "Net-(D4-Pad2)")
  (net 11 "Net-(D11-Pad2)")
  (net 12 "Net-(D10-Pad2)")
  (net 13 "Net-(D10-Pad1)")
  (net 14 "Net-(D11-Pad1)")
  (net 15 "Net-(D12-Pad1)")
  (net 16 "Net-(D13-Pad1)")
  (net 17 "Net-(D14-Pad1)")
  (net 18 "Net-(D15-Pad1)")
  (net 19 "Net-(D16-Pad1)")
  (net 20 "Net-(D17-Pad1)")
  (net 21 "Net-(D18-Pad1)")
  (net 22 "Net-(D20-Pad1)")
  (net 23 "Net-(D21-Pad1)")
  (net 24 "Net-(D22-Pad2)")
  (net 25 "Net-(D22-Pad1)")
  (net 26 "Net-(D23-Pad1)")
  (net 27 "Net-(D24-Pad1)")
  (net 28 "Net-(D25-Pad1)")
  (net 29 "Net-(D26-Pad1)")
  (net 30 "Net-(D27-Pad1)")
  (net 31 "Net-(D28-Pad1)")
  (net 32 "Net-(D29-Pad1)")
  (net 33 "Net-(D30-Pad1)")
  (net 34 "Net-(D32-Pad1)")
  (net 35 "Net-(D33-Pad1)")
  (net 36 "Net-(D34-Pad2)")
  (net 37 "Net-(D34-Pad1)")
  (net 38 "Net-(D35-Pad1)")
  (net 39 "Net-(D36-Pad1)")
  (net 40 "Net-(D37-Pad1)")
  (net 41 "Net-(D38-Pad1)")
  (net 42 "Net-(D39-Pad1)")
  (net 43 "Net-(D40-Pad1)")
  (net 44 "Net-(D41-Pad1)")
  (net 45 "Net-(D42-Pad1)")
  (net 46 "Net-(D44-Pad1)")
  (net 47 "Net-(D45-Pad1)")
  (net 48 "Net-(D46-Pad2)")
  (net 49 "Net-(D46-Pad1)")
  (net 50 "Net-(D47-Pad1)")
  (net 51 "Net-(D48-Pad1)")
  (net 52 "Net-(D49-Pad1)")
  (net 53 "Net-(D50-Pad1)")
  (net 54 "Net-(D51-Pad1)")
  (net 55 "Net-(D52-Pad1)")
  (net 56 "Net-(D53-Pad1)")
  (net 57 "Net-(D54-Pad1)")
  (net 58 "Net-(D56-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad1)")
    (add_net "Net-(D21-Pad1)")
    (add_net "Net-(D22-Pad1)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad1)")
    (add_net "Net-(D24-Pad1)")
    (add_net "Net-(D25-Pad1)")
    (add_net "Net-(D26-Pad1)")
    (add_net "Net-(D27-Pad1)")
    (add_net "Net-(D28-Pad1)")
    (add_net "Net-(D29-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D30-Pad1)")
    (add_net "Net-(D32-Pad1)")
    (add_net "Net-(D33-Pad1)")
    (add_net "Net-(D34-Pad1)")
    (add_net "Net-(D34-Pad2)")
    (add_net "Net-(D35-Pad1)")
    (add_net "Net-(D36-Pad1)")
    (add_net "Net-(D37-Pad1)")
    (add_net "Net-(D38-Pad1)")
    (add_net "Net-(D39-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D40-Pad1)")
    (add_net "Net-(D41-Pad1)")
    (add_net "Net-(D42-Pad1)")
    (add_net "Net-(D44-Pad1)")
    (add_net "Net-(D45-Pad1)")
    (add_net "Net-(D46-Pad1)")
    (add_net "Net-(D46-Pad2)")
    (add_net "Net-(D47-Pad1)")
    (add_net "Net-(D48-Pad1)")
    (add_net "Net-(D49-Pad1)")
    (add_net "Net-(D50-Pad1)")
    (add_net "Net-(D51-Pad1)")
    (add_net "Net-(D52-Pad1)")
    (add_net "Net-(D53-Pad1)")
    (add_net "Net-(D54-Pad1)")
    (add_net "Net-(D56-Pad1)")
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 98.5 43 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0 -2.9) (layer F.SilkS))
    (fp_text value CAT4238 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D56-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 84.5 43 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 -2.9) (layer F.SilkS))
    (fp_text value CAT4238 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D44-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 70.5 43 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9) (layer F.SilkS))
    (fp_text value CAT4238 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D32-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 56.5 43 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS))
    (fp_text value CAT4238 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D20-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 94 45 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 58 "Net-(D56-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 80 45 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 46 "Net-(D44-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 66 45.0875 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 34 "Net-(D32-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 52 45.0875 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.243902)
      (net 22 "Net-(D20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Bourns-SRU1028_10.0x10.0mm (layer F.Cu) (tedit 5DA0DC6F)
    (at 98 35)
    (descr "Bourns SRU1028 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRU1028.pdf")
    (tags "Bourns SRU1028 SMD inductor")
    (attr smd)
    (fp_text reference L4 (at 0 -6.2) (layer F.SilkS))
    (fp_text value 47u (at 0 6.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns-SRU1028_10.0x10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Bourns-SRU1028_10.0x10.0mm (layer F.Cu) (tedit 5DA0DC6F)
    (at 84 35.02)
    (descr "Bourns SRU1028 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRU1028.pdf")
    (tags "Bourns SRU1028 SMD inductor")
    (attr smd)
    (fp_text reference L3 (at 0 -6.2) (layer F.SilkS))
    (fp_text value 47u (at 0 6.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns-SRU1028_10.0x10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Bourns-SRU1028_10.0x10.0mm (layer F.Cu) (tedit 5DA0DC6F)
    (at 70 35)
    (descr "Bourns SRU1028 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRU1028.pdf")
    (tags "Bourns SRU1028 SMD inductor")
    (attr smd)
    (fp_text reference L2 (at 0 -6.2) (layer F.SilkS))
    (fp_text value 47u (at 0 6.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns-SRU1028_10.0x10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Bourns-SRU1028_10.0x10.0mm (layer F.Cu) (tedit 5DA0DC6F)
    (at 56 35.02)
    (descr "Bourns SRU1028 series SMD inductor, https://www.bourns.com/docs/Product-Datasheets/SRU1028.pdf")
    (tags "Bourns SRU1028 SMD inductor")
    (attr smd)
    (fp_text reference L1 (at 0 -6.2) (layer F.SilkS))
    (fp_text value 47u (at 0 6.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -4.5 0) (size 1.8 3.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns-SRU1028_10.0x10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right (layer F.Cu) (tedit 59FED5CC)
    (at 77 25 90)
    (descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x02 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J1 (at 0 0 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 3.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 1.655 -1.27 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.655 1.27 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 101 25 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 53 25 270)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 53 82 270)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0 270) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 101 82 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2 90) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.4 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.4 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 95 50 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D56 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 57 "Net-(D54-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 58 "Net-(D56-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 57 "Net-(D54-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 58 "Net-(D56-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 102 75 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D55 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 56 "Net-(D53-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 48 "Net-(D46-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 56 "Net-(D53-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 48 "Net-(D46-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 95 55 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D54 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 55 "Net-(D52-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 57 "Net-(D54-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 55 "Net-(D52-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 57 "Net-(D54-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 102 70 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D53 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 54 "Net-(D51-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 56 "Net-(D53-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 54 "Net-(D51-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 56 "Net-(D53-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 95 60 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D52 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 53 "Net-(D50-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 55 "Net-(D52-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 53 "Net-(D50-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 55 "Net-(D52-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 102 65 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D51 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 52 "Net-(D49-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 54 "Net-(D51-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 52 "Net-(D49-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 54 "Net-(D51-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 95 65 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D50 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 51 "Net-(D48-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 53 "Net-(D50-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 51 "Net-(D48-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 53 "Net-(D50-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 102 60 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D49 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 50 "Net-(D47-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 52 "Net-(D49-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 50 "Net-(D47-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 52 "Net-(D49-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 95 70 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D48 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 49 "Net-(D46-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 51 "Net-(D48-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 49 "Net-(D46-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 51 "Net-(D48-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 102 55 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D47 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 47 "Net-(D45-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 50 "Net-(D47-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 47 "Net-(D45-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 50 "Net-(D47-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 95 75 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D46 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 48 "Net-(D46-Pad2)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 49 "Net-(D46-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 48 "Net-(D46-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 49 "Net-(D46-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 102 50 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D45 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 47 "Net-(D45-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 47 "Net-(D45-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 81 50 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D44 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 45 "Net-(D42-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 46 "Net-(D44-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 45 "Net-(D42-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 46 "Net-(D44-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 88 75 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D43 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 44 "Net-(D41-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 36 "Net-(D34-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 44 "Net-(D41-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 36 "Net-(D34-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 81 55 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D42 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 43 "Net-(D40-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 45 "Net-(D42-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 43 "Net-(D40-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 45 "Net-(D42-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 88 70 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D41 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 42 "Net-(D39-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 44 "Net-(D41-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 42 "Net-(D39-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 44 "Net-(D41-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 81 60 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D40 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 41 "Net-(D38-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 43 "Net-(D40-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 41 "Net-(D38-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 43 "Net-(D40-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 88 65 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D39 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 40 "Net-(D37-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 42 "Net-(D39-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 40 "Net-(D37-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 42 "Net-(D39-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 81 65 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D38 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 39 "Net-(D36-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 41 "Net-(D38-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 39 "Net-(D36-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 41 "Net-(D38-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 88 60 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D37 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 38 "Net-(D35-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 40 "Net-(D37-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 38 "Net-(D35-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 40 "Net-(D37-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 81 70 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D36 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 37 "Net-(D34-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 39 "Net-(D36-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 37 "Net-(D34-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 39 "Net-(D36-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 88 55 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D35 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 35 "Net-(D33-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 38 "Net-(D35-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 35 "Net-(D33-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 38 "Net-(D35-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 81 75 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D34 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 36 "Net-(D34-Pad2)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 37 "Net-(D34-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 36 "Net-(D34-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 37 "Net-(D34-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 88 50 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D33 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 35 "Net-(D33-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 35 "Net-(D33-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 67 50 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D32 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 33 "Net-(D30-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 34 "Net-(D32-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 33 "Net-(D30-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 34 "Net-(D32-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 74 75 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D31 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 32 "Net-(D29-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 24 "Net-(D22-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 32 "Net-(D29-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 24 "Net-(D22-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 67 55 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D30 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 31 "Net-(D28-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 33 "Net-(D30-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 31 "Net-(D28-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 33 "Net-(D30-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 74 70 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D29 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 30 "Net-(D27-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 32 "Net-(D29-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 30 "Net-(D27-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 32 "Net-(D29-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 67 60 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D28 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 29 "Net-(D26-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 31 "Net-(D28-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 29 "Net-(D26-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 31 "Net-(D28-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 74 65 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D27 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 28 "Net-(D25-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 30 "Net-(D27-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 28 "Net-(D25-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 30 "Net-(D27-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 67 65 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D26 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 27 "Net-(D24-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 29 "Net-(D26-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 27 "Net-(D24-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 29 "Net-(D26-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 74 60 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D25 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 26 "Net-(D23-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 28 "Net-(D25-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 26 "Net-(D23-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 28 "Net-(D25-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 67 70 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D24 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 25 "Net-(D22-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 27 "Net-(D24-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 25 "Net-(D22-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 27 "Net-(D24-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 74 55 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D23 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 23 "Net-(D21-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 26 "Net-(D23-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 23 "Net-(D21-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 26 "Net-(D23-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 67 75 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D22 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 24 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 25 "Net-(D22-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 24 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 25 "Net-(D22-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 74 50 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D21 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 23 "Net-(D21-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 23 "Net-(D21-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 53 50 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D20 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 21 "Net-(D18-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 22 "Net-(D20-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 21 "Net-(D18-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 22 "Net-(D20-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 60 75 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D19 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 20 "Net-(D17-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 12 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 20 "Net-(D17-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 12 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 53 55 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D18 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 19 "Net-(D16-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 21 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 19 "Net-(D16-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 21 "Net-(D18-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 60 70 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D17 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 18 "Net-(D15-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 20 "Net-(D17-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 18 "Net-(D15-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 20 "Net-(D17-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 53 60 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D16 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 17 "Net-(D14-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 19 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 17 "Net-(D14-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 19 "Net-(D16-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 60 65 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D15 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 16 "Net-(D13-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 18 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 16 "Net-(D13-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 18 "Net-(D15-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 53 65 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D14 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 15 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 17 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 15 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 17 "Net-(D14-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 60 60 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D13 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 14 "Net-(D11-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 16 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 14 "Net-(D11-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 16 "Net-(D13-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 53 70 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D12 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 13 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 15 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 13 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 15 "Net-(D12-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 60 55 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D11 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 11 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 14 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 11 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 14 "Net-(D11-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 53 75 270)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D10 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 270) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 270) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 12 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.5 0 270) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 13 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 0.8 3) (layers F.Cu F.Mask)
      (net 12 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1.7 3) (layers F.Cu F.Mask)
      (net 13 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XH (layer F.Cu) (tedit 5E7E4700)
    (at 60 50 90)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf)
    (tags "LED Cree XH")
    (attr smd)
    (fp_text reference D9 (at 0 -2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.7 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 1.1 -0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.1 0.75 90) (size 0.7 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.65 -0.75 90) (size 1.35 1.2) (layers F.Paste))
    (pad 2 smd rect (at 1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 3 "Net-(C9-Pad1)"))
    (pad 1 smd rect (at -1.5 0 90) (size 0.5 0.33) (layers F.Cu F.Mask)
      (net 11 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 3) (layers F.Cu F.Mask)
      (net 3 "Net-(C9-Pad1)"))
    (pad 1 smd rect (at -0.65 0 90) (size 1.7 3) (layers F.Cu F.Mask)
      (net 11 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 103.5 41 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 89.5 41 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 75.5 41 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 61.5 40.95 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102 46)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 88 46)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74 46)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 59.775 46)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 93 41 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 79 41 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 65 41 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 51 41 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "LED Lighting Board\nCorwin Hansen\ncorwinh.com/git\nakerunakayama@gmail.com" (at 85 57.5 270) (layer B.SilkS))
  (gr_text 5v (at 81 23) (layer F.SilkS))
  (gr_text GND (at 72.5 23) (layer F.SilkS))
  (gr_line (start 105 21) (end 49 21) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105 86) (end 105 21) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49 86) (end 105 86) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49 21) (end 49 86) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 86) (xy 49 86) (xy 49 21) (xy 105 21)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105 86) (xy 49 86) (xy 49 21) (xy 105 21)
      )
    )
  )
)
