(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "VADER Gondola")
		(date "2025-07-01")
		(rev "v1")
		(company "NASA")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(A1-GPIO28_ADC2-Pad34)")
	(net 2 "unconnected-(A1-GPIO19-Pad25)")
	(net 3 "GND")
	(net 4 "unconnected-(A1-GPIO17-Pad22)")
	(net 5 "Net-(A1-VSYS)")
	(net 6 "unconnected-(A1-GPIO13-Pad17)")
	(net 7 "Net-(A1-GPIO8)")
	(net 8 "unconnected-(A1-GPIO0-Pad1)")
	(net 9 "unconnected-(A1-GPIO4-Pad6)")
	(net 10 "VCC")
	(net 11 "unconnected-(A1-GPIO5-Pad7)")
	(net 12 "unconnected-(A1-GPIO26_ADC0-Pad31)")
	(net 13 "unconnected-(A1-GPIO10-Pad14)")
	(net 14 "Net-(A1-GPIO7)")
	(net 15 "Net-(A1-GPIO9)")
	(net 16 "unconnected-(A1-RUN-Pad30)")
	(net 17 "unconnected-(A1-GPIO11-Pad15)")
	(net 18 "unconnected-(A1-GPIO16-Pad21)")
	(net 19 "unconnected-(A1-3V3-Pad36)")
	(net 20 "Net-(A1-GPIO6)")
	(net 21 "unconnected-(A1-ADC_VREF-Pad35)")
	(net 22 "unconnected-(J3-Pin_5-Pad5)")
	(net 23 "unconnected-(A1-GPIO3-Pad5)_1")
	(net 24 "unconnected-(A1-GPIO1-Pad2)_1")
	(net 25 "unconnected-(A1-GPIO27_ADC1-Pad32)_1")
	(net 26 "unconnected-(A1-GPIO2-Pad4)_1")
	(net 27 "unconnected-(A1-AGND-Pad33)_1")
	(net 28 "unconnected-(A1-GPIO21-Pad27)_1")
	(net 29 "unconnected-(A1-3V3_EN-Pad37)_1")
	(net 30 "unconnected-(A1-GPIO15-Pad20)_1")
	(net 31 "unconnected-(A1-GPIO20-Pad26)_1")
	(net 32 "unconnected-(A1-GPIO14-Pad19)_1")
	(net 33 "unconnected-(A1-GPIO22-Pad29)_1")
	(net 34 "unconnected-(A1-GPIO18-Pad24)_1")
	(net 35 "unconnected-(A1-GPIO12-Pad16)_1")
	(net 36 "unconnected-(J1-Pin_5-Pad5)")
	(net 37 "unconnected-(A1-3V3_EN-Pad37)")
	(net 38 "unconnected-(A1-GPIO2-Pad4)")
	(net 39 "unconnected-(A1-GPIO4-Pad6)_1")
	(net 40 "unconnected-(A1-GPIO21-Pad27)")
	(net 41 "unconnected-(A1-GPIO3-Pad5)")
	(net 42 "unconnected-(A1-GPIO26_ADC0-Pad31)_1")
	(net 43 "unconnected-(A1-GPIO1-Pad2)")
	(net 44 "unconnected-(A1-GPIO27_ADC1-Pad32)")
	(net 45 "unconnected-(A1-GPIO18-Pad24)")
	(net 46 "unconnected-(A1-GPIO12-Pad16)")
	(net 47 "unconnected-(A1-GPIO17-Pad22)_1")
	(net 48 "unconnected-(A1-GPIO28_ADC2-Pad34)_1")
	(net 49 "unconnected-(A1-AGND-Pad33)")
	(net 50 "unconnected-(A1-GPIO19-Pad25)_1")
	(net 51 "unconnected-(A1-GPIO16-Pad21)_1")
	(net 52 "unconnected-(A1-GPIO14-Pad19)")
	(net 53 "unconnected-(A1-RUN-Pad30)_1")
	(net 54 "unconnected-(A1-GPIO11-Pad15)_1")
	(net 55 "unconnected-(A1-GPIO22-Pad29)")
	(net 56 "unconnected-(A1-GPIO10-Pad14)_1")
	(net 57 "unconnected-(A1-GPIO15-Pad20)")
	(net 58 "unconnected-(A1-GPIO20-Pad26)")
	(net 59 "unconnected-(A1-GPIO0-Pad1)_1")
	(net 60 "unconnected-(A1-GPIO5-Pad7)_1")
	(net 61 "unconnected-(A1-ADC_VREF-Pad35)_1")
	(net 62 "unconnected-(A1-GPIO13-Pad17)_1")
	(footprint "Module:RaspberryPi_Pico_Common_Unspecified"
		(layer "F.Cu")
		(at 177.89 110.37)
		(descr "Raspberry Pi Pico versatile common (Pico & Pico W) footprint for surface-mount or through-hole hand soldering, supports Raspberry Pi Pico 2, default socketed model has height of 8.51mm, https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
		(tags "module usb pcb antenna")
		(property "Reference" "A1"
			(at -0.89 -9.37 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RaspberryPi_Pico"
			(at 0 27.94 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Versatile and inexpensive microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RaspberryPi?Pico?Common* RaspberryPi?Pico?SMD*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center -5.7 -23.5)
			(end -4.65 -23.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center -5.7 23.5)
			(end -4.65 23.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 5.7 -23.5)
			(end 6.75 -23.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 5.7 23.5)
			(end 6.75 23.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "Copper"
			(at 1 -5.635 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep"
			(at 1 -5 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Copper"
			(at 0 -23.9825 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep Out"
			(at 0 21.59 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep"
			(at 0 -21.3175 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Exposed Copper Keep Out"
			(at -2.5 -14.25 90)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Exposed Copper Keep Out"
			(at 3.1241 5.7 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Out"
			(at 0 -20.6825 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep Out"
			(at 0 -36.195 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "AGND Plane"
			(at 5.08 -7.62 90)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Out"
			(at 1 -4.365 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Exposed Copper Keep Out"
			(at 0 24.765 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Possible Antenna"
			(at 0 19.685 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Exposed"
			(at 0 -24.6175 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "USB Cable"
			(at 0 -38.735 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.37 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.725 -24)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -2.425 -20.97)
			(size 1.85 1.85)
			(drill 1.85)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.425 -20.97)
			(size 1.85 1.85)
			(drill 1.85)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.725 -24)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Mask")
		)
		(pad "1" smd custom
			(at -9.69 -24.13)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 8 "unconnected-(A1-GPIO0-Pad1)")
			(pinfunction "GPIO0")
			(pintype "bidirectional+no_connect")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at -8.89 -24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 59 "unconnected-(A1-GPIO0-Pad1)_1")
			(pinfunction "GPIO0")
			(pintype "bidirectional+no_connect")
		)
		(pad "2" smd roundrect
			(at -9.69 -21.59)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 43 "unconnected-(A1-GPIO1-Pad2)")
			(pinfunction "GPIO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "2" thru_hole circle
			(at -8.89 -21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-GPIO1-Pad2)_1")
			(pinfunction "GPIO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd custom
			(at -9.69 -19.05)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" thru_hole custom
			(at -8.89 -19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "4" smd roundrect
			(at -9.69 -16.51)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 26 "unconnected-(A1-GPIO2-Pad4)_1")
			(pinfunction "GPIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" thru_hole circle
			(at -8.89 -16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(A1-GPIO2-Pad4)")
			(pinfunction "GPIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -9.69 -13.97)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 41 "unconnected-(A1-GPIO3-Pad5)")
			(pinfunction "GPIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" thru_hole circle
			(at -8.89 -13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(A1-GPIO3-Pad5)_1")
			(pinfunction "GPIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" smd roundrect
			(at -9.69 -11.43)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 39 "unconnected-(A1-GPIO4-Pad6)_1")
			(pinfunction "GPIO4")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole circle
			(at -8.89 -11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(A1-GPIO4-Pad6)")
			(pinfunction "GPIO4")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" smd roundrect
			(at -9.69 -8.89)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 11 "unconnected-(A1-GPIO5-Pad7)")
			(pinfunction "GPIO5")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole circle
			(at -8.89 -8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(A1-GPIO5-Pad7)_1")
			(pinfunction "GPIO5")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd custom
			(at -9.69 -6.35)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "8" thru_hole custom
			(at -8.89 -6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd roundrect
			(at -9.69 -3.81)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 20 "Net-(A1-GPIO6)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at -8.89 -3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(A1-GPIO6)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -9.69 -1.27)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 14 "Net-(A1-GPIO7)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at -8.89 -1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(A1-GPIO7)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -9.69 1.27)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 7 "Net-(A1-GPIO8)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at -8.89 1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(A1-GPIO8)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -9.69 3.81)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 15 "Net-(A1-GPIO9)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at -8.89 3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(A1-GPIO9)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd custom
			(at -9.69 6.35)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "13" thru_hole custom
			(at -8.89 6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "14" smd roundrect
			(at -9.69 8.89)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 13 "unconnected-(A1-GPIO10-Pad14)")
			(pinfunction "GPIO10")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole circle
			(at -8.89 8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(A1-GPIO10-Pad14)_1")
			(pinfunction "GPIO10")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd roundrect
			(at -9.69 11.43)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 17 "unconnected-(A1-GPIO11-Pad15)")
			(pinfunction "GPIO11")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" thru_hole circle
			(at -8.89 11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(A1-GPIO11-Pad15)_1")
			(pinfunction "GPIO11")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" smd roundrect
			(at -9.69 13.97)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 35 "unconnected-(A1-GPIO12-Pad16)_1")
			(pinfunction "GPIO12")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole circle
			(at -8.89 13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(A1-GPIO12-Pad16)")
			(pinfunction "GPIO12")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd roundrect
			(at -9.69 16.51)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 6 "unconnected-(A1-GPIO13-Pad17)")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" thru_hole circle
			(at -8.89 16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(A1-GPIO13-Pad17)_1")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd custom
			(at -9.69 19.05)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "18" thru_hole custom
			(at -8.89 19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "19" smd roundrect
			(at -9.69 21.59)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 32 "unconnected-(A1-GPIO14-Pad19)_1")
			(pinfunction "GPIO14")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" thru_hole circle
			(at -8.89 21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(A1-GPIO14-Pad19)")
			(pinfunction "GPIO14")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" smd roundrect
			(at -9.69 24.13)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 57 "unconnected-(A1-GPIO15-Pad20)")
			(pinfunction "GPIO15")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" thru_hole circle
			(at -8.89 24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(A1-GPIO15-Pad20)_1")
			(pinfunction "GPIO15")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" thru_hole circle
			(at 8.89 24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-GPIO16-Pad21)")
			(pinfunction "GPIO16")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd roundrect
			(at 9.69 24.13)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 51 "unconnected-(A1-GPIO16-Pad21)_1")
			(pinfunction "GPIO16")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" thru_hole circle
			(at 8.89 21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-GPIO17-Pad22)")
			(pinfunction "GPIO17")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd roundrect
			(at 9.69 21.59)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 47 "unconnected-(A1-GPIO17-Pad22)_1")
			(pinfunction "GPIO17")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole custom
			(at 8.89 19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "23" smd custom
			(at 9.69 19.05)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "24" thru_hole circle
			(at 8.89 16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(A1-GPIO18-Pad24)_1")
			(pinfunction "GPIO18")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd roundrect
			(at 9.69 16.51)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 45 "unconnected-(A1-GPIO18-Pad24)")
			(pinfunction "GPIO18")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole circle
			(at 8.89 13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(A1-GPIO19-Pad25)")
			(pinfunction "GPIO19")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd roundrect
			(at 9.69 13.97)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 50 "unconnected-(A1-GPIO19-Pad25)_1")
			(pinfunction "GPIO19")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" thru_hole circle
			(at 8.89 11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(A1-GPIO20-Pad26)")
			(pinfunction "GPIO20")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" smd roundrect
			(at 9.69 11.43)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 31 "unconnected-(A1-GPIO20-Pad26)_1")
			(pinfunction "GPIO20")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" thru_hole circle
			(at 8.89 8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(A1-GPIO21-Pad27)_1")
			(pinfunction "GPIO21")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd roundrect
			(at 9.69 8.89)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 40 "unconnected-(A1-GPIO21-Pad27)")
			(pinfunction "GPIO21")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" thru_hole custom
			(at 8.89 6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "28" smd custom
			(at 9.69 6.35)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "29" thru_hole circle
			(at 8.89 3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(A1-GPIO22-Pad29)_1")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd roundrect
			(at 9.69 3.81)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 55 "unconnected-(A1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" thru_hole circle
			(at 8.89 1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "passive+no_connect")
		)
		(pad "30" smd roundrect
			(at 9.69 1.27)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 53 "unconnected-(A1-RUN-Pad30)_1")
			(pinfunction "RUN")
			(pintype "passive+no_connect")
		)
		(pad "31" thru_hole circle
			(at 8.89 -1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(A1-GPIO26_ADC0-Pad31)_1")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" smd roundrect
			(at 9.69 -1.27)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 12 "unconnected-(A1-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" thru_hole circle
			(at 8.89 -3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(A1-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" smd roundrect
			(at 9.69 -3.81)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 25 "unconnected-(A1-GPIO27_ADC1-Pad32)_1")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" thru_hole custom
			(at 8.89 -6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(A1-AGND-Pad33)")
			(pinfunction "AGND")
			(pintype "power_out+no_connect")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "33" smd custom
			(at 9.69 -6.35)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 27 "unconnected-(A1-AGND-Pad33)_1")
			(pinfunction "AGND")
			(pintype "power_out+no_connect")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "34" thru_hole circle
			(at 8.89 -8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(A1-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd roundrect
			(at 9.69 -8.89)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 48 "unconnected-(A1-GPIO28_ADC2-Pad34)_1")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" thru_hole circle
			(at 8.89 -11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(A1-ADC_VREF-Pad35)_1")
			(pinfunction "ADC_VREF")
			(pintype "power_in+no_connect")
		)
		(pad "35" smd roundrect
			(at 9.69 -11.43)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 21 "unconnected-(A1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "power_in+no_connect")
		)
		(pad "36" thru_hole circle
			(at 8.89 -13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(A1-3V3-Pad36)")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "36" smd roundrect
			(at 9.69 -13.97)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 19 "unconnected-(A1-3V3-Pad36)")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "37" thru_hole circle
			(at 8.89 -16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-3V3_EN-Pad37)_1")
			(pinfunction "3V3_EN")
			(pintype "passive+no_connect")
		)
		(pad "37" smd roundrect
			(at 9.69 -16.51)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 37 "unconnected-(A1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "passive+no_connect")
		)
		(pad "38" thru_hole custom
			(at 8.89 -19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "38" smd custom
			(at 9.69 -19.05)
			(size 1.6 0.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "39" thru_hole circle
			(at 8.89 -21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(A1-VSYS)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at 9.69 -21.59)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 5 "Net-(A1-VSYS)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at 8.89 -24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "VCC")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(pad "40" smd roundrect
			(at 9.69 -24.13)
			(size 3.2 1.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.5)
			(net 10 "VCC")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "B.Cu" "F.Paste" "B.Paste")
			(name "Antenna Copper Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 175.49 135.359895) (xy 170.79 131.709895) (xy 170.79 127.37) (xy 184.99 127.37) (xy 184.99 131.709895)
					(xy 180.29 135.359895) (xy 180.29 136.37) (xy 175.49 136.37)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D1-W")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 177.518778 115.170398) (xy 177.574498 115.114678) (xy 177.6473 115.084522) (xy 177.6867 115.0826)
					(xy 178.4741 115.0826) (xy 178.4741 117.0574) (xy 177.6867 117.0574) (xy 177.6473 117.055478) (xy 177.574498 117.025322)
					(xy 177.518778 116.969602) (xy 177.488622 116.8968) (xy 177.4867 116.8574) (xy 177.4867 115.2826)
					(xy 177.488622 115.2432)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D1-W")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 179.2615 117.0574) (xy 178.4741 117.0574) (xy 178.4741 115.0826) (xy 179.2615 115.0826) (xy 179.3009 115.084522)
					(xy 179.373702 115.114677) (xy 179.429423 115.170398) (xy 179.459578 115.2432) (xy 179.4615 115.2826)
					(xy 179.4615 116.8574) (xy 179.459578 116.8968) (xy 179.429423 116.969602) (xy 179.373702 117.025323)
					(xy 179.3009 117.055478)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP6")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 174.874455 100.317861) (xy 174.747833 100.283932) (xy 174.634306 100.218388) (xy 174.541612 100.125694)
					(xy 174.476068 100.012167) (xy 174.442139 99.885545) (xy 174.44 99.82) (xy 174.44 96.12) (xy 176.34 96.12)
					(xy 176.34 99.82) (xy 176.337861 99.885545) (xy 176.303932 100.012167) (xy 176.238388 100.125694)
					(xy 176.145694 100.218388) (xy 176.032167 100.283932) (xy 175.905545 100.317861) (xy 175.84 100.32)
					(xy 174.94 100.32)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP3")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 175.942139 85.554455) (xy 175.976068 85.427833) (xy 176.041612 85.314306) (xy 176.134306 85.221612)
					(xy 176.247833 85.156068) (xy 176.374455 85.122139) (xy 176.44 85.12) (xy 176.89 85.12) (xy 176.89 87.02)
					(xy 176.44 87.02) (xy 176.374455 87.017861) (xy 176.247833 86.983932) (xy 176.134306 86.918388)
					(xy 176.041612 86.825694) (xy 175.976068 86.712167) (xy 175.942139 86.585545) (xy 175.94 86.52)
					(xy 175.94 85.62)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP4")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 176.34 96.12) (xy 176.34 92.42) (xy 176.337861 92.354455) (xy 176.303933 92.227833) (xy 176.238388 92.114306)
					(xy 176.145694 92.021612) (xy 176.032167 91.956067) (xy 175.905545 91.922139) (xy 175.84 91.92)
					(xy 174.94 91.92) (xy 174.874455 91.922139) (xy 174.747833 91.956067) (xy 174.634306 92.021612)
					(xy 174.541612 92.114306) (xy 174.476067 92.227833) (xy 174.442139 92.354455) (xy 174.44 92.42)
					(xy 174.44 96.12)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP3")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 176.89 87.02) (xy 177.34 87.02) (xy 177.405545 87.017861) (xy 177.532167 86.983933) (xy 177.645694 86.918388)
					(xy 177.738388 86.825694) (xy 177.803933 86.712167) (xy 177.837861 86.585545) (xy 177.84 86.52)
					(xy 177.84 85.62) (xy 177.837861 85.554455) (xy 177.803933 85.427833) (xy 177.738388 85.314306)
					(xy 177.645694 85.221612) (xy 177.532167 85.156067) (xy 177.405545 85.122139) (xy 177.34 85.12)
					(xy 176.89 85.12)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP1")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 176.942139 88.854455) (xy 176.976068 88.727833) (xy 177.041612 88.614306) (xy 177.134306 88.521612)
					(xy 177.247833 88.456068) (xy 177.374455 88.422139) (xy 177.44 88.42) (xy 177.89 88.42) (xy 177.89 90.32)
					(xy 177.44 90.32) (xy 177.374455 90.317861) (xy 177.247833 90.283932) (xy 177.134306 90.218388)
					(xy 177.041612 90.125694) (xy 176.976068 90.012167) (xy 176.942139 89.885545) (xy 176.94 89.82)
					(xy 176.94 88.92)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D2")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 177.29 133.27) (xy 177.89 133.27)
					(arc
						(start 177.89 136.87)
						(mid 177.182893 136.577107)
						(end 176.89 135.87)
					)
					(xy 176.89 133.67) (xy 176.892193 133.606994) (xy 176.931133 133.487148) (xy 177.005201 133.385201)
					(xy 177.107148 133.311133) (xy 177.226994 133.272193)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP1")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 177.89 90.32) (xy 178.34 90.32) (xy 178.405545 90.317861) (xy 178.532167 90.283933) (xy 178.645694 90.218388)
					(xy 178.738388 90.125694) (xy 178.803933 90.012167) (xy 178.837861 89.885545) (xy 178.84 89.82)
					(xy 178.84 88.92) (xy 178.837861 88.854455) (xy 178.803933 88.727833) (xy 178.738388 88.614306)
					(xy 178.645694 88.521612) (xy 178.532167 88.456067) (xy 178.405545 88.422139) (xy 178.34 88.42)
					(xy 177.89 88.42)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP2")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 177.942139 85.569455) (xy 177.976068 85.442833) (xy 178.041612 85.329306) (xy 178.134306 85.236612)
					(xy 178.247833 85.171068) (xy 178.374455 85.137139) (xy 178.44 85.135) (xy 178.89 85.135) (xy 178.89 87.035)
					(xy 178.44 87.035) (xy 178.374455 87.032861) (xy 178.247833 86.998932) (xy 178.134306 86.933388)
					(xy 178.041612 86.840694) (xy 177.976068 86.727167) (xy 177.942139 86.600545) (xy 177.94 86.535)
					(xy 177.94 85.635)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP7")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 177.942139 104.854455) (xy 177.976068 104.727833) (xy 178.041612 104.614306) (xy 178.134306 104.521612)
					(xy 178.247833 104.456068) (xy 178.374455 104.422139) (xy 178.44 104.42) (xy 178.89 104.42) (xy 178.89 106.32)
					(xy 178.44 106.32) (xy 178.374455 106.317861) (xy 178.247833 106.283932) (xy 178.134306 106.218388)
					(xy 178.041612 106.125694) (xy 177.976068 106.012167) (xy 177.942139 105.885545) (xy 177.94 105.82)
					(xy 177.94 104.92)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D2")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 178.49 133.27) (xy 178.552964 133.272462) (xy 178.672728 133.311376) (xy 178.774606 133.385394)
					(xy 178.848624 133.487272) (xy 178.887538 133.607036) (xy 178.89 133.67)
					(arc
						(start 178.89 135.87)
						(mid 178.597107 136.577107)
						(end 177.89 136.87)
					)
					(xy 177.89 133.27)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP2")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 178.89 87.035) (xy 179.34 87.035) (xy 179.405545 87.032861) (xy 179.532167 86.998933) (xy 179.645694 86.933388)
					(xy 179.738388 86.840694) (xy 179.803933 86.727167) (xy 179.837861 86.600545) (xy 179.84 86.535)
					(xy 179.84 85.635) (xy 179.837861 85.569455) (xy 179.803933 85.442833) (xy 179.738388 85.329306)
					(xy 179.645694 85.236612) (xy 179.532167 85.171067) (xy 179.405545 85.137139) (xy 179.34 85.135)
					(xy 178.89 85.135)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out TP7")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 178.89 106.32) (xy 179.34 106.32) (xy 179.405545 106.317861) (xy 179.532167 106.283933) (xy 179.645694 106.218388)
					(xy 179.738388 106.125694) (xy 179.803933 106.012167) (xy 179.837861 105.885545) (xy 179.84 105.82)
					(xy 179.84 104.92) (xy 179.837861 104.854455) (xy 179.803933 104.727833) (xy 179.738388 104.614306)
					(xy 179.645694 104.521612) (xy 179.532167 104.456067) (xy 179.405545 104.422139) (xy 179.34 104.42)
					(xy 178.89 104.42)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D1")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(arc
						(start 174.35 135.87)
						(mid 174.642893 136.577107)
						(end 175.35 136.87)
					)
					(arc
						(start 175.35 133.27)
						(mid 174.642893 133.562893)
						(end 174.35 134.27)
					)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D1")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(arc
						(start 175.35 136.87)
						(mid 176.057107 136.577107)
						(end 176.35 135.87)
					)
					(arc
						(start 176.35 134.27)
						(mid 176.057107 133.562893)
						(end 175.35 133.27)
					)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D3")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(arc
						(start 179.430141 135.869925)
						(mid 179.723034 136.577032)
						(end 180.430141 136.869925)
					)
					(arc
						(start 180.430141 133.269925)
						(mid 179.723034 133.562818)
						(end 179.430141 134.269925)
					)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D3")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(arc
						(start 180.430141 136.869925)
						(mid 181.137248 136.577032)
						(end 181.430141 135.869925)
					)
					(arc
						(start 181.430141 134.269925)
						(mid 181.137248 133.562818)
						(end 180.430141 133.269925)
					)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D2-W")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 182.006278 116.07) (xy 181.987382 115.877285) (xy 181.931414 115.69191) (xy 181.840506 115.520937)
					(xy 181.71812 115.370877) (xy 181.568919 115.247447) (xy 181.398584 115.155348) (xy 181.213605 115.098087)
					(xy 181.021027 115.077846) (xy 180.828184 115.095396) (xy 180.642424 115.150069) (xy 180.47082 115.239781)
					(xy 180.319909 115.361116) (xy 180.195441 115.509452) (xy 180.102154 115.67914) (xy 180.043603 115.863715)
					(xy 180.022019 116.056147) (xy 180.038222 116.249107) (xy 180.091596 116.435245) (xy 180.180108 116.607471)
					(xy 180.300387 116.759225) (xy 180.447851 116.884726) (xy 180.616882 116.979195) (xy 180.801044 117.039033)
					(xy 180.993321 117.06196) (xy 181.18639 117.047105) (xy 181.372896 116.995031) (xy 181.545736 116.907724)
					(xy 181.698325 116.788507) (xy 181.824853 116.641923) (xy 181.9205 116.473555) (xy 181.981622 116.289816)
					(xy 182.005891 116.097703)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste")
			(name "Pad Keep Out D3-W")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 184.546278 116.07) (xy 184.527382 115.877285) (xy 184.471414 115.69191) (xy 184.380506 115.520937)
					(xy 184.25812 115.370877) (xy 184.108919 115.247447) (xy 183.938584 115.155348) (xy 183.753605 115.098087)
					(xy 183.561027 115.077846) (xy 183.368184 115.095396) (xy 183.182424 115.150069) (xy 183.01082 115.239781)
					(xy 182.859909 115.361116) (xy 182.735441 115.509452) (xy 182.642154 115.67914) (xy 182.583603 115.863715)
					(xy 182.562019 116.056147) (xy 182.578222 116.249107) (xy 182.631596 116.435245) (xy 182.720108 116.607471)
					(xy 182.840387 116.759225) (xy 182.987851 116.884726) (xy 183.156882 116.979195) (xy 183.341044 117.039033)
					(xy 183.533321 117.06196) (xy 183.72639 117.047105) (xy 183.912896 116.995031) (xy 184.085736 116.907724)
					(xy 184.238325 116.788507) (xy 184.364853 116.641923) (xy 184.4605 116.473555) (xy 184.521622 116.289816)
					(xy 184.545891 116.097703)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "Edge.Cuts")
			(name "Board Keep Out USB Cable")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 171.69 62.72) (xy 184.09 62.72) (xy 184.09 83.12) (xy 171.69 83.12)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.CrtYd")
			(name "USB Cable Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 172.14 82.67) (xy 173.95 82.67) (xy 173.95 83.07) (xy 181.83 83.07) (xy 181.83 82.67) (xy 183.64 82.67)
					(xy 183.64 63.17) (xy 172.14 63.17)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_DIP-40_W17.78mm_H8.51mm_Socket.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders_Socketed.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H_Socketed.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders_Socketed.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH_Socketed.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/blchase1/OneDrive - NASA/Documents/VADER/CAD/Pico v1.step"
			(offset
				(xyz -10.5 -25.5 9.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad_TopBottom"
		(layer "F.Cu")
		(at 178 140)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H2"
			(at 5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.5 5.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.5 5.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_ISO14580_Pad_TopBottom"
		(layer "F.Cu")
		(at 181.5 96)
		(descr "Mounting Hole 2.2mm, M2, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2 ISO14580")
		(property "Reference" "H3"
			(at 3.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.6 2.6)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 3.8 3.8)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 3.8 3.8)
			(layers "B.Cu" "B.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad_TopBottom"
		(layer "F.Cu")
		(at 178 82)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H1"
			(at 4.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0.154437 -4.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.5 5.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.5 5.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 183 119.5 90)
		(descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x05 2.54mm single row")
		(property "Reference" "J1"
			(at 2.5 -11.5 90)
			(layer "B.SilkS")
		)
		(property "Value" "LW20 LiDAR"
			(at 3 -5.12 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -5.08 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(A1-GPIO7)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(A1-GPIO6)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x05_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x05_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 183 112.5 90)
		(descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x05 2.54mm single row")
		(property "Reference" "J3"
			(at -2 1.5 90)
			(layer "B.SilkS")
		)
		(property "Value" "MinIMU-9 v6"
			(at 3 -5.62 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -5.08 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(A1-GPIO7)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(A1-GPIO6)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "VCC")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J3-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x05_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/blchase1/OneDrive - NASA/Documents/VADER/CAD/minimu-9-v6-gyro-accelerometer-and-compass v1.step"
			(offset
				(xyz -1.3 -11.42 9.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 182 124 90)
		(descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x04 2.54mm single row")
		(property "Reference" "J2"
			(at 0 2.77 90)
			(layer "B.SilkS")
		)
		(property "Value" "UART Winch-Gondola"
			(at -2.5 -4.3 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "gondola.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(A1-VSYS)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(A1-GPIO8)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(A1-GPIO9)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 166.5 138.5)
		(mid 169.328427 139.671573)
		(end 170.5 142.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.5 78.5)
		(end 185.5 78.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.5 138.5)
		(end 166.5 138.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.5 83.5)
		(end 166.5 83.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.5 79.5)
		(end 170.5 78.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.5 143.5)
		(end 170.5 142.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.5 143.5)
		(end 185.5 142.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 189.5 83.5)
		(mid 186.671573 82.328427)
		(end 185.5 79.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.5 83.5)
		(end 190.5 83.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.5 138.5)
		(end 190.5 83.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.5 78.5)
		(end 185.5 79.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.5 138.5)
		(end 189.5 138.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.5 143.5)
		(end 185.5 143.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.5 79.5)
		(mid 169.328427 82.328427)
		(end 166.5 83.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.5 142.5)
		(mid 186.671573 139.671573)
		(end 189.5 138.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.5 83.5)
		(end 165.5 138.5)
		(layer "Edge.Cuts")
	)
	(gr_text "Raspberry Pi Pico"
		(at 171 103.5 0)
		(layer "F.SilkS")
	)
	(gr_text "UART\nWinch-Gondola"
		(at 178 128.5 0)
		(layer "B.SilkS")
	)
	(gr_text "VADER Gondola\nPCB v1\n07/01/2025\nBenjamin Chase\nWFF Balloon Program"
		(at 178 130 180)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
