<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="18.03" width="0" layer="20"/>
<wire x1="35.56" y1="18.03" x2="0" y2="18.03" width="0" layer="20"/>
<wire x1="0" y1="18.03" x2="0" y2="0" width="0" layer="20"/>
<text>RA0</text>
<text>RA1</text>
<text>RA2</text>
<text>RA3</text>
<text>RA4</text>
<text>RA5</text>
<text>RA6</text>
<text>RA7</text>
<text>RB0</text>
<text>RB1</text>
<text>RB2</text>
<text>RB3</text>
<text>RB4</text>
<text>RB5</text>
<text>RB6</text>
<text>RB7</text>
<text>RC0</text>
<text>RC1</text>
<text>RC2</text>
<text>RC3</text>
<text>RC4</text>
<text>RC5</text>
<text>RC6</text>
<text>RC7</text>
<text>GND</text>
<text>RE3</text>
<text>+5V
VDD</text>
<text>GND</text>
</plain>
<libraries>
<library name="The Library">
<packages>
<package name="SSOP-28">
</package>
<package name="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL">
</package>
<package name="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_8.08MM-LNGTH_MALE-HDR_HRZNTL">
</package>
<package name="1MM-DMTR_2.54MM-PITCH_1-ROW_5-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL">
</package>
<package name="0603(1608)">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="The Library" package="SSOP-28" value="SSOP-28(PIC16F18857)">
<attribute name="PACKAGE-SIZE" value="SSOP-28"/>
<attribute name="TYPE" value="IC1"/>
</element>
<element name="HDR1" library="The Library" package="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL" value="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL">
<attribute name="PACKAGE-SIZE" value="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL"/>
<attribute name="TYPE" value="HDR1"/>
</element>
<element name="HDR2" library="The Library" package="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_8.08MM-LNGTH_MALE-HDR_HRZNTL" value="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_8.08MM-LNGTH_MALE-HDR_HRZNTL">
<attribute name="PACKAGE-SIZE" value="1MM-DMTR_2.54MM-PITCH_1-ROW_14-POS_8.08MM-LNGTH_MALE-HDR_HRZNTL"/>
<attribute name="TYPE" value="HDR2"/>
</element>
<element name="HDR3" library="The Library" package="1MM-DMTR_2.54MM-PITCH_1-ROW_5-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL" value="1MM-DMTR_2.54MM-PITCH_1-ROW_5-POS_5.84MM-LNGTH_MALE-HDR_HRZNTL">
<attribute name="TYPE" value="HDR3"/>
<attribute name="PACKAGE-SIZE" value="1MM-DMTR_2.54MM-PITCH_1-ROW_5-POS_5.84MM-LNGTH_MALE-HDR_HZNTL"/>
</element>
<element name="R1" library="The Library" package="0603(1608)" value="">
<attribute name="TYPE" value="R1"/>
<attribute name="PACKAGE-SIZE" value="0603(1608)"/>
</element>
<element name="C1" library="The Library" package="0603(1608)" value="">
<attribute name="TYPE" value="C1"/>
<attribute name="PACKAGE-SIZE" value="0603(1608)"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="8"/>
<contactref element="HDR2" pad="6"/>
<contactref element="HDR1" pad="2"/>
<contactref element="HDR3" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="HDR2" pad="14"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="HDR2" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="4"/>
<contactref element="HDR2" pad="12"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="5"/>
<contactref element="HDR2" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="6"/>
<contactref element="HDR2" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="7"/>
<contactref element="HDR2" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="10"/>
<contactref element="HDR2" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="9"/>
<contactref element="HDR2" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="20"/>
<contactref element="HDR2" pad="5"/>
<contactref element="HDR3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="21"/>
<contactref element="HDR2" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="11"/>
<contactref element="HDR1" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="12"/>
<contactref element="HDR1" pad="9"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="13"/>
<contactref element="HDR1" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="14"/>
<contactref element="HDR1" pad="7"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="22"/>
<contactref element="HDR2" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="23"/>
<contactref element="HDR2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="24"/>
<contactref element="HDR2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="15"/>
<contactref element="HDR1" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="16"/>
<contactref element="HDR1" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="17"/>
<contactref element="HDR1" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="18"/>
<contactref element="HDR1" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="25"/>
<contactref element="HDR1" pad="14"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="26"/>
<contactref element="HDR1" pad="13"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="27"/>
<contactref element="HDR1" pad="12"/>
<contactref element="HDR3" pad="5"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="1"/>
<contactref element="HDR1" pad="1"/>
<contactref element="HDR3" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="HDR3" pad="4"/>
<contactref element="IC1" pad="28"/>
<contactref element="HDR1" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
