<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="49.53" y1="48.26" x2="49.53" y2="75.565" width="0.4064" layer="20"/>
<wire x1="49.53" y1="75.565" x2="27.305" y2="75.565" width="0.4064" layer="20"/>
<wire x1="27.305" y1="75.565" x2="27.305" y2="48.26" width="0.4064" layer="20"/>
<wire x1="27.305" y1="48.26" x2="49.53" y2="48.26" width="0.4064" layer="20"/>
<text>OP: Audio 2017</text>
</plain>
<libraries>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/1V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
vertical position&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 1 hole

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FOOTPRINT" library="burr-brown" package="DIL14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5532" library="burr-brown" package="DIL08" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="capacitor-wima" package="C2.5-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="10R" library="gm-resistors" package="R0207/1V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="gm-caps-film-box" package="072X025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gm-caps-film-box" package="072X025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gm-caps-film-box" package="072X025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="gm-caps-film-box" package="072X025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="5532" pad="1"/>
<contactref element="FOOTPRINT" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="S$2">
<contactref element="5532" pad="2"/>
<contactref element="FOOTPRINT" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="S$4">
<contactref element="5532" pad="3"/>
<contactref element="FOOTPRINT" pad="6"/>
</signal>
<signal name="S$5">
<contactref element="10R" pad="2"/>
<contactref element="FOOTPRINT" pad="14"/>
</signal>
<signal name="S$9">
<contactref element="10R" pad="1"/>
<contactref element="5532" pad="8"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="S$10">
<contactref element="C3" pad="2"/>
<contactref element="5532" pad="4"/>
<contactref element="FOOTPRINT" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="S$12">
<contactref element="5532" pad="5"/>
<contactref element="FOOTPRINT" pad="8"/>
</signal>
<signal name="S$11">
<contactref element="C2" pad="1"/>
<contactref element="5532" pad="6"/>
<contactref element="FOOTPRINT" pad="9"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="S$3">
<contactref element="C5" pad="2"/>
<contactref element="5532" pad="7"/>
<contactref element="FOOTPRINT" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
