(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 108)
    (zones 0)
    (modules 18)
    (nets 9)
  )
  (page A4)
  (title_block
    (title "TS2596 6 to 40V to 5V @ 3A out")
    (date 2019-07-26)
    (rev V0)
    (company www.wire2wire.org)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.3556)
    (zone_45_only yes)
    (trace_min 0.1778)
    (via_size 0.69)
    (via_drill 0.33)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.127)
    (pad_size 4.550001 5.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFDDF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +VSW)
  (net 3 +5V)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(J3-Pad2)")
  (net 6 "Net-(J4-Pad3)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.69)
    (via_drill 0.33)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net +VSW)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
  )
  (module TO_SOT_Packages_SMD:TO-263-5_TabPin3 (layer F.Cu) (tedit 5D3BD9AF)
    (at 173.99 80.01 90)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
    (zone_connect 2)
    (attr smd)
    (fp_text reference U1 (at -3.81 -5.08 90) (layer F.SilkS))
    (fp_text value TS2596 (at 0 6.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -3.4 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 +VSW) (zone_connect 2))
    (pad 2 smd rect (at -5.775 -1.7 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)") (zone_connect 2))
    (pad 3 smd rect (at -5.775 0 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at -5.775 1.7 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 5 smd rect (at -5.775 3.4 90) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad2)") (zone_connect 2))
    (pad 3 smd rect (at 3.375 0 90) (size 9.399999 10.800001) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 5.8 2.775 90) (size 4.550001 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -2.775 90) (size 4.550001 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 5.8 -2.775 90) (size 4.550001 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 2.775 90) (size 4.550001 5.25) (layers F.Cu F.Paste)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-263-5_TabPin3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS_smt_parts:EEE-HA1AxxxUP (layer F.Cu) (tedit 5D3BD643)
    (at 187.325 90.805)
    (fp_text reference C4 (at -3.175 -5.08 180) (layer F.SilkS))
    (fp_text value 470uF (at -5 0 90) (layer F.Fab))
    (fp_text user + (at 1.9 3.1) (layer F.SilkS))
    (pad 2 smd rect (at 0 -3.55) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 3.55) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 201.295 67.945)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 2.54 -7.62) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 201.295 100.33)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at 8.255 -3.175) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 56D1B4CB)
    (at 153.035 67.945)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference REF** (at -1.27 -7.62) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module digikey-footprints:DO-214AC (layer F.Cu) (tedit 5D3BCA07)
    (at 162.56 97.79 180)
    (fp_text reference D2 (at 0 1.905) (layer F.SilkS))
    (fp_text value TSSA3U45 (at 0 2.45 180) (layer F.Fab))
    (fp_text user %R (at 0.40894 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 189.23 77.47 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 181.61 87.63 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Bourns:SRP1265A (layer F.Cu) (tedit 5D3BAE0C)
    (at 173.99 97.79)
    (fp_text reference L1 (at -5.715 -6.985) (layer F.SilkS))
    (fp_text value 47uH (at 0 -5.25) (layer F.Fab))
    (pad 2 smd rect (at 5.55 0) (size 3.1 5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -5.55 0) (size 3.1 5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
  )
  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289)
    (at 193.675 87.63 90)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J4 (at 10.795 -1.905 90) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 4.57 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole circle (at 10.16 2.67) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -3.56 2.67) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_A.wrl
      (offset (xyz 3.555999946594238 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 181.61 80.645)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Header (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_2pol (layer F.Cu) (tedit 59FF0756)
    (at 153.035 97.79 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J2 (at 6.35 -2.54) (layer F.SilkS))
    (fp_text value "3.5mm screw" (at 1.75 6 270) (layer F.Fab))
    (fp_text user %R (at 1.75 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +VSW))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_2pol (layer F.Cu) (tedit 59FF0756)
    (at 188.27 100.33)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J1 (at -2.85 -2.54) (layer F.SilkS))
    (fp_text value "3.5mm screw" (at 1.75 6) (layer F.Fab))
    (fp_text user %R (at 1.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS-icons:metroid (layer F.Cu) (tedit 5A0106A6)
    (at 187.774013 73.474013 45)
    (fp_text reference icon1 (at 0 2.54 45) (layer F.Fab) hide)
    (fp_text value Metroid (at 0 -2.54 45) (layer F.SilkS) hide)
    (pad "" smd circle (at 0 -0.635 45) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0.635 0 45) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at -0.635 0 45) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803)
    (at 189.23 81.745 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.54 0) (layer F.SilkS))
    (fp_text value Red (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 184.15 100.965 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 167.005 85.725 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +VSW))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS_smt_parts:EEE-FK1HxxxAM (layer F.Cu) (tedit 5D3BBC98)
    (at 156.845 85.725)
    (fp_text reference C1 (at -6.5 -9.5) (layer F.SilkS))
    (fp_text value 470uF (at -7.25 -2 90) (layer F.Fab))
    (fp_text user + (at 2.75 7.25) (layer F.SilkS))
    (pad 2 smd rect (at 0 -6.35) (size 2.5 6.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 6.25) (size 2.5 6.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +VSW))
  )
  (dimension 42.545 (width 0.15) (layer F.Fab)
    (gr_text "1.6750 in" (at 215.93 84.1375 90) (layer F.Fab))
    (feature1 (pts (xy 206.375 62.865) (xy 215.216421 62.865)))
    (feature2 (pts (xy 206.375 105.41) (xy 215.216421 105.41)))
    (crossbar (pts (xy 214.63 105.41) (xy 214.63 62.865)))
    (arrow1a (pts (xy 214.63 62.865) (xy 215.216421 63.991504)))
    (arrow1b (pts (xy 214.63 62.865) (xy 214.043579 63.991504)))
    (arrow2a (pts (xy 214.63 105.41) (xy 215.216421 104.283496)))
    (arrow2b (pts (xy 214.63 105.41) (xy 214.043579 104.283496)))
  )
  (dimension 58.42 (width 0.15) (layer F.Fab)
    (gr_text "2.3000 in" (at 177.165 113.06) (layer F.Fab))
    (feature1 (pts (xy 206.375 105.41) (xy 206.375 112.346421)))
    (feature2 (pts (xy 147.955 105.41) (xy 147.955 112.346421)))
    (crossbar (pts (xy 147.955 111.76) (xy 206.375 111.76)))
    (arrow1a (pts (xy 206.375 111.76) (xy 205.248496 112.346421)))
    (arrow1b (pts (xy 206.375 111.76) (xy 205.248496 111.173579)))
    (arrow2a (pts (xy 147.955 111.76) (xy 149.081504 112.346421)))
    (arrow2b (pts (xy 147.955 111.76) (xy 149.081504 111.173579)))
  )
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 281.94 173.99) (layer B.SilkS))
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 208.28 173.99) (layer F.SilkS))
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 281.94 173.99) (layer B.Cu))
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 208.28 173.99) (layer F.Cu))
  (gr_text 5Vout (at 194.945 101.6 90) (layer F.SilkS))
  (gr_text Vin (at 157.48 99.695 90) (layer F.SilkS))
  (gr_text "TS2596 Vin 6V to 40V in 5V @ 3A out.\nPJS 26Jul2019 MIT License " (at 177.165 66.04) (layer F.SilkS))
  (gr_line (start 147.955 62.865) (end 147.955 105.41) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 206.375 62.865) (end 147.955 62.865) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 206.375 105.41) (end 206.375 62.865) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.955 105.41) (end 206.375 105.41) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.955 62.865) (xy 206.375 62.865) (xy 206.375 105.41) (xy 147.955 105.41)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.955 62.865) (xy 206.375 62.865) (xy 206.375 105.41) (xy 147.955 105.41)
      )
    )
  )
)
