(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 88)
    (zones 0)
    (modules 5)
    (nets 12)
  )
  (page A4)
  (title_block
    (title "DebugEdge Adapter")
    (date 2020-08-27)
    (rev 1)
    (company debug-edge.io)
    (comment 1 "Brainchild of @tannewt, @_nitz, and @GregDavill")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /~RESET~)
  (net 2 GND)
  (net 3 /SWCLK)
  (net 4 /SWDIO)
  (net 5 VCC)
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad10)")
  (net 8 "Net-(J1-Pad9)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad6)")
  (net 11 "Net-(J2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /~RESET~)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad5)")
    (add_net VCC)
  )
  (module Connector_DebugEdge:DebugEdge_2x05_Host (layer F.Cu) (tedit 5F5EA31C)
    (at 170 95 270)
    (attr virtual)
    (fp_text reference J2 (at 0.05 -3.2 180 unlocked) (layer F.Fab))
    (fp_text value DebugEdge_02x05 (at -1.2 -2 90) (layer F.Fab))
    (fp_arc (start 0 0.5) (end 0 0) (angle -90) (layer Edge.Cuts) (width 0.05))
    (fp_arc (start -2 0.5) (end -1.5 0.5) (angle -90) (layer Edge.Cuts) (width 0.05))
    (fp_arc (start -1 2.6) (end -1.5 2.6) (angle -180) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -1.5 0.5) (end -1.5 2.6) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -0.5 2.6) (end -0.5 0.5) (layer Edge.Cuts) (width 0.05))
    (fp_line (start -5 0) (end -2 0) (layer Edge.Cuts) (width 0.05))
    (fp_line (start 0 0) (end 5 0) (layer Edge.Cuts) (width 0.05))
    (pad 1 smd custom (at -2 3.6 270) (size 1 1) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.3 -0.99) (xy 0.31 -0.88) (xy 0.33 -0.8) (xy 0.35 -0.74) (xy 0.37 -0.69)
           (xy 0.4 -0.64) (xy 0.44 -0.58) (xy 0.48 -0.53) (xy 0.5 -0.51) (xy 0.5 0.5)
           (xy -0.5 0.5) (xy -0.5 -3.2) (xy 0.3 -3.2)) (width 0))
      ))
    (pad 2 smd custom (at 0 3.6 270) (size 1 1) (layers F.Cu F.Mask)
      (net 4 /SWDIO) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.3 -0.99) (xy -0.31 -0.88) (xy -0.33 -0.8) (xy -0.35 -0.74) (xy -0.37 -0.69)
           (xy -0.4 -0.64) (xy -0.44 -0.58) (xy -0.48 -0.53) (xy -0.5 -0.51) (xy -0.5 0.5)
           (xy 0.5 0.5) (xy 0.5 -3) (xy -0.3 -3)) (width 0))
      ))
    (pad 4 smd custom (at 0 2.1 90) (size 0.4 0.4) (layers B.Cu B.Mask)
      (net 1 /~RESET~) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.3 -0.51) (xy 0.31 -0.62) (xy 0.33 -0.7) (xy 0.35 -0.76) (xy 0.37 -0.81)
           (xy 0.4 -0.86) (xy 0.44 -0.92) (xy 0.48 -0.97) (xy 0.5 -0.99) (xy 0.5 -1.9)
           (xy -0.5 -2) (xy -0.5 1.5) (xy 0.3 1.5)) (width 0))
      ))
    (pad 3 smd custom (at -2 2.1 90) (size 0.4 0.4) (layers B.Cu B.Mask)
      (net 3 /SWCLK) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.3 -0.51) (xy -0.31 -0.62) (xy -0.33 -0.7) (xy -0.35 -0.76) (xy -0.37 -0.81)
           (xy -0.4 -0.86) (xy -0.44 -0.92) (xy -0.48 -0.97) (xy -0.5 -0.99) (xy -0.5 -1.9)
           (xy 0.5 -2) (xy 0.5 1.5) (xy -0.3 1.5)) (width 0))
      ))
    (pad 5 smd rect (at 2 2.35 270) (size 1 3.5) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad5)") (zone_connect 0))
    (pad 10 smd custom (at 4 2.5 90) (size 1 3.8) (layers B.Cu B.Mask)
      (net 7 "Net-(J1-Pad10)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 -1.9) (xy -0.5 -2) (xy -0.5 -1.9)) (width 0))
      ))
    (pad 6 smd custom (at 2 2.4 90) (size 1 3.6) (layers B.Cu B.Mask)
      (net 10 "Net-(J1-Pad6)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 -1.8) (xy -0.5 -1.9) (xy -0.5 -1.8)) (width 0))
      ))
    (pad 8 smd custom (at -4 2.4 90) (size 1 3.6) (layers B.Cu B.Mask)
      (net 9 "Net-(J1-Pad8)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.5 -1.8) (xy 0.5 -1.9) (xy -0.5 -1.8)) (width 0))
      ))
    (pad 9 smd rect (at 4 2.35 270) (size 1 3.5) (layers F.Cu F.Mask)
      (net 8 "Net-(J1-Pad9)") (zone_connect 0))
    (pad 7 smd rect (at -4 2.35 270) (size 1 3.5) (layers F.Cu F.Mask)
      (net 6 "Net-(J1-Pad7)") (zone_connect 0))
  )
  (module Connector_DebugEdge:DebugEdge_URL_Silk (layer F.Cu) (tedit 5F4720B6)
    (at 161.6 89 180)
    (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 155.4 98.4 270)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (fp_text reference J3 (at 0 2.2 90) (layer F.SilkS) hide)
    (fp_text value "BYOP - Bring Your Own Power" (at 0 4 90) (layer F.Fab))
    (fp_text user %R (at 0 0.5) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 1 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 159.4 98.6)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0.6 2.4) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 11 "Net-(J2-Pad5)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 157 93.75 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -3.8 270) (layer F.SilkS) hide)
    (fp_text value "Upstream Host Connector" (at -1.45 -7.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET~))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 /SWCLK))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 4 /SWDIO))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 155.4 99.8) (layer F.SilkS))
  (gr_text - (at 154.3 99.8) (layer F.SilkS))
  (gr_arc (start 153 100) (end 152 100) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169.0022 100) (end 169.0022 101) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169 89) (end 170 89) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 153 89) (end 153 88) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Revision 1.1" (at 159.2 94.4 270) (layer B.SilkS))
  (gr_text Vref (at 159.6 100.1 180) (layer F.SilkS))
  (gr_text BYOP (at 153 98.4 90) (layer F.SilkS))
  (gr_line (start 153 101) (end 169 101) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 89) (end 152 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169 88) (end 153 88) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170 90) (end 170 89) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172 102) (xy 151 102) (xy 151 87) (xy 172 87)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172 102) (xy 151 102) (xy 151 87) (xy 172 87)
      )
    )
  )
)
