(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(H1-Pad1)")
  (net 2 "Net-(H2-Pad1)")
  (net 3 "Net-(H3-Pad1)")
  (net 4 "Net-(H4-Pad1)")
  (net 5 "Net-(H5-Pad1)")
  (net 6 "Net-(H6-Pad1)")
  (net 7 "Net-(H9-Pad1)")
  (net 8 "Net-(H10-Pad1)")
  (net 9 "Net-(H12-Pad1)")
  (net 10 "Net-(H13-Pad1)")
  (net 11 "Net-(H14-Pad1)")
  (net 12 "unconnected-(J1-Pad4)")
  (net 13 "unconnected-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 28.187 57.921)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "RX" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 5 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 "Net-(H5-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 30.95 95.5 90)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x16_Female" (at 0 40.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 19.05) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(H1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(H14-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(H4-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(H2-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(H3-Pad1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(H5-Pad1)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(H6-Pad1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(H13-Pad1)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(H12-Pad1)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(H10-Pad1)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(H9-Pad1)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 32.212 35.068)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "SCL" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 2 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(H2-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 71.813 42.079)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H10" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "A2" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 8 "Net-(H10-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(H10-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 8 "Net-(H10-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 71.813 57.921)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H12" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "A1" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 "Net-(H12-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(H12-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 9 "Net-(H12-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 67.768 35.068)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H9" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "A3" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(H9-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 7 "Net-(H9-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 "Net-(H9-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 28.187 42.079)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "SDA" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 3 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 3 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(H3-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 67.788 64.932)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H13" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "A0" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(H13-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 10 "Net-(H13-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 "Net-(H13-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 73.178 50)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H11" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "GND" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 26.822 50)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "3.3V" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 4 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 40.602 40.094 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "Express" (at -2.581 2.698) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 38.443 29.875)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "GND" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 61.557 29.875)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "3.3V" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 4 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(H4-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 32.212 64.932)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "TX" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 "Net-(H6-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(H6-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 6 "Net-(H6-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 61.557 70.125)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H14" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "VCC" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(H14-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 11 "Net-(H14-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 11 "Net-(H14-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 41.364 46.444 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "Bluefruit" (at -2.575 2.45) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 38.443 70.125)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "CPX_ASM.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "GND" (at 0 3.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.6 5.6) (layers "B.Cu" "B.Mask")
      (net 1 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (gr_line (start 20.75 98) (end 79.25 98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 20.75 50) (end 20.75 98) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 79.25 98) (end 79.25 50) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 20.75 50) (mid 50 20.75) (end 79.25 50) (layer "Edge.Cuts") (width 0.2))
  (gr_text "GND\nVCC\n3.3V\n\nSCL\nSDA\nRX\nTX\nA0\nA1\nA2\nA3\n\nSWCLK\nSWDIO\nRESET" (at 50.125 93.35 90) (layer "F.SilkS"))
  (gr_text "Circuit Playground\nExpress/Bluefruit\nCarrier" (at 50 58) (layer "F.SilkS"))
)
