(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.4)
    (drawings 32)
    (tracks 66)
    (zones 0)
    (modules 20)
    (nets 48)
  )
  (page A4)
  (title_block
    (title "Human Activity Detector")
    (date 2022-02-25)
    (rev A)
    (company UTDesign)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 111.6 117)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "out/"))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(IC1-Pad7)")
  (net 3 "Net-(IC1-Pad6)")
  (net 4 "Net-(IC1-Pad5)")
  (net 5 GND)
  (net 6 "Net-(C2-Pad1)")
  (net 7 "Net-(C1-Pad1)")
  (net 8 AUD)
  (net 9 "Net-(J1-Pad20)")
  (net 10 "Net-(J1-Pad19)")
  (net 11 "Net-(J1-Pad18)")
  (net 12 "Net-(J1-Pad17)")
  (net 13 "Net-(J1-Pad16)")
  (net 14 "Net-(J1-Pad15)")
  (net 15 "Net-(J1-Pad14)")
  (net 16 "Net-(J1-Pad13)")
  (net 17 "Net-(J1-Pad12)")
  (net 18 "Net-(J1-Pad11)")
  (net 19 "Net-(J1-Pad9)")
  (net 20 PIR)
  (net 21 "Net-(J1-Pad7)")
  (net 22 "Net-(J1-Pad6)")
  (net 23 "Net-(J1-Pad5)")
  (net 24 "Net-(J1-Pad3)")
  (net 25 "Net-(J1-Pad2)")
  (net 26 "Net-(J2-Pad20)")
  (net 27 "Net-(J2-Pad19)")
  (net 28 "Net-(J2-Pad18)")
  (net 29 "Net-(J2-Pad17)")
  (net 30 "Net-(J2-Pad16)")
  (net 31 "Net-(J2-Pad15)")
  (net 32 "Net-(J2-Pad14)")
  (net 33 "Net-(J2-Pad13)")
  (net 34 "Net-(J2-Pad12)")
  (net 35 "Net-(J2-Pad11)")
  (net 36 "Net-(J2-Pad10)")
  (net 37 "Net-(J2-Pad9)")
  (net 38 "Net-(J2-Pad8)")
  (net 39 "Net-(J2-Pad7)")
  (net 40 "Net-(J2-Pad6)")
  (net 41 "Net-(J2-Pad5)")
  (net 42 "Net-(J2-Pad4)")
  (net 43 "Net-(J2-Pad3)")
  (net 44 "Net-(J2-Pad1)")
  (net 45 "Net-(C1-Pad2)")
  (net 46 "Net-(S1-Pad3)")
  (net 47 "Net-(S1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AUD)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S1-Pad3)")
    (add_net PIR)
    (add_net VDD)
  )
  (module WiSUN-PCB:SSQ-110-XX-YYY-D (layer F.Cu) (tedit 621947E6)
    (at 163.725 73.725 90)
    (descr SSQ-110-XX-YYY-D)
    (tags Connector)
    (fp_text reference J1 (at 0.2 0.01 90) (layer F.SilkS) hide)
    (fp_text value SSQ-110-23-F-D (at -7.9 -6.01 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.2 0.01 90) (layer F.Fab))
    (pad 20 thru_hole circle (at -22.86 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at -22.86 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad19)"))
    (pad 18 thru_hole circle (at -20.32 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at -20.32 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad17)"))
    (pad 16 thru_hole circle (at -17.78 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad16)"))
    (pad 15 thru_hole circle (at -17.78 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at -15.24 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at -15.24 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at -12.7 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad12)"))
    (pad 11 thru_hole circle (at -12.7 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad11)"))
    (pad 10 thru_hole circle (at -10.16 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 AUD))
    (pad 9 thru_hole circle (at -10.16 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad9)"))
    (pad 8 thru_hole circle (at -7.62 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 PIR))
    (pad 7 thru_hole circle (at -7.62 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad7)"))
    (pad 6 thru_hole circle (at -5.08 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -5.08 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at -2.54 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at -2.54 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0.01) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KIPRJMOD}/packages3d/HeaderConnector.step
      (offset (xyz -24.4 -3.7 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module WiSUN-PCB:SSQ-110-XX-YYY-D (layer F.Cu) (tedit 621947E6)
    (at 120.525 73.725 90)
    (descr SSQ-110-XX-YYY-D)
    (tags Connector)
    (fp_text reference J2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value SSQ-110-23-F-D (at 24.865 -2.505 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 20 thru_hole circle (at -22.86 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad20)"))
    (pad 19 thru_hole circle (at -22.86 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad19)"))
    (pad 18 thru_hole circle (at -20.32 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad18)"))
    (pad 17 thru_hole circle (at -20.32 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad17)"))
    (pad 16 thru_hole circle (at -17.78 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad16)"))
    (pad 15 thru_hole circle (at -17.78 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad15)"))
    (pad 14 thru_hole circle (at -15.24 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad14)"))
    (pad 13 thru_hole circle (at -15.24 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad13)"))
    (pad 12 thru_hole circle (at -12.7 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad12)"))
    (pad 11 thru_hole circle (at -12.7 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad11)"))
    (pad 10 thru_hole circle (at -10.16 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad10)"))
    (pad 9 thru_hole circle (at -10.16 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad9)"))
    (pad 8 thru_hole circle (at -7.62 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad8)"))
    (pad 7 thru_hole circle (at -7.62 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad7)"))
    (pad 6 thru_hole circle (at -5.08 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at -5.08 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad5)"))
    (pad 4 thru_hole circle (at -2.54 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 42 "Net-(J2-Pad4)"))
    (pad 3 thru_hole circle (at -2.54 0.01 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 43 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 0 -2.53 90) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0.01) (size 1.55 1.55) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad1)"))
    (model ${KIPRJMOD}/packages3d/HeaderConnector.step
      (offset (xyz -24.4 -3.7 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 131.33 47.47 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1 -3.75 90) (layer F.SilkS))
    (fp_text value 39u (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WiSUN-PCB:BS412-PIR locked (layer F.Cu) (tedit 62190D94)
    (at 140.85 32.2 270)
    (fp_text reference IC2 (at 7.19 -3.23) (layer F.SilkS))
    (fp_text value BS412 (at -3.81 -5.08 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 270) (size 1.545 1.545) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.545 1.545) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.545 1.545) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 4 thru_hole circle (at 2.54 0 270) (size 1.545 1.545) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 PIR))
    (model ${KIPRJMOD}/packages3d/PIR.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WiSUN-PCB:CMEJ062742P (layer F.Cu) (tedit 6218FA9A)
    (at 126.75 32 180)
    (descr CMEJ-0627-42-P-2)
    (tags Connector)
    (fp_text reference J3 (at -0.81 -5.15) (layer F.SilkS))
    (fp_text value CMEJ-0627-42-P (at 0.3 5 180) (layer F.SilkS) hide)
    (fp_text user %R (at 0.8 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.95 -1 180) (size 1.545 1.545) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0.05 -1 180) (size 1.545 1.545) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KIPRJMOD}/SamacSys_PCB_Library/SamacSys_Parts.3dshapes/CMEJ-0627-42-P.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WiSUN-PCB:TLV2782IP (layer F.Cu) (tedit 6218F407)
    (at 140.85 48.7 90)
    (descr "8-DIP (0.300\", 7.62mm)")
    (tags "Integrated Circuit")
    (fp_text reference IC1 (at 0 0 270) (layer F.SilkS))
    (fp_text value TLV2782IP (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.97 -3.81 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 AUD))
    (pad 2 thru_hole circle (at -3.97 -1.27 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at -3.97 1.27 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (pad 4 thru_hole circle (at -3.97 3.81 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole circle (at 3.97 3.81 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole circle (at 3.97 1.27 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole circle (at 3.97 -1.27 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at 3.97 -3.81 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KIPRJMOD}/SamacSys_PCB_Library/SamacSys_Parts.3dshapes/TLV2782IP.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 163.85 32.2)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference H2 (at 0 4.6) (layer B.SilkS))
    (fp_text value MountingHole_Pad (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 connect circle (at 0 0) (size 7 7) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0) (size 3.9 3.9) (drill 3.5) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module MountingHole:MountingHole_3.5mm_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 117.9 32.2)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference H1 (at 0 4.5) (layer B.SilkS))
    (fp_text value MountingHole_Pad (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 connect circle (at 0 0) (size 7 7) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0) (size 3.9 3.9) (drill 3.5) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module WiSUN-PCB:Nameplate-Rev-A (layer B.Cu) (tedit 0)
    (at 159.9 110.7 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module WiSUN-PCB:Nameplate-Rev-A (layer F.Cu) (tedit 0)
    (at 118.4 107 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module SamacSys_Parts:10TC605 (layer F.Cu) (tedit 6216C386)
    (at 155.8 34.7 90)
    (descr 10TC605-2)
    (tags Switch)
    (fp_text reference S1 (at -3.95 -2.38 180) (layer F.SilkS))
    (fp_text value 10TC605 (at 2.54 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.68 1.68) (drill 1.12) (layers *.Cu *.Mask)
      (net 46 "Net-(S1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.68 1.68) (drill 1.12) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.68 1.68) (drill 1.12) (layers *.Cu *.Mask)
      (net 47 "Net-(S1-Pad1)"))
    (model ${KIPRJMOD}/packages3d/MountainSwitch.step
      (offset (xyz -2 -3 1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Battery:BatteryHolder_Keystone_2462_2xAA locked (layer F.Cu) (tedit 5BB4D45D)
    (at 148.35 57.9 270)
    (descr "2xAA cell battery holder, Keystone P/N 2462, https://www.keyelco.com/product-pdf.cfm?p=1027")
    (tags "AA battery cell holder")
    (fp_text reference U1 (at 0.2286 0.4873 90) (layer F.SilkS))
    (fp_text value 2462 (at 21.7 10.24 90) (layer F.Fab))
    (fp_text user - (at -6.8 17.4 90) (layer F.SilkS))
    (fp_text user + (at -3.81 0 90) (layer F.SilkS))
    (fp_text user - (at 16.355 14.99 90) (layer F.SilkS))
    (fp_text user + (at 37.945 14.99 90) (layer F.SilkS))
    (fp_text user %R (at 0 -10.16 90) (layer F.Fab))
    (fp_text user + (at 16.355 0 90) (layer F.SilkS))
    (fp_text user - (at 37.945 0 90) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 27.165 0 270) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 27.165 14.99 270) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 14.99 270) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 47 "Net-(S1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_2462_2xAA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 120.522 66.041 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 5.022 0.041) (layer F.SilkS))
    (fp_text value 39u (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 125.91 51.49 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 10.41 -2.41 180) (layer F.SilkS))
    (fp_text value 180k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at -6.74 1) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 AUD))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 155.81 51.59)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -0.21 2.31) (layer F.SilkS))
    (fp_text value 1M (at 5.29 -2.29) (layer F.Fab))
    (fp_text user %R (at 5.09 0.01) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 165.98 45.45 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 10.38 -2.35) (layer F.SilkS))
    (fp_text value 1M (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 115.73 45.45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -0.23 2.45 180) (layer F.SilkS))
    (fp_text value 820 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 4.7 0.3) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 120.522 58.541 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at 5.022 0.041) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.4) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 161.2 58.5)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 5.2 0) (layer F.SilkS))
    (fp_text value 0.1u (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 150.38 49.46 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at -3 0 90) (layer F.SilkS))
    (fp_text value 39u (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PIR (at 137.78 39.39) (layer F.SilkS))
  (gr_text Mic (at 123.56 37.05) (layer F.SilkS))
  (dimension 94.8 (width 0.15) (layer Dwgs.User)
    (gr_text "94.800 mm" (at 192.3 69.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 170.1 22.2) (xy 191.586421 22.2)))
    (feature2 (pts (xy 170.1 117) (xy 191.586421 117)))
    (crossbar (pts (xy 191 117) (xy 191 22.2)))
    (arrow1a (pts (xy 191 22.2) (xy 191.586421 23.326504)))
    (arrow1b (pts (xy 191 22.2) (xy 190.413579 23.326504)))
    (arrow2a (pts (xy 191 117) (xy 191.586421 115.873496)))
    (arrow2b (pts (xy 191 117) (xy 190.413579 115.873496)))
  )
  (gr_text J2 (at 166.3 97.4) (layer F.SilkS))
  (gr_arc (start 168.6 23.7) (end 170.1 23.7) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.1 23.7) (end 113.1 22.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Launchpad Footprint" (at 139.3 144.5) (layer Dwgs.User))
  (dimension 38.25 (width 0.15) (layer Dwgs.User)
    (gr_text "38.250 mm" (at 140.825 102) (layer Dwgs.User))
    (feature1 (pts (xy 159.95 97.800001) (xy 159.95 101.286421)))
    (feature2 (pts (xy 121.7 97.800001) (xy 121.7 101.286421)))
    (crossbar (pts (xy 121.7 100.7) (xy 159.95 100.7)))
    (arrow1a (pts (xy 159.95 100.7) (xy 158.823496 101.286421)))
    (arrow1b (pts (xy 159.95 100.7) (xy 158.823496 100.113579)))
    (arrow2a (pts (xy 121.7 100.7) (xy 122.826504 101.286421)))
    (arrow2b (pts (xy 121.7 100.7) (xy 122.826504 100.113579)))
  )
  (dimension 5.175 (width 0.15) (layer Dwgs.User)
    (gr_text "5.175 mm" (at 114.1875 104.3) (layer Dwgs.User))
    (feature1 (pts (xy 116.775 97.925) (xy 116.775 103.586421)))
    (feature2 (pts (xy 111.6 97.925) (xy 111.6 103.586421)))
    (crossbar (pts (xy 111.6 103) (xy 116.775 103)))
    (arrow1a (pts (xy 116.775 103) (xy 115.648496 103.586421)))
    (arrow1b (pts (xy 116.775 103) (xy 115.648496 102.413579)))
    (arrow2a (pts (xy 111.6 103) (xy 112.726504 103.586421)))
    (arrow2b (pts (xy 111.6 103) (xy 112.726504 102.413579)))
  )
  (dimension 44.075 (width 0.15) (layer Dwgs.User)
    (gr_text "44.075 mm" (at 99.8 119.9625 90) (layer Dwgs.User))
    (feature1 (pts (xy 111.6 97.925) (xy 100.513579 97.925)))
    (feature2 (pts (xy 111.6 142) (xy 100.513579 142)))
    (crossbar (pts (xy 101.1 142) (xy 101.1 97.925)))
    (arrow1a (pts (xy 101.1 97.925) (xy 101.686421 99.051504)))
    (arrow1b (pts (xy 101.1 97.925) (xy 100.513579 99.051504)))
    (arrow2a (pts (xy 101.1 142) (xy 101.686421 140.873496)))
    (arrow2b (pts (xy 101.1 142) (xy 100.513579 140.873496)))
  )
  (dimension 119.8 (width 0.15) (layer Dwgs.User)
    (gr_text "119.800 mm" (at 104.8 82.1 90) (layer Dwgs.User))
    (feature1 (pts (xy 111.6 22.2) (xy 105.513579 22.2)))
    (feature2 (pts (xy 111.6 142) (xy 105.513579 142)))
    (crossbar (pts (xy 106.1 142) (xy 106.1 22.2)))
    (arrow1a (pts (xy 106.1 22.2) (xy 106.686421 23.326504)))
    (arrow1b (pts (xy 106.1 22.2) (xy 105.513579 23.326504)))
    (arrow2a (pts (xy 106.1 142) (xy 106.686421 140.873496)))
    (arrow2b (pts (xy 106.1 142) (xy 105.513579 140.873496)))
  )
  (gr_line (start 111.6 23.7) (end 111.6 115.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.1 115.5) (end 170.1 23.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.1 117) (end 168.6 117) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.1 22.2) (end 168.6 22.2) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 168.6 115.5) (end 168.6 117) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.1 115.5) (end 111.6 115.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (dimension 58.5 (width 0.15) (layer Dwgs.User)
    (gr_text "58.500 mm" (at 140.85 155.299999) (layer Dwgs.User))
    (feature1 (pts (xy 170.1 142) (xy 170.1 154.58642)))
    (feature2 (pts (xy 111.6 142) (xy 111.6 154.58642)))
    (crossbar (pts (xy 111.6 153.999999) (xy 170.1 153.999999)))
    (arrow1a (pts (xy 170.1 153.999999) (xy 168.973496 154.58642)))
    (arrow1b (pts (xy 170.1 153.999999) (xy 168.973496 153.413578)))
    (arrow2a (pts (xy 111.6 153.999999) (xy 112.726504 154.58642)))
    (arrow2b (pts (xy 111.6 153.999999) (xy 112.726504 153.413578)))
  )
  (gr_text J1 (at 115.6 97.4) (layer F.SilkS))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 168.6 23.7) (xy 168.6 115.5) (xy 113.1 115.5) (xy 113.1 23.7)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 168.6 115.5) (xy 113.1 115.5) (xy 113.1 23.7) (xy 168.6 23.7)
      )
    )
  )
)
