<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="17.78" width="0" layer="20"/>
<wire x1="25.4" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<text>HSYN</text>
<text>VSYN</text>
<text>BACK</text>
<text>B</text>
<text>G</text>
<text>R</text>
<text>KC</text>
<text>KD</text>
<text>RX</text>
<text>TX</text>
<text>PA4</text>
<text>PA3</text>
<text>PA2</text>
<text>BOOT</text>
<text>3V3</text>
<text>SWDIO</text>
<text>GND</text>
<text>SWDCLK</text>
<text>(C)2016 
K. C. Lee</text>
<text>5V</text>
<text>K. C. Lee</text>
<text>GND</text>
<text>GND</text>
<text>(c) 2016</text>
<text>ChibiTerm</text>
</plain>
<libraries>
<library name="Misc Processor">
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ipc-7351-capacitor">
<description>&lt;b&gt;IPC-7351 compliant SMT capacitors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr&lt;br&gt;
Packages generated using genpkg_chp.ulp, genpkg_cae.ulp and genpkg_mld.ulp&lt;br&gt;
Devices are Vishay chip types, generic AEC types and Kemet T491 series molded body types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="CAPC2012X145AN">
</package>
<package name="CAPC1608X92N">
</package>
</packages>
</library>
<library name="ipc-7351-resistor">
<description>&lt;b&gt;IPC-7351 compliant SMT resistors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr.&lt;br&gt;
Packages generated using genpkg_chp.ulp.&lt;br&gt;
Devices are Panasonic ERJ series types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="RESC1608X55N">
</package>
</packages>
</library>
<library name="Misc logo">
<packages>
<package name="CC-BY-NC-75">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Misc Conn">
<packages>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="Misc Passives">
<packages>
<package name="CAT16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
<package name="SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Misc Power">
<packages>
<package name="SOT95P280X135-3N">
</package>
</packages>
</library>
<library name="ipc-7351-transistor">
<description>&lt;b&gt;IPC-7351 compliant SMT transistors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft transistor.lbr.&lt;br&gt;
Packages generated using genpkg_sot.ulp.&lt;br&gt;
Devices are Fairchild Semiconductor types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="SOT95P280X135-3N">
</package>
</packages>
</library>
<library name="ipc-7351-diode">
<description>&lt;b&gt;IPC-7351 compliant SMT diodes&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft diode.lbr.&lt;br&gt;
Packages generated using genpkg_sod.ulp, genpkg_sot.ulp and genpkg_mld.ulp.&lt;br&gt;
Devices are Fairchild Semiconductor types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="SOT95P280X135-3N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="Misc Processor" package="TSSOP20" value="STM32F030F4P6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="STM32F030F4P6"/>
</element>
<element name="R1" library="ipc-7351-resistor" package="RESC1608X55N" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="4K7, 0603"/>
</element>
<element name="C4" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="0.1UF, 0603"/>
</element>
<element name="C8" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="0.1UF, 0603"/>
</element>
<element name="C9" library="ipc-7351-capacitor" package="CAPC1608X92N" value="1uF">
<attribute name="PARTNO" value="1UF, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="ipc-7351-resistor" package="RESC1608X55N" value="4K7">
<attribute name="PARTNO" value="4K7, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="ipc-7351-resistor" package="RESC1608X55N" value="4K7">
<attribute name="PARTNO" value="4K7, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LICENSE" library="Misc logo" package="CC-BY-NC-75" value="CC-BY-NC">
<attribute name="PARTNO" value="LICENSE"/>
</element>
<element name="X1" library="crystal" package="SM49" value="25MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="25MHZ FUND. HC49"/>
</element>
<element name="C6" library="ipc-7351-capacitor" package="CAPC1608X92N" value="22pF">
<attribute name="PARTNO" value="22PF, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="ipc-7351-capacitor" package="CAPC1608X92N" value="22pF">
<attribute name="PARTNO" value="22PF, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="Misc Passives" package="CAT16" value="220R">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAT16-221J4"/>
</element>
<element name="J3" library="Misc Conn" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="0.1 IN HEADER 1X10"/>
</element>
<element name="J1" library="Misc Conn" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="0.1 IN HEADER 1X10"/>
</element>
<element name="U1" library="Misc Power" package="SOT95P280X135-3N" value="MCP1700/TT">
<attribute name="PARTNO" value="MCP1700T-3302E/TT"/>
</element>
<element name="C3" library="ipc-7351-capacitor" package="CAPC2012X145AN" value="1uF">
<attribute name="PARTNO" value="1UF, 0805"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ipc-7351-capacitor" package="CAPC2012X145AN" value="10uF">
<attribute name="PARTNO" value="10UF/10V X5R 0805"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="Misc Passives" package="CAT16" value="220R">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="CAT16-221J4"/>
</element>
<element name="Q1" library="ipc-7351-transistor" package="SOT95P280X135-3N" value="3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="MMBT3904"/>
</element>
<element name="R6" library="ipc-7351-resistor" package="RESC1608X55N" value="475R">
<attribute name="PARTNO" value="475R, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="ipc-7351-resistor" package="RESC1608X55N" value="2K">
<attribute name="PARTNO" value="2K, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ipc-7351-resistor" package="RESC1608X55N" value="475R">
<attribute name="PARTNO" value="475R, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="ipc-7351-capacitor" package="CAPC1608X92N" value="22pF">
<attribute name="PARTNO" value="22PF, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Misc Passives" package="SOD-123" value="3V3 Zener">
<attribute name="NAME"/>
<attribute name="PARTNO" value="BZT52C3V3"/>
</element>
<element name="D2" library="Misc Passives" package="SOD-123" value="3V3 Zener">
<attribute name="NAME"/>
<attribute name="PARTNO" value="BZT52C3V3"/>
</element>
<element name="J2" library="Misc Conn" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="0.1 IN HEADER 1X4"/>
</element>
<element name="R7" library="ipc-7351-resistor" package="RESC1608X55N" value="475R">
<attribute name="PARTNO" value="475R, 0603"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="ipc-7351-diode" package="SOT95P280X135-3N" value="BAT54">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="BAT54"/>
</element>
</elements>
<signals>
<signal name="+3.3V">
<contactref element="U2" pad="16"/>
<contactref element="C9" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="15"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="7"/>
<contactref element="U1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="J1" pad="8"/>
<contactref element="J3" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="SWCLK">
<contactref element="U2" pad="20"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SWDIO">
<contactref element="U2" pad="19"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="U2" pad="4"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="BOOT0">
<contactref element="U2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="11"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="12"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="7"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="6"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="PS2_CLK">
<contactref element="R5" pad="1"/>
<contactref element="RN1" pad="5"/>
<contactref element="J1" pad="9"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="PS2_DAT">
<contactref element="R3" pad="1"/>
<contactref element="RN1" pad="6"/>
<contactref element="J1" pad="10"/>
<contactref element="D3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="3"/>
<contactref element="X1" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="14"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="BACKGROUND">
<contactref element="J3" pad="8"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RN2" pad="2"/>
<contactref element="RN2" pad="1"/>
<contactref element="RN2" pad="3"/>
<contactref element="Q1" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="B">
<contactref element="J3" pad="6"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="G">
<contactref element="J3" pad="5"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="R">
<contactref element="J3" pad="4"/>
<contactref element="RN2" pad="8"/>
</signal>
<signal name="HSYNC">
<contactref element="RN1" pad="7"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="C10" pad="1"/>
<contactref element="U2" pad="13"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VSYNC">
<contactref element="J3" pad="9"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="PA4">
<contactref element="U2" pad="10"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="PA3">
<contactref element="U2" pad="9"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="PA2">
<contactref element="U2" pad="8"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="RXD">
<contactref element="U2" pad="18"/>
<contactref element="J1" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="TXD">
<contactref element="J1" pad="3"/>
<contactref element="U2" pad="17"/>
<contactref element="D1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
