(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 19)
    (no_connects 0)
    (area 201.625999 150.825999 220.014001 166.674001)
    (thickness 1.6)
    (drawings 33)
    (tracks 63)
    (zones 0)
    (modules 7)
    (nets 18)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.254)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.7112)
    (via_min_drill 0.3556)
    (user_via 0.7112 0.3556)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /nRST)
  (net 2 /WDI)
  (net 3 /nEXTR)
  (net 4 /PSW/nIRQ2)
  (net 5 /nCE)
  (net 6 /FOUT/nIRQ)
  (net 7 /EXTI)
  (net 8 /SDI)
  (net 9 /CLKOUT/nIRQ3)
  (net 10 /SCL)
  (net 11 /SDO)
  (net 12 /VBAT)
  (net 13 /VCC)
  (net 14 "Net-(C1-Pad1)")
  (net 15 "Net-(U1-Pad15)")
  (net 16 "Net-(U1-Pad16)")
  (net 17 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /CLKOUT/nIRQ3)
    (add_net /EXTI)
    (add_net /FOUT/nIRQ)
    (add_net /PSW/nIRQ2)
    (add_net /SCL)
    (add_net /SDI)
    (add_net /SDO)
    (add_net /VBAT)
    (add_net /VCC)
    (add_net /WDI)
    (add_net /nCE)
    (add_net /nEXTR)
    (add_net /nRST)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
  )
  (module Pin_Header_Straight_1x07_Pitch2.54mm2 (layer F.Cu) (tedit 58F9855C)
    (at 203.2 165.1 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at -0.254 -3.048 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at -2.921 12.446 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /nRST))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /WDI))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /nEXTR))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PSW/nIRQ2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /VBAT))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SDO))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58F984C3)
    (at 203.2 152.4 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -3.302 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 2.794 12.573 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /nCE))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /FOUT/nIRQ))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /EXTI))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDI))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /CLKOUT/nIRQ3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58F97AC7)
    (at 207.772 156.718 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.921 0 180) (layer F.SilkS))
    (fp_text value 47pF (at -0.4445 3.8989 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module crystal:crystal (layer F.Cu) (tedit 58F97C73)
    (at 207.518 160.02 90)
    (fp_text reference Y1 (at 0 -2.413 360) (layer F.SilkS))
    (fp_text value Crystal (at 0 -2.032 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad16)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad15)"))
    (model /home/frank/data/projects/nixie-clock/ab18x5-breakout/crystal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module qfn16:qfn16 (layer F.Cu) (tedit 58FAC4D0)
    (at 211.836 159.004)
    (clearance 0.1)
    (fp_text reference U1 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value AB1815 (at 1.016 -2.54) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 1 /nRST))
    (pad 2 smd rect (at -0.25 1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 2 /WDI))
    (pad 3 smd rect (at 0.25 1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 3 /nEXTR))
    (pad 4 smd rect (at 0.75 1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 4 /PSW/nIRQ2))
    (pad 12 smd rect (at -0.75 -1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 5 /nCE))
    (pad 11 smd rect (at -0.25 -1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 6 /FOUT/nIRQ))
    (pad 10 smd rect (at 0.25 -1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 7 /EXTI))
    (pad 9 smd rect (at 0.75 -1.39 180) (size 0.3 0.52) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDI))
    (pad 8 smd rect (at 1.39 -0.75 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /CLKOUT/nIRQ3))
    (pad 7 smd rect (at 1.39 -0.25 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCL))
    (pad 6 smd rect (at 1.39 0.25 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /SDO))
    (pad 5 smd rect (at 1.39 0.75 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /VBAT))
    (pad 13 smd rect (at -1.39 -0.75 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /VCC))
    (pad 14 smd rect (at -1.39 -0.25 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 15 smd rect (at -1.39 0.25 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -1.39 0.75 180) (size 0.52 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad16)"))
    (pad PAD smd rect (at 0 0 180) (size 1.8 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (model /home/frank/data/projects/nixie-clock/ab18x5-breakout/ab18x5-package.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module qfn16:via (layer F.Cu) (tedit 58F9818A)
    (at 211.836 159.004)
    (fp_text reference REF** (at 0 1.778) (layer F.SilkS) hide)
    (fp_text value via (at 0 -1.778) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7112 0.7112) (drill 0.3556) (layers *.Cu)
      (net 17 GND) (zone_connect 2))
  )
  (module ab18x5-breakout:oshw (layer F.Cu) (tedit 58FAC454)
    (at 216.916 159.766)
    (fp_text reference G*** (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.508 2.54) (layer F.SilkS) hide)
  )
  (gr_text frank-buss.de (at 202.692 159.004 90) (layer F.SilkS))
  (gr_text "VSS PAD" (at 203.2 153.67 270) (layer B.SilkS))
  (gr_text "VCC 13" (at 205.74 153.67 270) (layer B.SilkS))
  (gr_text "nCE 12" (at 208.28 153.67 270) (layer B.SilkS))
  (gr_text "nIRQ 11" (at 210.82 153.67 270) (layer B.SilkS))
  (gr_text "EXTI 10" (at 213.36 153.67 270) (layer B.SilkS))
  (gr_text "SDI 9" (at 215.9 153.67 270) (layer B.SilkS))
  (gr_text "nIRQ3 8" (at 218.44 153.67 270) (layer B.SilkS))
  (gr_text "7 SCL" (at 218.44 163.83 270) (layer B.SilkS))
  (gr_text "6 SDO" (at 215.9 163.83 270) (layer B.SilkS))
  (gr_text "5 VBAT" (at 213.36 163.83 270) (layer B.SilkS))
  (gr_text "4 nIRQ2" (at 210.82 163.83 270) (layer B.SilkS))
  (gr_text "3 nEXTR" (at 208.28 163.83 270) (layer B.SilkS))
  (gr_text "2 WDI" (at 205.74 163.83 270) (layer B.SilkS))
  (gr_text "1 nRST" (at 203.2 163.83 270) (layer B.SilkS))
  (gr_text 14 (at 203.2 154.432) (layer F.SilkS))
  (gr_text 13 (at 205.74 154.432) (layer F.SilkS))
  (gr_text 12 (at 208.28 154.432) (layer F.SilkS))
  (gr_text 11 (at 210.82 154.432) (layer F.SilkS))
  (gr_text 10 (at 213.36 154.432) (layer F.SilkS))
  (gr_text 9 (at 215.9 154.432) (layer F.SilkS))
  (gr_text 8 (at 218.44 154.432) (layer F.SilkS))
  (gr_text 7 (at 218.44 163.068) (layer F.SilkS))
  (gr_text 6 (at 215.9 163.068) (layer F.SilkS))
  (gr_text 5 (at 213.36 163.068) (layer F.SilkS))
  (gr_text 4 (at 210.82 163.068) (layer F.SilkS))
  (gr_text 3 (at 208.28 163.068) (layer F.SilkS))
  (gr_text 2 (at 205.74 163.068) (layer F.SilkS))
  (gr_line (start 201.676 166.624) (end 219.964 166.624) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 201.676 150.876) (end 201.676 166.624) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 219.964 150.876) (end 201.676 150.876) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 219.964 166.624) (end 219.964 150.876) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text 1 (at 203.2 163.068) (layer F.SilkS))
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.345 167.005) (xy 201.295 167.005) (xy 201.295 150.495) (xy 220.345 150.495)
      )
    )
  )
)
