(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 45)
    (no_connects 2)
    (area 91.924999 87.924999 123.075001 110.075001)
    (thickness 1.6)
    (drawings 23)
    (tracks 140)
    (zones 0)
    (modules 23)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 GND)
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J2-Pad1)")
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(J2-Pad3)")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R2-Pad1)")
  (net 14 "Net-(R4-Pad2)")
  (net 15 "Net-(C2-Pad1)")
  (net 16 "Net-(C5-Pad1)")
  (net 17 "Net-(D1-Pad2)")
  (net 18 "Net-(D2-Pad2)")
  (net 19 "Net-(J4-Pad2)")
  (net 20 "Net-(J4-Pad3)")
  (net 21 "Net-(J4-Pad4)")
  (net 22 "Net-(J4-Pad5)")
  (net 23 "Net-(J4-Pad6)")
  (net 24 "Net-(J4-Pad7)")
  (net_class Default "Это класс цепей по умолчанию."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad2)")
  )
  (net_class 5v ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C52113C)
    (at 97.155 102.87 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.73 1.645 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0.87 1.545 90) (layer B.SilkS))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C520E8F)
    (at 113.665 106.68 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.68 -1.565 90) (layer B.SilkS))
    (fp_text value 105pF (at -0.92 -1.565 90) (layer B.SilkS))
    (fp_text user %R (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C520E30)
    (at 105.41 106.68 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -1.58 1.41 270) (layer B.SilkS))
    (fp_text value 105pF (at 0.92 1.51 270) (layer B.SilkS))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C52116C)
    (at 97.155 97.79 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -1.51 1.545 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.99 1.645 90) (layer B.SilkS))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C520E68)
    (at 109.855 106.68 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -1.68 1.555 270) (layer B.SilkS))
    (fp_text value 100pF (at 0.82 1.655 270) (layer B.SilkS))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5C52B1F7)
    (at 95.885 90.805 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.667 0 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5C52B1F5)
    (at 93.345 90.805 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.667 0 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module F6888:B0505S-1w (layer F.Cu) (tedit 5C52B1FD)
    (at 92.71 106.045 90)
    (fp_text reference B0505 (at 6.01 2.83 90) (layer F.SilkS) hide)
    (fp_text value DC (at 6.01 4.61 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.99 0.9 90) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 4.53 0.9 90) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at 7.07 0.9 90) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 4 thru_hole circle (at 9.61 0.9 90) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad2)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51D77F)
    (at 105.41 101.6 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.4 -1.61 180) (layer B.SilkS))
    (fp_text value 1k (at -0.6 -1.61 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51E295)
    (at 111.76 102.87 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.16 0.57 180) (layer B.SilkS))
    (fp_text value 1.2k (at 3.56 -0.43 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51D762)
    (at 105.41 91.44 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0.54 -1.61 180) (layer B.SilkS))
    (fp_text value 22k (at -0.56 -1.91 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51D870)
    (at 111.76 90.17 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.26 0.47 180) (layer B.SilkS))
    (fp_text value 1.8k (at 3.66 -0.53 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J4-Pad6)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51D8A6)
    (at 111.76 92.71 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.16 0.41 180) (layer B.SilkS))
    (fp_text value 3.6 (at 3.66 -0.59 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J4-Pad5)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51D8BC)
    (at 111.76 95.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.16 0.45 180) (layer B.SilkS))
    (fp_text value 6.8k (at 3.66 -0.45 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J4-Pad4)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51DBBE)
    (at 111.76 97.79 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 3.16 0.49 180) (layer B.SilkS))
    (fp_text value 15k (at 3.36 -0.51 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C51DBD1)
    (at 111.76 100.33 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.16 0.53 180) (layer B.SilkS))
    (fp_text value 47k (at 3.36 -0.57 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module F6888:F6888-S (layer F.Cu) (tedit 5C23CB5E)
    (at 109.22 93.98)
    (fp_text reference U1 (at -5.08 -8.89) (layer F.SilkS))
    (fp_text value F6888 (at -3.81 -10.16) (layer F.Fab))
    (pad 1 smd rect (at -7.1 -4.1) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 10 smd rect (at -7.1 5.8) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 11 smd rect (at -7.1 6.9) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 14 smd rect (at -7.1 10.2) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 15 smd rect (at -7.1 11.3) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad1)"))
    (pad 16 smd rect (at -7.1 12.4) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 25 smd rect (at 7.6 12.4) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 30 smd rect (at 7.6 6.9) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 31 smd rect (at 7.6 5.8) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 33 smd rect (at 7.6 3.6) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 34 smd rect (at 7.6 2.5) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 35 smd rect (at 7.6 1.4) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad3)"))
    (pad 37 smd rect (at 7.6 -0.8) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 38 smd rect (at 7.6 -1.9) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (pad 39 smd rect (at 7.6 -3) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R4-Pad2)"))
    (pad 40 smd rect (at 7.6 -4.1) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ADB0)
    (at 97 108 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value in (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module F6888:Pin_Header_Straight_1x07_Pitch1.50mm (layer F.Cu) (tedit 5C52B1F0)
    (at 121 99 180)
    (descr "Through hole straight pin header, 1x07, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x07 1.27mm single row")
    (fp_text reference J4 (at 0 10 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x07_Male (at 0 10.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 1.5 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 3 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 4.5 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 6 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 7.5 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 0 9 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module F6888:Pin_Header_Straight_1x03_Pitch1.50mm (layer F.Cu) (tedit 5C51C748)
    (at 121 104.5 180)
    (descr "Through hole straight pin header, 1x03, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x03 1.27mm single row")
    (fp_text reference J2 (at 2 0 180) (layer F.SilkS) hide)
    (fp_text value AOUT (at 0 5 180) (layer F.Fab) hide)
    (fp_text user %R (at -1.5 1.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 1.5 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 3 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module F6888:Pin_Header_Straight_1x02_Pitch1.50mm (layer F.Cu) (tedit 5C51C74D)
    (at 121 108 270)
    (descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.27mm single row")
    (fp_text reference J3 (at 0.127 -1.397 270) (layer F.SilkS) hide)
    (fp_text value Mic (at 0 2.965 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0.635 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 1.5 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module F6888:Pin_Header_Straight_1x03_Pitch1.50mm (layer F.Cu) (tedit 5C52AD8F)
    (at 99 89.5)
    (descr "Through hole straight pin header, 1x03, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x03 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value rx/tx (at 0 5) (layer F.Fab))
    (fp_text user %R (at -1.5 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 1.5) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 3) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C52AD84)
    (at 105.4 96.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.8 1.6 360) (layer B.SilkS))
    (fp_text value 1k (at 0.3 1.6 360) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "F6888 Board v 0.1\nnubo.rtg@gmail.com" (at 101.1 99.6 90) (layer B.SilkS))
  (gr_text MIC (at 117.6 108) (layer B.SilkS))
  (gr_text +5V (at 97 106.3) (layer B.SilkS))
  (gr_text -5V (at 94.5 106.3) (layer B.SilkS))
  (gr_text RX (at 97.6 92.6) (layer B.SilkS))
  (gr_text TX (at 97.6 91) (layer B.SilkS))
  (gr_text GND (at 97.2 89.6) (layer B.SilkS))
  (gr_text M (at 119.5 90) (layer B.SilkS))
  (gr_text P (at 119.5 91.5) (layer B.SilkS))
  (gr_text + (at 119.5 93) (layer B.SilkS))
  (gr_text - (at 119.5 94.5) (layer B.SilkS))
  (gr_text N (at 119.5 96) (layer B.SilkS))
  (gr_text U (at 119.5 97.5) (layer B.SilkS))
  (gr_text G (at 119.5 99) (layer B.SilkS))
  (gr_text AGND (at 118.8 101.4) (layer B.SilkS))
  (gr_text ALCH (at 118.8 103) (layer B.SilkS))
  (gr_text ARCH (at 118.8 104.6) (layer B.SilkS))
  (gr_text "+\n" (at 119.5 106.5) (layer B.SilkS))
  (gr_text - (at 121 106.5) (layer B.SilkS))
  (gr_line (start 92 110) (end 92 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123 110) (end 92 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123 88) (end 123 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92 88) (end 123 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123 88) (xy 123 110) (xy 92 110) (xy 92 88)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123 88) (xy 123 110) (xy 92 110) (xy 92 88)
      )
    )
  )
)
